{"text_format":"1","workbook":"xlsx","n_sheets":4,"sheets":["OPFOKLEGHEN","opfok WW+droogt","Max waarden","Reductietechnieken"],"not_rendered":{"charts":0,"images":3,"macros":1,"external_links":0,"defined_names":1,"comments":2,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"OPFOKLEGHEN","index":0,"n_rows":47,"n_cols":22,"rows_kept":47,"cut":false,"hidden":false,"merged":[[8,4,10,5],[14,8,14,11],[32,4,33,8],[23,8,24,10],[18,4,20,4],[24,4,25,4],[20,8,22,10],[13,5,15,6],[13,16,25,16],[16,11,17,11],[16,12,18,14],[25,12,25,15],[12,12,13,14],[23,14,24,14],[19,12,20,15],[21,12,22,15]]}
[null,null,null,null,"Rekenmodel Vee-combistof - pluimvee - opfok leghennen (V2.0, 15 maart 2021)",null,null,null,null,null,"Berekenen van het reductiepercentage van combinaties van fijnstof reducerende technieken"]
[]
[null,null,null,null,null,null,null,"TOELICHTING GEBRUIK REKENMODEL (Er is online ook een handleiding beschikbaar)."]
[null,null,null,null,"invullen","naam",null,"Bij alle GEEL gekleurde vakjes dient een keuze gemaakt te worden. Ga op het vakje staan, klik rechts naast vakje en kies een optie.                              "]
[null,null,null,null,"invullen","adres",null,"De gerealiseerde reductiepercentages staan in GROENE blokjes vermeld. Helemaal rechts is het reductiepercentage van de combinatie van de fijnstofreducerende "]
[null,null,null,null,{"$f":"TODAY()","v":"2021-03-15"},"datum",null,"technieken weergegeven. Als combinaties niet mogelijk of zinvol zijn, verschijnt er tekst in ROOD. Bij 'niet mogelijk' dient u keuze(s) aan te passen."]
[null,null,null,null," ",null,null,"Bij warmtewisselaar en stoffilter kan de ventilatiehoeveelheid door een techniek aangepast worden met de pijltjes omhoog/omlaag. "]
[null,null,null,{"$f":"IF(H20=\"ja\",IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.2,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.145/0.15,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.4,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.36/0.35,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.5,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.435/0.4,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.55,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.42/0.4,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<1.5,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.616/0.6))))),IF(H20=\"nee\",IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.25,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.175/0.2,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.35,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19),IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.45,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.434/0.4,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.6,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.53/0.55,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<0.9,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*0.754/0.8,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<1.63,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*1.2/1.25,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<1.85,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*1.723/1.8,IF(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19<4.7,(OPFOKLEGHEN!H14+OPFOKLEGHEN!F19)*1.74/1.8)))))))),OPFOKLEGHEN!H14+OPFOKLEGHEN!F19))","v":0}]
[null,null,null,0,{"$f":"IF(H17<0,\"Klik een keer op de pijl met ventilatiehoeveelheid tussen droogtunnel en warmtewisselaar\",\"   \")","v":"   "},null,null,null,"Lucht droogtunnel door overige techniek?",null,null,"NEE"]
[null,null,null,{"$f":"IF($H$13=\"parallel geschakeld met warmtewisselaar\",D19/100,0)","v":0},null,null,null,{"$f":"IF(E24=\"oliefilm bij voliere dmv leidingen\",IF(H11=\"droogtunnel (platen) 55%\",\"Oliefilm met leidingen en droogtunnel kunnen niet gecombineerd worden\",IF(H12=\"droogtunnel (banden) 30%\",\"Oliefilm met leidingen en droogtunnel kunnen niet gecombineerd worden\",\"    \")),IF(E20=\"strooiselschuif icm oliefilm bij voliere dmv leidingen\",IF(H12=\"droogtunnel (platen) 55%\",\"Oliefilm met leidingen en droogtunnel kunnen niet gecombineerd worden\",IF(H12=\"droogtunnel (banden) 30%\",\"Oliefilm met leidingen en droogtunnel kunnen niet gecombineerd worden\",\"    \")),IF(H12=\"geen droogtunnel\",\"    \",IF(E16=\"GRONDHUISVESTING\",\"   \",IF(E16=\"VOLIEREHUISVESTING\",\"   \",IF(E16=\"kOLONIEHUISVESTING\",\"   \",IF(E16=\"leghennen verrijkte kooi/kolonie\",\"   \",IF(E16=\"leghennen voliere\",\"   \",IF(E16=\"leghennen grondhuisvesting\",\"   \",IF(H12=\"droogtunnel (platen) 55%\",\"Droogtunnel kan alleen bij (opfok) leghennen\",IF(H12=\"droogtunnel (banden) 30%\",\"Droogtunnel kan alleen bij (opfok) leghennen\",\"      \")))))))))))","v":"      "}]
[null,null,null,"KIES EEN CATEGORIE",null,null,null,"GEEN DROOGTUNNEL",null,{"$f":"IF(L25=\"GEEN TECHNIEK\",F13-H14,IF(L9=\"nee\",J30-J13-J16-J19-J26-J28,0))","v":0},"m3"]
[null,null,null,"GRONDHUISVESTING",null,null,null,{"$f":"IF(H11=\"geen droogtunnel\",0,IF(H7=\"Droogtunnel kan alleen bij (opfok) leghennen\",\"   \",IF(H13=\"parallel geschakeld met warmtewisselaar\",'opfok WW+droogt'!$Q$138*(1-E28),IF(H11=\"droogtunnel (banden) 30%\",30%*(1-E28),IF(H11=\"droogtunnel (platen) 55%\",55%*(1-E28),0)))))","v":0}]
[null,null,null,"VOLIEREHUISVESTING",null,{"$f":"'opfok WW+droogt'!$I$3","v":0},"m3","PARALLEL GESCHAKELD MET WARMTEWISSELAAR",null,{"$f":"IF(L25=\"GEEN TECHNIEK\",0,IF(L9=\"ja\",F13-H14,0))","v":0},"m3",null,{"$f":"IF(L25=\"luchtconditioneringsunit\",\"   \",IF(L25=\"geen techniek\",\"    \",IF(L25=\"chemische wasser 35%\",\"    \",IF(L25=\"chemische wasser 70%\",\"    \",IF(L25=\"bio wasser 60%\",\"    \",IF(L25=\"bio wasser 75%\",\"    \",IF(L25=\"waterluchtwassysteem\",\"   \",IF(L25=\"biofilter\",\"    \",IF(L25=\"Droogfilterwand\",\"   \",IF(L25=\"ionisatiefilter\",IF(E24=\"ionisatie dmv koolstofborsteltjes\",\"Combinatie van ionisatietechnieken is niet zinvol\",IF(E24=\"ionisatie dmv koolstof-borsteltjes icm strooiselschuif\",\"Combinatie van ionisatietechnieken is niet zinvol\",\"   \"))))))))))))","v":"    "}]
[null,null,null,"KOLONIEHUISVESTING",null,{"$f":"IF(J30=0,\"   \",IF(H12>0,IF(H13=\"parallel geschakeld met warmtewisselaar\",IF(F19>0.2,\"De eerste weken van de opfok te weinig ventilatie voor mestdroging\",\"  \"),IF(F13+F19+F25+F26>J30,\"Dit volume door droogtunnel wordt niet volledig benut. Verlaag ventilatie stoffilter of warmtewisselaar.\",\"     \")),\"   \"))","v":"   "},null,{"$f":"IF(H10=\"Geen droogtunnel mogelijk\",0,IF(H11=\"geen droogtunnel\",0,IF(H13=\"PARALLEL GESCHAKELD MET WARMTEWISSELAAR\",0,F13)))","v":0},"m3",null,null,null,null,null,null,null,"Reductiepercentage PM10"]
[null,null,"̌",null,null,null,null,{"$f":"IF(H14+F19+H21=0,\"Geen warmtewisselaar\",\"Warmtewisselaar\")","v":"Geen warmtewisselaar"},{"$f":"IF(E24=\"oliefilm bij voliere dmv leidingen\",IF(F19>0,\"Oliefilm met leidingen niet combineren met warmtewisselaar\",\"   \"),\"  \")","v":"  "}]
[null,null,null,null,null,null,null,{"$f":"IF(H15=\"warmtewisselaar\",\"Reductiepercentage WW 80%\",\"   \")","v":"   "},null,{"$f":"IF(L25=\"geen techniek\",H14+F19+H21,IF(J18=\"ja\",0,F19+H14))","v":0},"m3"]
[null,null,null,null,null,null,null,{"$f":"IF(E19=\"Kies een categorie\",0,IF(F13+F19=0,0,IF(I15=\"Oliefilm met leidingen niet combineren met warmtewisselaar\",\"error\",IF(H13=\"serie geschakeld met warmtewisselaar\",('opfok WW+droogt'!$O$138-'opfok WW+droogt'!$P$138)*(1-E28),'opfok WW+droogt'!$N$138*(1-E28)))))","v":0},{"$f":"\"Lucht WW door overige techniek?\"","v":"Lucht WW door overige techniek?"},null,null,null,{"$f":"IF(E24=\"oliefilm bij voliere dmv leidingen\",IF(H25>0,\"Oliefilm dmv leidingen niet combineren met techniek buiten de stal\",IF(L27>0,\"Oliefilm dmv leidingen niet combineren met techniek buiten de stal\",\"    \")),IF(E24=\"strooiselschuif icm oliefilm bij voliere dmv leidingen\",IF(H25>0,\"Oliefilm dmv leidingen niet combineren met techniek buiten de stal\",IF(L27>0,\"Oliefilm dmv leidingen niet combineren met techniek buiten de stal\",\"    \")),\"    \"))","v":"    "}]
[null,null,null,null,"Stal voor opfok leg",null,null,"Warmtewisselaar met stoffilter?",null,"NEE"]
[null,null,null,0,"KIES EEN CATEGORIE",{"$f":"IF(E19=\"kies een categorie\",0,IF(F13+F25>J30,0,D19/100))","v":0},"m3",{"$f":"IF(F20=0,\"    \",\"Reductie% stoffilter 99%\")","v":"Reductie% stoffilter 99%"},null,{"$f":"IF(L25=\"geen techniek\",0,IF(J18=\"ja\",F19+H14,0))","v":0},"m3"]
[null,null,null,{"$f":"MAX(0,D19-F13*100)","v":0},null,"% t.o.v. maximum",null,"NEE",null,{"$f":"IF(J18=\"nee\",\"     \",IF(L25=\"geen techniek\",IF(J18=\"ja\",\"Indien 'geen techniek', dan is er geen luchtstroom\"),\"   \"))","v":"     "},null,null,{"$f":"IF(F19>0,IF(L25=\"Luchtconditioneringsunit\",\"Twee keer eenzelfde type techniek in de uitgaande luchtstroom is niet logisch\",\"    \"),\"   \")","v":"   "}]
[null,null,null,null,null,{"$f":"IF(J30=0,\"    \",F19/J30)","v":"    "},null,null,{"$f":"IF(J16=0,IF(J11=0,\"   \",IF(J11>0,IF(L25=\"chemische wasser 35%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"chemische wasser 70%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Bio wasser 60%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Bio wasser 75%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Biofilter\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Luchtconditioneringsunit\",\"Alle lucht moet door overige techniek\",\"   \")))))),\"   \")),IF(J16>0,IF(L25=\"chemische wasser 35%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"chemische wasser 70%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Bio wasser 60%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Bio wasser 75%\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Biofilter\",\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",IF(L25=\"Luchtconditioneringsunit\",\"Alle lucht moet door overige techniek\",\"   \")))))),\"  \"))","v":"   "}]
[null,null,null,null,{"$f":"IF(F19>0,\"Reset: Zet ventilatie door WW en/of stoffilter in 1 klik op 0 m3\",IF(F25>0,\"Zet ventilatie door WW en/of stoffilter in 1 klik op 0 m3\",\"  \"))","v":"  "},null,null,null,null,null,null,null,{"$f":"IF(L25=\"Biofilter\",IF(H20=\"ja\",IF(J18>0,\"Deze combinatie met WW stoffilter is toepasbaar, maar niet zinvol\",\"     \"),\"  \"),IF(L25=\"bio wasser 60%\",IF(H20=\"ja\",IF(J18>0,\"Deze combinatie met WW stoffilter is toepasbaar, maar niet zinvol\",\"   \"),\"   \"),IF(L25=\"bio wasser 75%\",IF(H20=\"ja\",IF(J18>0,\"Deze combinatie met WW stoffilter is toepasbaar, maar niet zinvol\",\"   \"),\"    \"),\"   \")))","v":"   "}]
[null,null,null,null,"Staltechniek",null,null,{"$f":"IF(F25=0,\"Geen stoffilter\",\"Stoffilter\")","v":"Geen stoffilter"},null,null,null,"Overige technieken"]
[null,null,null,0,"GEEN STALTECHNIEK",null,null,{"$f":"IF(F25=0,\"    \",\"Reductie% stoffilter 99%\")","v":"    "},{"$f":"IF(F25>0,IF(L25=\"chemische wasser 35%\",\"Alle lucht moet door de luchtwasser of biofilter. De combinatie met een stoffilter is daarom niet mogelijk.\",IF(L25=\"chemische wasser 70%\",\"Alle lucht moet door de luchtwasser of biofilter. De combinatie met een stoffilter is daarom niet mogelijk.\",IF(L25=\"bio wasser 60%\",\"Alle lucht moet door de luchtwasser of biofilter. De combinatie met een stoffilter is daarom niet mogelijk.\",IF(L25=\"bio wasser 75%\",\"Alle lucht moet door de luchtwasser of biofilter. De combinatie met een stoffilter is daarom niet mogelijk.\",IF(L25=\"biofilter\",\"Alle lucht moet door de luchtwasser of biofilter. De combinatie met een stoffilter is daarom niet mogelijk.\",\"  \"))))),\"   \")","v":"   "},null,null,{"$f":"IF(L25=\"chemische wasser 35%\",\"Potentieel reductie: 35%\",IF(L25=\"chemische wasser 70%\",\"Potentieel reductie: 70%\",IF(L25=\"bio wasser 60%\",\"Potentieel reductie: 60%\",IF(L25=\"bio wasser 75%\",\"Potentieel reductie: 75%\",IF(L25=\"biofilter\",\"Potentieel reductie: 80%\",IF(L25=\"waterluchtwassysteem\",\"Potentieel reductie: 33%\",IF(L25=\"droogfilterwand\",\"Potentieel reductie: 40%\",IF(L25=\"ionisatiefilter\",\"Potentieel reductie: 57%\",IF(L25=\"luchtconditioneringsunit\",\"Potentieel reductie: 80%\",\"  \")))))))))","v":"  "}]
[null,null,null,null,{"$f":"IF(E24=\"geen staltechniek\",\"    \",IF(E24=\"oliefilm bij voliere dmv leidingen\",IF(E19=\"VOLIEREHUISVESTING\",\"     \",\"Deze techniek kan alleen bij volière\"),IF(E24=\"oliefilm dmv olierobot\",IF(E19=\"GRONDHUISVESTING\",\"    \",\"Deze techniek kan alleen bij grondhuisvesting\"),\"  \")))","v":"    "},{"$f":"IF(E19=\"kies een categorie\",0,IF(F13*100+D20+D24>J30*100,(J30*100-F13*100-D20)/100,MAX(D24/100,D24/100-D20/100)))","v":0},"m3",{"$f":"ROUND(IF(F13>0,'opfok WW+droogt'!$S$138*(1-E28),IF(H15=\"warmtewisselaar\",'opfok WW+droogt'!$S$138*(1-E28),'opfok WW+droogt'!$R$138*(1-E28))),2)","v":0},null,null,null,"GEEN TECHNIEK"]
[null,null,null,null,null,{"$f":"MAX(J30-F13-F19-F25,0)","v":0},"m3",null,null,{"$f":"IF(L25=\"geen techniek\",0,F26)","v":0},"m3","Reductiepercentage overige techniek",{"$f":"IF(L25=\"Luchtconditioneringsunit\",IF(F25>0,\"Niet alle lucht gaat door luchtconditioneringsunit, dus niet combineren met droog stoffilter\",\"    \"),\"   \")","v":"   "}]
[null,null,null,null,"Reductiepercentage in stal","Max. ventilatiedebiet m3/d/uur",null," ",null,null,null,{"$f":"IF(M20=\"Twee keer eenzelfde type techniek in de uitgaande luchtstroom is niet logisch\",\"error\",IF(M26=\"Niet alle lucht gaat door luchtconditioneringsunit, dus niet combineren met droog stoffilter\",\"error\",IF(I21=\"Alle lucht moet door overige techniek vanwege ammoniak en/of geur\",\"error\",IF(I21=\"Alle lucht moet door overige techniek\",\"error\",IF(I24=\"Alle lucht moet door de luchtwasser of biofilter. De combinatie met een stoffilter is daarom niet mogelijk.\",\"error\",IF(L25=\"geen techniek\",0,IF(J13+J19+J26=0,0,IF(I21=\"Combinatie met warmtewisselaar is niet toegestaan\",\"error\",'opfok WW+droogt'!$I$10*(1-E28)))))))))","v":0},null,null,null,null,{"$f":"ROUNDDOWN(IF(H10=\"Oliefilm met leidingen en droogtunnel kunnen niet gecombineerd worden\",\"error\",IF(M17=\"Oliefilm dmv leidingen niet combineren met techniek buiten de stal\",\"error\",IF(H17<0,\"error\",IF(E19=\"Kies een categorie\",0,IF(M19=\"Oliefilm dmv leidingen niet combineren met techniek buiten de stal\",\"error\",IF(G28<>J30,\"error\",100%-(1-E28)+(H12+H25+H17)+L27)))))),3)","v":0}]
[null,null,null,null,{"$f":"IF(E25=\"deze combinatie kan niet\",0,IF(E25=\"Deze techniek kan alleen bij volière\",0,IF(E25=\"Deze techniek kan alleen bij grondhuisvesting\",0,IF(E24=\"oliefilm bij voliere dmv leidingen\",15%,IF(E24=\"oliefilm dmv olierobot\",30%,IF(E24=\"OLIEFILM bij voliere DMV LEIDINGEN\",15%,IF(E24=\"ionisatie dmv koolstofborsteltjes\",31%,0)))))))","v":0},null,{"$f":"J11+J13+J16+J19+J26+J28","v":0},null,null,{"$f":"F25+F26-H21-J26","v":0},"m3"]
[null,null,null,null,null,null,null,null,null,null,{"$f":"IF(G28<>J30,\"Optelsom debiet klopt niet\",\"   \")","v":"   "}]
[null,null,null,"GEEN STALTECHNIEK",null,null,null,"Maximale ventilatie in de stal",null,{"$f":"IF(E19=\"Kies een categorie\",0,IF(E19=\"kOLONIEHUISVESTING\",'Max waarden'!$B$6,IF(E19=\"GRONDHUISVESTING\",'Max waarden'!$B$6,IF(E19=\"VOLIEREHUISVESTING\",'Max waarden'!$B$6,IF(E19=\"voliereHUISVESTING\",#REF!,IF(E19=\"grondhuisvesting\",#REF!,IF(E19=\"kolonieHUISVESTING\",#REF!,IF(E19=\"opfok vleeskuikenouderdieren\",#REF!,IF(E19=\"vleeskuikenouderdieren groepskooi\",#REF!,IF(E19=\"vleeskuikenouderdieren VOLIERE\",#REF!,IF(E19=\"vleeskuikenouderdieren grondhuisvesting\",#REF!,IF(E19=\"vleeskuikens\",6.17619,IF(E19=\"kalkoen hennen\",#REF!,IF(E19=\"kalkoen hanen\",#REF!,IF(E19=\"vleeseenden\",12.56)))))))))))))))","v":0},"m3"]
[null,null,null,"OLIEFILM bij VOLIERE dmv LEIDINGEN"]
[null,null,null,"OLIEFILM dmv OLIEROBOT",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,"IONISATIE dmv KOOLSTOFBORSTELTJES","Gemaakt in opdracht van het ministerie van Infrastructuur en Waterstaat"]
[]
[null,null,null,null,null,null,null," "]
[null,null,null,{"$f":"IF(H22=\"zonder stoffilter\",IF(D37=\"opfok leghennen\",IF(H20=\"warmtewisselaar 13%\",0.2,IF(H20=\"warmtewisselaar 31%\",0.43,IF(H20=\"warmtewisselaar 37%\",0.55,IF(H20=\"warmtewisselaar 50%\",0.78)))),IF(D37=\"leghennen\",IF(H20=\"warmtewisselaar 13%\",0.4,IF(H20=\"warmtewisselaar 31%\",1,IF(H20=\"warmtewisselaar 37%\",1.25,IF(H20=\"warmtewisselaar 50%\",1.8)))),IF(E19=\"opfok vleeskuikenouderdieren\",IF(H20=\"warmtewisselaar 13%\",0.4,IF(H20=\"warmtewisselaar 31%\",1,IF(H20=\"warmtewisselaar 37%\",1.3,IF(H20=\"warmtewisselaar 50%\",1.9)))),IF(D37=\"vleeskuikenouderdieren\",IF(H20=\"warmtewisselaar 13%\",0.6,IF(H20=\"warmtewisselaar 31%\",1.5,IF(H20=\"warmtewisselaar 37%\",1.85,IF(H20=\"warmtewisselaar 50%\",2.9))))))+IF(E19=\"vleeskuikens\",IF(H20=\"warmtewisselaar 13%\",0.35,IF(H20=\"warmtewisselaar 31%\",1,IF(H20=\"warmtewisselaar 37%\",1.3,IF(H20=\"warmtewisselaar 50%\",2,0)))))+IF(E19=\"vleeseenden\",IF(H20=\"warmtewisselaar 13%\",0.8,IF(H20=\"warmtewisselaar 31%\",2.3,IF(H20=\"warmtewisselaar 37%\",3.15,IF(H20=\"warmtewisselaar 50%\",4.8)))))))+IF(E19=\"kalkoen hennen\",IF(H20=\"warmtewisselaar 13%\",1.1,IF(H20=\"warmtewisselaar 31%\",3,IF(H20=\"warmtewisselaar 37%\",3.85,IF(H20=\"warmtewisselaar 50%\",5.6)))))+IF(E19=\"kalkoen hanen\",IF(H20=\"warmtewisselaar 13%\",2.5,IF(H20=\"warmtewisselaar 31%\",6.2,IF(H20=\"warmtewisselaar 37%\",8.2,IF(H20=\"warmtewisselaar 50%\",11.7))))),0)+IF(H22=\"met stoffilter\",IF(D37=\"opfok leghennen\",IF(H20=\"warmtewisselaar 13%\",0.15,IF(H20=\"warmtewisselaar 31%\",0.35,IF(H20=\"warmtewisselaar 37%\",0.4,IF(H20=\"warmtewisselaar 50%\",0.6)))),IF(D37=\"leghennen\",IF(H20=\"warmtewisselaar 13%\",0.35,IF(H20=\"warmtewisselaar 31%\",0.85,IF(H20=\"warmtewisselaar 37%\",1,IF(H20=\"warmtewisselaar 50%\",1.4)))),IF(E19=\"leghennen grondhuisvesting\",IF(H20=\"warmtewisselaar 13%\",0.35,IF(H20=\"warmtewisselaar 31%\",0.85,IF(H20=\"warmtewisselaar 37%\",1,IF(H20=\"warmtewisselaar 50%\",1.4)))),IF(E19=\"opfok vleeskuikenouderdieren\",IF(H20=\"warmtewisselaar 13%\",0.35,IF(H20=\"warmtewisselaar 31%\",0.85,IF(H20=\"warmtewisselaar 37%\",1.1,IF(H20=\"warmtewisselaar 50%\",1.45)))),IF(D37=\"vleeskuikenouderdieren\",IF(H20=\"warmtewisselaar 13%\",0.5,IF(H20=\"warmtewisselaar 31%\",1.2,IF(H20=\"warmtewisselaar 37%\",1.5,IF(H20=\"warmtewisselaar 50%\",2.1))))))+IF(E19=\"vleeskuikens\",IF(H20=\"warmtewisselaar 13%\",0.3,IF(H20=\"warmtewisselaar 31%\",0.75,IF(H20=\"warmtewisselaar 37%\",1,IF(H20=\"warmtewisselaar 50%\",1.45,0)))))+IF(E19=\"vleeseenden\",IF(H20=\"warmtewisselaar 13%\",0.7,IF(H20=\"warmtewisselaar 31%\",1.9,IF(H20=\"warmtewisselaar 37%\",2.3,IF(H20=\"warmtewisselaar 50%\",3.6)))))))+IF(E19=\"kalkoen hennen\",IF(H20=\"warmtewisselaar 13%\",0.9,IF(H20=\"warmtewisselaar 31%\",2.5,IF(H20=\"warmtewisselaar 37%\",3,IF(H20=\"warmtewisselaar 50%\",4.3)))))+IF(E19=\"kalkoen hanen\",IF(H20=\"warmtewisselaar 13%\",2.2,IF(H20=\"warmtewisselaar 31%\",5.3,IF(H20=\"warmtewisselaar 37%\",6.2,IF(H20=\"warmtewisselaar 50%\",9)))))),0)","v":0}]
[null,null,null,{"$f":"IF(H24=\"zonder stoffilter\",IF(D38=\"opfok leghennen\",IF(H17=\"warmtewisselaar 13%\",0.2,IF(H17=\"warmtewisselaar 31%\",0.43,IF(H17=\"warmtewisselaar 37%\",0.55,IF(H17=\"warmtewisselaar 50%\",0.78)))),IF(D38=\"leghennen\",IF(H17=\"warmtewisselaar 13%\",0.4,IF(H17=\"warmtewisselaar 31%\",1,IF(H17=\"warmtewisselaar 37%\",1.25,IF(H17=\"warmtewisselaar 50%\",1.8)))),IF(E19=\"opfok vleeskuikenouderdieren\",IF(H17=\"warmtewisselaar 13%\",0.4,IF(H17=\"warmtewisselaar 31%\",1,IF(H17=\"warmtewisselaar 37%\",1.3,IF(H17=\"warmtewisselaar 50%\",1.9)))),IF(D38=\"vleeskuikenouderdieren\",IF(H17=\"warmtewisselaar 13%\",0.6,IF(H17=\"warmtewisselaar 31%\",1.5,IF(H17=\"warmtewisselaar 37%\",1.85,IF(H17=\"warmtewisselaar 50%\",2.9))))))+IF(E19=\"vleeskuikens\",IF(H17=\"warmtewisselaar 13%\",0.35,IF(H17=\"warmtewisselaar 31%\",1,IF(H17=\"warmtewisselaar 37%\",1.3,IF(H17=\"warmtewisselaar 50%\",2,0)))))+IF(E19=\"vleeseenden\",IF(H17=\"warmtewisselaar 13%\",0.8,IF(H17=\"warmtewisselaar 31%\",2.3,IF(H17=\"warmtewisselaar 37%\",3.15,IF(H17=\"warmtewisselaar 50%\",4.8)))))))+IF(E19=\"kalkoen hennen\",IF(H17=\"warmtewisselaar 13%\",1.1,IF(H17=\"warmtewisselaar 31%\",3,IF(H17=\"warmtewisselaar 37%\",3.85,IF(H17=\"warmtewisselaar 50%\",5.6)))))+IF(E19=\"kalkoen hanen\",IF(H17=\"warmtewisselaar 13%\",2.5,IF(H17=\"warmtewisselaar 31%\",6.2,IF(H17=\"warmtewisselaar 37%\",8.2,IF(H17=\"warmtewisselaar 50%\",11.7))))),0)+IF(H24=\"met stoffilter\",IF(D38=\"opfok leghennen\",IF(H17=\"warmtewisselaar 13%\",0.15,IF(H17=\"warmtewisselaar 31%\",0.35,IF(H17=\"warmtewisselaar 37%\",0.4,IF(H17=\"warmtewisselaar 50%\",0.6)))),IF(D38=\"leghennen\",IF(H17=\"warmtewisselaar 13%\",0.35,IF(H17=\"warmtewisselaar 31%\",0.85,IF(H17=\"warmtewisselaar 37%\",1,IF(H17=\"warmtewisselaar 50%\",1.4)))),IF(E19=\"leghennen grondhuisvesting\",IF(H17=\"warmtewisselaar 13%\",0.35,IF(H17=\"warmtewisselaar 31%\",0.85,IF(H17=\"warmtewisselaar 37%\",1,IF(H17=\"warmtewisselaar 50%\",1.4)))),IF(E19=\"opfok vleeskuikenouderdieren\",IF(H17=\"warmtewisselaar 13%\",0.35,IF(H17=\"warmtewisselaar 31%\",0.85,IF(H17=\"warmtewisselaar 37%\",1.1,IF(H17=\"warmtewisselaar 50%\",1.45)))),IF(D38=\"vleeskuikenouderdieren\",IF(H17=\"warmtewisselaar 13%\",0.5,IF(H17=\"warmtewisselaar 31%\",1.2,IF(H17=\"warmtewisselaar 37%\",1.5,IF(H17=\"warmtewisselaar 50%\",2.1))))))+IF(E19=\"vleeskuikens\",IF(H17=\"warmtewisselaar 13%\",0.3,IF(H17=\"warmtewisselaar 31%\",0.75,IF(H17=\"warmtewisselaar 37%\",1,IF(H17=\"warmtewisselaar 50%\",1.45,0)))))+IF(E19=\"vleeseenden\",IF(H17=\"warmtewisselaar 13%\",0.7,IF(H17=\"warmtewisselaar 31%\",1.9,IF(H17=\"warmtewisselaar 37%\",2.3,IF(H17=\"warmtewisselaar 50%\",3.6)))))))+IF(E19=\"kalkoen hennen\",IF(H17=\"warmtewisselaar 13%\",0.9,IF(H17=\"warmtewisselaar 31%\",2.5,IF(H17=\"warmtewisselaar 37%\",3,IF(H17=\"warmtewisselaar 50%\",4.3)))))+IF(E19=\"kalkoen hanen\",IF(H17=\"warmtewisselaar 13%\",2.2,IF(H17=\"warmtewisselaar 31%\",5.3,IF(H17=\"warmtewisselaar 37%\",6.2,IF(H17=\"warmtewisselaar 50%\",9)))))),0)","v":0},null,null,null,null,null,null," "]
[null,null,null,{"$f":"IF(E19=\"kOLONIEHUISVESTING\",\"opfok leghennen\",IF(E19=\"GRONDHUISVESTING\",\"opfok leghennen\",IF(E19=\"VOLIEREHUISVESTING\",\"opfok leghennen\",IF(E19=\"leghennen verrijkte kooi/kolonie\",\"leghennen\",IF(E19=\"leghennen grondhuisvesting\",\"leghennen\",IF(E19=\"leghennen voliere\",\"leghennen\",IF(E19=\"vleeskuikenouderdieren groepskooi\",\"vleeskuikenouderdieren\",IF(E19=\"vleeskuikenouderdieren grondhuisvesting\",\"vleeskuikenouderdieren\",IF(E19=\"vleeskuikenouderdieren voliere\",\"vleeskuikenouderdieren\",0)))))))))","v":0}]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,"Kies ALLE VENTILATIELUCHT ivm vereiste NH3 reductie"]

{"sheet":"opfok WW+droogt","index":1,"n_rows":143,"n_cols":45,"rows_kept":143,"cut":false,"hidden":true,"merged":[[13,30,13,38]]}
["Berekening reductie PM10 op stalniveau leghennen",null,null,null,null,null,null,null,{"$f":"OPFOKLEGHEN!$E$19","v":"KIES EEN CATEGORIE"},null,null,null,null,null,null,null,null,null,null,null,null,"y","z","aa","ab"]
["maximale ventilatiebehoefte",null,null,null,null,null,null,null,{"$f":"'Max waarden'!$B$6","v":1.73},"m3/dier/uur"]
["Maximale debiet door droogtunnel",null,null,null,null,null,null,null,{"$f":"IF(OPFOKLEGHEN!H11=\"geen droogtunnel\",0,IF(OPFOKLEGHEN!H11=\"DROOGTUNNEL (PLATEN) 55%\",0.85,0.85))","v":0},"m3/dier/uur"]
["Verwijderingsrendement droogtunnel",null,null,null,null,null,null,null,{"$f":"IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",79%,IF(OPFOKLEGHEN!$H$11=\"droogtunnel (banden) 30%\",43%,0))","v":0},null,null,null,"platendroger: 80% verwijdering",null,null,"bandendroger: 45% verwijdering"]
["Maximale debiet door warmtewisselaar:",null,null,null,null,null,null,null,{"$f":"OPFOKLEGHEN!H14+OPFOKLEGHEN!F19","v":0},{"$f":"IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",OPFOKLEGHEN!D8,IF(OPFOKLEGHEN!$H$13=\"SERIE GESCHAKELD MET WARMTEWISSELAAR\",OPFOKLEGHEN!D9,OPFOKLEGHEN!D10))","v":0},"m3/dier/uur"]
["Verwijderingsrendement warmtewisselaar:",null,null,null,null," ",null,null,{"$f":"IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",0,IF(OPFOKLEGHEN!$H$20=\"ja\",95%,80%))","v":0},null,null," ","standaard: 80% verwijdering",null,null,"bij toepassen filters: 99% verwijdering"]
["Maximale debiet door stoffilter:",null,null,null,null,null,null,null,{"$f":"OPFOKLEGHEN!$F$25","v":0}]
["Eventueel reductie op PM10 concentratie in de stal:",null,null,null,null,null,null,null,{"$f":"OPFOKLEGHEN!$E$28","v":0},{"$f":"OPFOKLEGHEN!$H$20","v":"NEE"},"stoffilter"]
["Eventueel verwijderingsrendement hoofdventilatie (lucht NIET door andere technieken):",null,null,null,null,null,null,null,0,{"$f":"OPFOKLEGHEN!$L$9","v":"NEE"},"droogtunnel"]
["Eventueel reductie door luchtwasser (op ALLE lucht)",null,null,null,null,null,{"$f":"IF(OPFOKLEGHEN!$L$25=\"chemische wasser 35%\",35%,IF(OPFOKLEGHEN!$L$25=\"chemische wasser 70%\",70%,IF(OPFOKLEGHEN!$L$25=\"bio wasser 60%\",60%,IF(OPFOKLEGHEN!$L$25=\"bio wasser 75%\",75%,IF(OPFOKLEGHEN!$L$25=\"biofilter\",80%,IF(OPFOKLEGHEN!$L$25=\"waterluchtwassysteem\",33%,IF(OPFOKLEGHEN!$L$25=\"droogfilterwand\",40%,IF(OPFOKLEGHEN!$L$25=\"ionisatiefilter\",57%,IF(OPFOKLEGHEN!$L$25=\"luchtconditioneringsunit\",IF(OPFOKLEGHEN!$M$26=\"Luchtconditioneringsunit niet combineren met techniek buiten stal\",\"error\",80%),0)))))))))","v":0},null,{"$f":"ROUND(IF(OPFOKLEGHEN!$H$13=\"SERIE GESCHAKELD MET WARMTEWISSELAAR\",AC138*G10,IF(OPFOKLEGHEN!$H$13=\"PARALLEL GESCHAKELD MET WARMTEWISSELAAR\",AD138*G10)),3)","v":0},{"$f":"OPFOKLEGHEN!$J$18","v":"NEE"},"WW",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Serie geschakeld","Parallel geschakeld"]
[null,null,null,null," ","hulprek",{"$f":"IF(OPFOKLEGHEN!$H$13=\"SERIE GESCHAKELD MET WARMTEWISSELAAR\",IF(OPFOKLEGHEN!$H$20=\"nee\",0.8,0.65),IF(OPFOKLEGHEN!$H$13=\"Parallel GESCHAKELD MET WARMTEWISSELAAR\",IF(OPFOKLEGHEN!$H$20=\"nee\",1,0.94)))","v":1}]
["Totale gemiddelde reductiepercentage op stalniveau:",null,null,null," ",null," ",null,null,"droogt. en wwlaar parallel geschakeld (wwlaar als basis voor ventilatie, daarna droogt.)",null,null,null,null,null,null,null,null," "]
[null,null,null,{"$f":"IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$5,C17),MIN(C17,I$5))","v":0},null,null,null,null,null,"droogt. en wwlaar serie geschakeld (lucht eerst door droogt.)",null,null,null,null,{"$f":"K34-(D34/C34*K34*I$6*(1-55%))","v":0.69523404514079346}]
[null,null,null,{"$f":"OPFOKLEGHEN!$H$13","v":"PARALLEL GESCHAKELD MET WARMTEWISSELAAR"},null,null,null,null,null,null,null,null,null,{"$f":"(1-$I$6)/(C53-D53)/C53","v":4.534403644369676},{"$f":"(1-($I$6*(D49-E49)))*$C49/$D49","v":{"$error":"#DIV/0!"}},null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"Berekening droogt. en wwlaar in serie geschakeld. Lucht eerst door droogtunnel",null,null,null,null,null,null,null,null,null,"Emissie bij toepassing luchtwasser: wwlaar en droogtunnel parallel"]
["Wk","Lft","Debiet","Debiet door WWlaar (m3/dier/uur)","Debiet door droogtunnel (m3/dier/uur) serie geschakeld","Debiet door droogtunnel (m3/dier/uur) parallel geschakeld","Debiet door stoffilter (m3/dier/uur) ","Debiet door overige techniek","Debiet hoofdventilatie (m3/dier/uur)","PM10 concentratie (mg/m3)","PM10 emissie zonder reductie (gr/d/jaar)","Cumulatief aandeel emissie","PM10 emissie met reductie staltechniek (gr/d/jaar)","PM10 emissie wwlaar  parallel","PM10 emissie wwlaar serie","PM10 emissie droogtunnel  (gr/d/jaar) serie","PM10 emissie droogtunnel  (gr/d/jaar) parallel","Emissie alleen Stoffilter","Emissie Stoffilter na ww droogtunnel","PM10 emissie wwlaar en drtunnel parallel en staltechniek (gr/d/jaar)","PM10 emissie wwlaar en drtunnel parallel en staltechniek en luchtwasser (gr/d/jaar)","Potentie Reductie overige techniek","Potentie Reductie overige techniek,      nee, nee, nee","Potentie Reductie overige techniek,      nee, ja droogtunnel, nee","Potentie Reductie overige techniek,      nee, ja droogtunnel, ja ww naar overig","100% minus reductie",null,null,null,null,"Debiet door droogtunnel (m3/dier/ uur)","PM10 conc. na droogtunnel (mg/m3)","PM10 emissie na droogtunnel (gr/d/jaar)","Debiet door WWlaar (m3/dier/ uur)","PM10 conc. na wwlaar (mg/m3)","PM10 emissie uit wwlaar (gr/d/jaar)","Debiet hoofd-ventilatie (m3/dier/uur)","PM10 emissie hoofddebiet (gr/d/jaar)","Wk","Lft","gew br","gew wit","gem gew","Totale PM10 emissie (gr/d/jaar)"]
[1,1,{"$f":"0.000000000384*AQ16^3-0.000000342064*AQ16^2+0.001060852819*AQ16+0.088327034395","v":0.135046348130446},{"$f":"MIN(C16,J$5)","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C16)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C16<$I$3,C16-D16,MIN($I$3,C16-D16))))","v":0},{"$f":"IF(C16<$I$7,MAX(0,C16-D16-E16-F16,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C16-D16-F16)),MIN(I$7,MAX(0,C16-D16-E16-F16))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C16-D16-E16-F16,MIN(I$7,C16-E16-F16)),MIN(I$7,MAX(0,C16-D16-F16))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C16-F16-G16,C16-D16-F16-G16),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C16-G16,IF(OPFOKLEGHEN!$J$18=\"nee\",C16-D16-G16)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C16-G16,C16-D16-F16-G16),C16-D16-F16-G16))","v":0.135046348130446},{"$f":"IF(C16-D16-E16<0, 0, C16-D16-E16)","v":0.135046348130446},0.21206634125781271,{"$f":"(J16/1000)*C16*24*365","v":0.25087575614669222},{"$f":"SUM(K$16:K16)/$K$137","v":2.9378557518576937E-4},{"$f":"(((($J16/1000)*(1-$I$8))*$B16*$C16))","v":2.8638784948252538E-5},{"$f":"(((($K16)*(1-($I$6*(D16)/C16)))))","v":0.25087575614669222},{"$f":"IF(E16<I$3,P16*(1-I$6*D16/C16),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P16*(1-$I$6)+(C16-D16)/C16*(K16-P16*(1-I$6)),P16*(1-$I$6)+(C16-D16)/C16*(K16-P16*(1-I$6))))","v":0.25087575614669222},{"$f":"IF(E16=0,K16,K16-K16*I$4*E16/C16)","v":0.25087575614669222},{"$f":"IF(F16=0,K16,K16-K16*I$4*F16/C16)","v":0.25087575614669222},{"$f":"K16-(G16/C16)*K16*97.25%","v":0.25087575614669222},{"$f":"MIN(K16,K16-(G16/C16)*(K16)*96.5%)","v":0.25087575614669222},{"$f":"(((($J16/1000)*(1-$I$8))*$B16*$I16)*(1-$I$9))+(((($J16/1000)*(1-$I$8))*$B16*$D16)*(1-$I$6))+(((($J16/1000)*(1-$I$8))*$B16*$E16)*(1-$I$4))","v":2.8638784948252538E-5},{"$f":"(($AP16/1000)*(1-$I$10)*$D16*$B16)+(($AQ16/1000)*(1-$I$10)*$E16*$B16)","v":0},{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H16/C16*K16,IF(OPFOKLEGHEN!$H$20=\"ja\",O16-(K16-Q16)-(K16-S16),Q16-(K16-O16)-(K16-S16)))","v":0.25087575614669222},{"$f":"IF(H16=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q16-(K16-R16)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O16*80%-(K16-S16)),(Q16-(K16-S16)-(K16-T16))),(N16-(K16-S16))))","v":0.50175151229338444},{"$f":"IF(H16=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q16-(K16-R16)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O16*80%-(K16-S16)),(Q16-(K16-S16/80%)-(K16-N16/80%))),(N16-(K16-S16))))","v":0.50175151229338444},{"$f":"IF(H16=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q16-(K16-R16)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O16-(K16-S16)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N16-(K16-Q16)-(K16-S16)),(Q16-(K16-N16/80%)))))),(O16-(K16-S16))))","v":0.50175151229338444},{"$f":"Q16/K16","v":1},null,null,{"$f":"IF(H16=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P16-(K16-R16),O16-(K16-R16)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O16-(K16-S16),IF(OPFOKLEGHEN!$H$20=\"nee\",(O16-(K16-S16)),(O16-(K16-S16)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O16*80%-(K16-S16),0+O16-(K16-S16)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O16*80%-(K16-S16)),O16*93%-(K16-S16)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O16-(K16-S16))),O16-(K16-S16))),6)),8)))","v":0.25087575614669222},{"$f":"IF(H16=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q16-(K16-R16),N16-(K16-R16)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q16-(K16-N16)-(K16-S16),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q16-(K16-N16)-(K16-S16)),(O16-(K16-S16)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q16*$N$135-(K16-N16)-(K16-S16),(Q16-(K16-N16)-(K16-S16))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N16*95%-(K16-Q16)/I$4-(K16-S16)),N16-(K16-Q16)/I$4-(K16-S16)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N16-(K16-Q16)/I$4-(K16-S16))),N16-(K16-Q16)/I$4-(K16-S16))))))))","v":0.25087575614669222},{"$f":"IF((D16+E16)<$I$3,D16+E16,$I$3)","v":0},{"$f":"IF($I$3>0,(J16*(1-$I$8)*(1-$I$4)),(J16*(1-$I$8)))","v":0.21206634125781271},{"$f":"($AF16/1000)*$B16*$AE16","v":0},{"$f":"D16","v":0},{"$f":"IF($I$5>0,AF16*(1-$I$6),AF16)","v":0.21206634125781271},{"$f":"(AI16/1000)*B16*AH16","v":0},{"$f":"IF($I$3>$I$5,C16-AE16,C16-AH16)","v":0.135046348130446},{"$f":"((($J16/1000)*(1-$I$8))*$B16*$AK16)*(1-$I$9)","v":2.8638784948252538E-5},1,1,45,44.3,{"$f":"(AO16+AP16)/2","v":44.65},{"$f":"(($AP16/1000)*(1-$I$10)*$D16*$B16)+(($AQ16/1000)*(1-$I$10)*$E16*$B16)+(($AO16/1000)*(1-$I$10)*$I16*$B16)","v":6.0770856658700695E-3}]
[1,2,{"$f":"0.000000000384*AQ17^3-0.000000342064*AQ17^2+0.001060852819*AQ17+0.088327034395","v":0.13984170733262799},0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C17)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C17<$I$3,C17-D17,MIN($I$3,C17-D17))))","v":0},{"$f":"IF(C17<$I$7,MAX(0,C17-D17-E17-F17,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C17-D17-F17)),MIN(I$7,MAX(0,C17-D17-E17-F17))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C17-D17-E17-F17,MIN(I$7,C17-E17-F17)),MIN(I$7,MAX(0,C17-D17-F17))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C17-F17-G17,C17-D17-F17-G17),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C17-G17,IF(OPFOKLEGHEN!$J$18=\"nee\",C17-D17-G17)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C17-G17,C17-D17-F17-G17),C17-D17-F17-G17))","v":0.13984170733262799},{"$f":"IF(C17-D17-E17<0, 0, C17-D17-E17)","v":0.13984170733262799},0.21600448172178227,{"$f":"(J17/1000)*C17*24*365","v":0.26460837511554758},{"$f":"SUM(K$16:K17)/$K$137","v":6.0365259811499133E-4},{"$f":"(((($J17/1000)*(1-$I$8))*$B17*$C17))","v":6.0412871030946938E-5},0.26460837511554758,{"$f":"IF(E17<I$3,P17*(1-I$6*D17/C17),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P17*(1-$I$6)+(C17-D17)/C17*(K17-P17*(1-I$6)),P17*(1-$I$6)+(C17-D17)/C17*(K17-P17*(1-I$6))))","v":0.26460837511554758},0.26460837511554758,0.26460837511554758,0.26460837511554758,0.26460837511554758,{"$f":"$K17*(1-($I$6*(D17)/C17))","v":0.26460837511554758},{"$f":"(($AP17/1000)*(1-$I$10)*$D17*$B17)+(($AQ17/1000)*(1-$I$10)*$E17*$B17)+(($AO17/1000)*(1-$I$10)*$I17*$B17)","v":1.39841707332628E-2},{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H17/C17*K17,IF(OPFOKLEGHEN!$H$20=\"ja\",O17-(K17-Q17)-(K17-S17),Q17-(K17-O17)-(K17-S17)))","v":0.26460837511554758},{"$f":"IF(H17=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q17-(K17-R17)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O17*80%-(K17-S17)),(Q17-(K17-S17)-(K17-T17))),(N17-(K17-S17))))","v":0.52921675023109516},{"$f":"IF(H17=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q17-(K17-R17)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O17*80%-(K17-S17)),(Q17-(K17-S17)-(K17-N17))),(N17-(K17-S17))))","v":0.52921675023109516},{"$f":"IF(H17=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q17-(K17-R17)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O17-(K17-S17)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N17-(K17-Q17)-(K17-S17)),(Q17-(K17-N17/80%)))))),(O17-(K17-S17))))","v":0.52921675023109516},1,null,null,{"$f":"IF(H17=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P17-(K17-R17),K17-(K17-O17)/I$6-(K17-R17)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K17-O17)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O17-(K17-S17),IF(OPFOKLEGHEN!$H$20=\"nee\",(O17-(K17-S17)),(O17-(K17-S17)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O17*80%-(K17-S17),0+O17-(K17-S17)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O17*80%-(K17-S17)),O17*93%-(K17-S17)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O17-(K17-S17))),O17-(K17-S17))))))))","v":0.26460837511554758},{"$f":"IF(H17=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q17-(K17-R17),N17-(K17-R17)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q17-(K17-N17)-(K17-S17),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q17-(K17-N17)-(K17-S17)),(O17-(K17-S17)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q17*$N$135-(K17-N17)-(K17-S17),(Q17-(K17-N17)-(K17-S17))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N17*95%-(K17-Q17)/I$4-(K17-S17)),N17-(K17-Q17)/I$4-(K17-S17)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N17-(K17-Q17)/I$4-(K17-S17))),N17-(K17-Q17)/I$4-(K17-S17))))))))","v":0.26460837511554758},0,0.21600448172178227,0,0,{"$f":"IF($I$5>0,AF17*(1-$I$6),AF17)","v":0.21600448172178227},0,0.13984170733262799,6.0412871030946938E-5,1,2,50,48.6,{"$f":"(AO17+AP17)/2","v":49.3},1.39841707332628E-2]
[1,3,0.144624730016362,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C18)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C18<$I$3,C18-D18,MIN($I$3,C18-D18))))","v":0},{"$f":"IF(C18<$I$7,MAX(0,C18-D18-E18-F18,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C18-D18-F18)),MIN(I$7,MAX(0,C18-D18-E18-F18))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C18-D18-E18-F18,MIN(I$7,C18-E18-F18)),MIN(I$7,MAX(0,C18-D18-F18))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C18-F18-G18,C18-D18-F18-G18),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C18-G18,IF(OPFOKLEGHEN!$J$18=\"nee\",C18-D18-G18)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C18-G18,C18-D18-F18-G18),C18-D18-F18-G18))","v":0.144624730016362},0.144624730016362,0.22001575472636142,0.27874073954942025,{"$f":"SUM(K$16:K18)/$K$137","v":9.3006918676435599E-4},9.5459157379938436E-5,0.27874073954942025,{"$f":"IF(E18<I$3,P18*(1-I$6*D18/C18),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P18*(1-$I$6)+(C18-D18)/C18*(K18-P18*(1-I$6)),P18*(1-$I$6)+(C18-D18)/C18*(K18-P18*(1-I$6))))","v":0.27874073954942025},0.27874073954942025,0.27874073954942025,0.27874073954942025,{"$f":"MIN(K18,K18-(G18/C18)*(Q18)*95%)","v":0.27874073954942025},{"$f":"$K18*(1-($I$6*(D18)/C18))-($I$4*F18/C18)","v":0.27874073954942025},{"$f":"(($AP18/1000)*(1-$I$10)*$D18*$B18)+(($AQ18/1000)*(1-$I$10)*$E18*$B18)+(($AO18/1000)*(1-$I$10)*$I18*$B18)","v":2.3863080452699727E-2},{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H18/C18*K18,IF(OPFOKLEGHEN!$H$20=\"ja\",O18-(K18-Q18)-(K18-S18),Q18-(K18-O18)-(K18-S18)))","v":0.27874073954942025},{"$f":"IF(H18=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q18-(K18-R18)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O18*80%-(K18-S18)),(Q18-(K18-S18)-(K18-T18))),(N18-(K18-S18))))","v":0.55748147909884049},{"$f":"IF(H18=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q18-(K18-R18)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O18*80%-(K18-S18)),(Q18-(K18-S18)-(K18-N18))),(N18-(K18-S18))))","v":0.55748147909884049},{"$f":"IF(H18=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q18-(K18-R18)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O18-(K18-S18)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N18-(K18-Q18)-(K18-S18)),(Q18-(K18-N18/80%)))))),(O18-(K18-S18))))","v":0.55748147909884049},1,null,null,{"$f":"IF(H18=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P18-(K18-R18),K18-(K18-O18)/I$6-(K18-R18)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K18-O18)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O18-(K18-S18),IF(OPFOKLEGHEN!$H$20=\"nee\",(O18-(K18-S18)),(O18-(K18-S18)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O18*80%-(K18-S18),0+O18-(K18-S18)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O18*80%-(K18-S18)),O18*93%-(K18-S18)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O18-(K18-S18))),O18-(K18-S18))))))))","v":0.27874073954942025},{"$f":"IF(H18=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q18-(K18-R18),N18-(K18-R18)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q18-(K18-N18)-(K18-S18),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q18-(K18-N18)-(K18-S18)),(O18-(K18-S18)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q18*$N$135-(K18-N18)-(K18-S18),(Q18-(K18-N18)-(K18-S18))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N18*95%-(K18-Q18)/I$4-(K18-S18)),N18-(K18-Q18)/I$4-(K18-S18)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N18-(K18-Q18)/I$4-(K18-S18))),N18-(K18-Q18)/I$4-(K18-S18))))))))","v":0.27874073954942025},0,0.22001575472636142,0,0,0.22001575472636142,0,0.144624730016362,9.5459157379938436E-5,1,3,55,52.9,53.95,2.3863080452699727E-2]
[1,4,0.149395647836464,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C19)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C19<$I$3,C19-D19,MIN($I$3,C19-D19))))","v":0},{"$f":"IF(C19<$I$7,MAX(0,C19-D19-E19-F19,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C19-D19-F19)),MIN(I$7,MAX(0,C19-D19-E19-F19))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C19-D19-E19-F19,MIN(I$7,C19-E19-F19)),MIN(I$7,MAX(0,C19-D19-F19))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C19-F19-G19,C19-D19-F19-G19),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C19-G19,IF(OPFOKLEGHEN!$J$18=\"nee\",C19-D19-G19)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C19-G19,C19-D19-F19-G19),C19-D19-F19-G19))","v":0.149395647836464},0.149395647836464,0.22410151836645426,0.29328297369322703,{"$f":"SUM(K$16:K19)/$K$137","v":1.2735153150075201E-3},1.3391916606996667E-4,0.29328297369322703,{"$f":"IF(E19<I$3,P19*(1-I$6*D19/C19),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P19*(1-$I$6)+(C19-D19)/C19*(K19-P19*(1-I$6)),P19*(1-$I$6)+(C19-D19)/C19*(K19-P19*(1-I$6))))","v":0.29328297369322703},0.29328297369322703,0.29328297369322703,0.29328297369322703,0.29328297369322703,0.29328297369322703,{"$f":"(($AP19/1000)*(1-$I$10)*$D19*$B19)+(($AQ19/1000)*(1-$I$10)*$E19*$B19)+(($AO19/1000)*(1-$I$10)*$I19*$B19)","v":3.5854955480751356E-2},{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H19/C19*K19,IF(OPFOKLEGHEN!$H$20=\"ja\",O19-(K19-Q19)-(K19-S19),Q19-(K19-O19)-(K19-S19)))","v":0.29328297369322703},{"$f":"IF(H19=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q19-(K19-R19)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O19*80%-(K19-S19)),(Q19-(K19-S19)-(K19-T19))),(N19-(K19-S19))))","v":0.58656594738645407},{"$f":"IF(H19=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q19-(K19-R19)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O19*80%-(K19-S19)),(Q19-(K19-S19)-(K19-N19))),(N19-(K19-S19))))","v":0.58656594738645407},{"$f":"IF(H19=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q19-(K19-R19)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O19-(K19-S19)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N19-(K19-Q19)-(K19-S19)),(Q19-(K19-N19/80%)))))),(O19-(K19-S19))))","v":0.58656594738645407},1,null,null,{"$f":"IF(H19=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P19-(K19-R19),K19-(K19-O19)/I$6-(K19-R19)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K19-O19)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O19-(K19-S19),IF(OPFOKLEGHEN!$H$20=\"nee\",(O19-(K19-S19)),(O19-(K19-S19)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O19*80%-(K19-S19),0+O19-(K19-S19)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O19*80%-(K19-S19)),O19*93%-(K19-S19)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O19-(K19-S19))),O19-(K19-S19))))))))","v":0.29328297369322703},{"$f":"IF(H19=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q19-(K19-R19),N19-(K19-R19)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q19-(K19-N19)-(K19-S19),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q19-(K19-N19)-(K19-S19)),(O19-(K19-S19)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q19*$N$135-(K19-N19)-(K19-S19),(Q19-(K19-N19)-(K19-S19))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N19*95%-(K19-Q19)/I$4-(K19-S19)),N19-(K19-Q19)/I$4-(K19-S19)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N19-(K19-Q19)/I$4-(K19-S19))),N19-(K19-Q19)/I$4-(K19-S19))))))))","v":0.29328297369322703},0,0.22410151836645426,0,0,0.22410151836645426,0,0.149395647836464,1.3391916606996667E-4,1,4,60,57.2,58.6,3.5854955480751356E-2]
[1,5,0.15415469244774999,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C20)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C20<$I$3,C20-D20,MIN($I$3,C20-D20))))","v":0},{"$f":"IF(C20<$I$7,MAX(0,C20-D20-E20-F20,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C20-D20-F20)),MIN(I$7,MAX(0,C20-D20-E20-F20))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C20-D20-E20-F20,MIN(I$7,C20-E20-F20)),MIN(I$7,MAX(0,C20-D20-F20))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C20-F20-G20,C20-D20-F20-G20),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C20-G20,IF(OPFOKLEGHEN!$J$18=\"nee\",C20-D20-G20)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C20-G20,C20-D20-F20-G20),C20-D20-F20-G20))","v":0.15415469244774999},0.15415469244774999,0.22826315595722607,0.30824544864875342,{"$f":"SUM(K$16:K20)/$K$137","v":1.6344831016944024E-3},1.7593918301869488E-4,0.30824544864875342,{"$f":"IF(E20<I$3,P20*(1-I$6*D20/C20),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P20*(1-$I$6)+(C20-D20)/C20*(K20-P20*(1-I$6)),P20*(1-$I$6)+(C20-D20)/C20*(K20-P20*(1-I$6))))","v":0.30824544864875342},0.30824544864875342,0.30824544864875342,0.30824544864875342,{"$f":"MIN(K20,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K20-(G20/(C20-G20))*(Q20)*95%,K20-(G20/(C20-G20))*(P20)*84%))","v":0.30824544864875342},0.30824544864875342,{"$f":"AR20","v":5.0100275045518741E-2},{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H20/C20*K20,IF(OPFOKLEGHEN!$H$20=\"ja\",O20-(K20-Q20)-(K20-S20),Q20-(K20-O20)-(K20-S20)))","v":0.30824544864875342},{"$f":"IF(H20=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q20-(K20-R20)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O20*80%-(K20-S20)),(Q20-(K20-S20)-(K20-T20))),(N20-(K20-S20))))","v":0.61649089729750683},{"$f":"IF(H20=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q20-(K20-R20)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O20*80%-(K20-S20)),(Q20-(K20-S20)-(K20-N20))),(N20-(K20-S20))))","v":0.61649089729750683},{"$f":"IF(H20=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q20-(K20-R20)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O20-(K20-S20)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N20-(K20-Q20)-(K20-S20)),(Q20-(K20-N20/80%)))))),(O20-(K20-S20))))","v":0.61649089729750683},1,null,null,{"$f":"IF(H20=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P20-(K20-R20),K20-(K20-O20)/I$6-(K20-R20)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K20-O20)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O20-(K20-S20),IF(OPFOKLEGHEN!$H$20=\"nee\",(O20-(K20-S20)),(O20-(K20-S20)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O20*80%-(K20-S20),0+O20-(K20-S20)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O20*80%-(K20-S20)),O20*93%-(K20-S20)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O20-(K20-S20))),O20-(K20-S20))))))))","v":0.30824544864875342},{"$f":"IF(H20=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q20-(K20-R20),N20-(K20-R20)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q20-(K20-N20)-(K20-S20),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q20-(K20-N20)-(K20-S20)),(O20-(K20-S20)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q20*$N$135-(K20-N20)-(K20-S20),(Q20-(K20-N20)-(K20-S20))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N20*95%-(K20-Q20)/I$4-(K20-S20)),N20-(K20-Q20)/I$4-(K20-S20)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N20-(K20-Q20)/I$4-(K20-S20))),N20-(K20-Q20)/I$4-(K20-S20))))))))","v":0.30824544864875342},0,0.22826315595722607,0,0,0.22826315595722607,0,0.15415469244774999,1.7593918301869488E-4,1,5,65,61.5,63.25,5.0100275045518741E-2]
[1,6,0.15890209550503601,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C21)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C21<$I$3,C21-D21,MIN($I$3,C21-D21))))","v":0},{"$f":"IF(C21<$I$7,MAX(0,C21-D21-E21-F21,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C21-D21-F21)),MIN(I$7,MAX(0,C21-D21-E21-F21))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C21-D21-E21-F21,MIN(I$7,C21-E21-F21)),MIN(I$7,MAX(0,C21-D21-F21))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C21-F21-G21,C21-D21-F21-G21),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C21-G21,IF(OPFOKLEGHEN!$J$18=\"nee\",C21-D21-G21)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C21-G21,C21-D21-F21-G21),C21-D21-F21-G21))","v":0.15890209550503601},0.15890209550503601,0.23250207650245164,0.32363878836988297,{"$f":"SUM(K$16:K21)/$K$137","v":2.0134771067511371E-3},2.2167040299307057E-4,0.32363878836988297,{"$f":"IF(E21<I$3,P21*(1-I$6*D21/C21),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P21*(1-$I$6)+(C21-D21)/C21*(K21-P21*(1-I$6)),P21*(1-$I$6)+(C21-D21)/C21*(K21-P21*(1-I$6))))","v":0.32363878836988297},0.32363878836988297,0.32363878836988297,0.32363878836988297,{"$f":"MIN(K21,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K21-(G21/(C21-G21))*(Q21)*95%,K21-(G21/(C21-G21))*(P21)*84%))","v":0.32363878836988297},0.32363878836988297,6.6738880112115123E-2,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H21/C21*K21,IF(OPFOKLEGHEN!$H$20=\"ja\",O21-(K21-Q21)-(K21-S21),Q21-(K21-O21)-(K21-S21)))","v":0.32363878836988297},{"$f":"IF(H21=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q21-(K21-R21)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O21*80%-(K21-S21)),(Q21-(K21-S21)-(K21-T21))),(N21-(K21-S21))))","v":0.64727757673976594},{"$f":"IF(H21=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q21-(K21-R21)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O21*80%-(K21-S21)),(Q21-(K21-S21)-(K21-N21))),(N21-(K21-S21))))","v":0.64727757673976594},{"$f":"IF(H21=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q21-(K21-R21)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O21-(K21-S21)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N21-(K21-Q21)-(K21-S21)),(Q21-(K21-N21/80%)))))),(O21-(K21-S21))))","v":0.64727757673976594},1,null,null,{"$f":"IF(H21=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P21-(K21-R21),K21-(K21-O21)/I$6-(K21-R21)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K21-O21)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O21-(K21-S21),IF(OPFOKLEGHEN!$H$20=\"nee\",(O21-(K21-S21)),(O21-(K21-S21)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O21*80%-(K21-S21),0+O21-(K21-S21)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O21*80%-(K21-S21)),O21*93%-(K21-S21)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O21-(K21-S21))),O21-(K21-S21))))))))","v":0.32363878836988297},{"$f":"IF(H21=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q21-(K21-R21),N21-(K21-R21)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q21-(K21-N21)-(K21-S21),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q21-(K21-N21)-(K21-S21)),(O21-(K21-S21)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q21*$N$135-(K21-N21)-(K21-S21),(Q21-(K21-N21)-(K21-S21))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N21*95%-(K21-Q21)/I$4-(K21-S21)),N21-(K21-Q21)/I$4-(K21-S21)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N21-(K21-Q21)/I$4-(K21-S21))),N21-(K21-Q21)/I$4-(K21-S21))))))))","v":0.32363878836988297},0,0.23250207650245164,0,0,0.23250207650245164,0,0.15890209550503601,2.2167040299307057E-4,1,6,70,65.8,67.900000000000006,6.6738880112115123E-2]
[1,7,0.16358722387249999,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C22)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C22<$I$3,C22-D22,MIN($I$3,C22-D22))))","v":0},{"$f":"IF(C22<$I$7,MAX(0,C22-D22-E22-F22,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C22-D22-F22)),MIN(I$7,MAX(0,C22-D22-E22-F22))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C22-D22-E22-F22,MIN(I$7,C22-E22-F22)),MIN(I$7,MAX(0,C22-D22-F22))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C22-F22-G22,C22-D22-F22-G22),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C22-G22,IF(OPFOKLEGHEN!$J$18=\"nee\",C22-D22-G22)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C22-G22,C22-D22-F22-G22),C22-D22-F22-G22))","v":0.16358722387249999},0.16358722387249999,0.23681971517156092,0.33936835472556032,{"$f":"SUM(K$16:K22)/$K$137","v":2.4108910650556589E-3},2.7118475834234275E-4,0.33936835472556032,{"$f":"IF(E22<I$3,P22*(1-I$6*D22/C22),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P22*(1-$I$6)+(C22-D22)/C22*(K22-P22*(1-I$6)),P22*(1-$I$6)+(C22-D22)/C22*(K22-P22*(1-I$6))))","v":0.33936835472556032},0.33936835472556032,0.33936835472556032,0.33936835472556032,{"$f":"MIN(K22,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K22-(G22/(C22-G22))*(Q22)*95%,K22-(G22/(C22-G22))*(P22)*84%))","v":0.33936835472556032},0.33936835472556032,8.5883292533062497E-2,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H22/C22*K22,IF(OPFOKLEGHEN!$H$20=\"ja\",O22-(K22-Q22)-(K22-S22),Q22-(K22-O22)-(K22-S22)))","v":0.33936835472556032},{"$f":"IF(H22=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q22-(K22-R22)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O22*80%-(K22-S22)),(Q22-(K22-S22)-(K22-T22))),(N22-(K22-S22))))","v":0.67873670945112063},{"$f":"IF(H22=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q22-(K22-R22)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O22*80%-(K22-S22)),(Q22-(K22-S22)-(K22-N22))),(N22-(K22-S22))))","v":0.67873670945112063},{"$f":"IF(H22=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q22-(K22-R22)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O22-(K22-S22)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N22-(K22-Q22)-(K22-S22)),(Q22-(K22-N22/80%)))))),(O22-(K22-S22))))","v":0.67873670945112063},1,null,null,{"$f":"IF(H22=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P22-(K22-R22),K22-(K22-O22)/I$6-(K22-R22)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K22-O22)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O22-(K22-S22),IF(OPFOKLEGHEN!$H$20=\"nee\",(O22-(K22-S22)),(O22-(K22-S22)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O22*80%-(K22-S22),0+O22-(K22-S22)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O22*80%-(K22-S22)),O22*93%-(K22-S22)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O22-(K22-S22))),O22-(K22-S22))))))))","v":0.33936835472556032},{"$f":"IF(H22=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q22-(K22-R22),N22-(K22-R22)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q22-(K22-N22)-(K22-S22),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q22-(K22-N22)-(K22-S22)),(O22-(K22-S22)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q22*$N$135-(K22-N22)-(K22-S22),(Q22-(K22-N22)-(K22-S22))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N22*95%-(K22-Q22)/I$4-(K22-S22)),N22-(K22-Q22)/I$4-(K22-S22)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N22-(K22-Q22)/I$4-(K22-S22))),N22-(K22-Q22)/I$4-(K22-S22))))))))","v":0.33936835472556032},0,0.23681971517156092,0,0,0.23681971517156092,0,0.16358722387249999,2.7118475834234275E-4,1,7,75,70,72.5,8.5883292533062497E-2]
[2,8,0.17191198275905201,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C23)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C23<$I$3,C23-D23,MIN($I$3,C23-D23))))","v":0},{"$f":"IF(C23<$I$7,MAX(0,C23-D23-E23-F23,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C23-D23-F23)),MIN(I$7,MAX(0,C23-D23-E23-F23))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C23-D23-E23-F23,MIN(I$7,C23-E23-F23)),MIN(I$7,MAX(0,C23-D23-F23))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C23-F23-G23,C23-D23-F23-G23),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C23-G23,IF(OPFOKLEGHEN!$J$18=\"nee\",C23-D23-G23)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C23-G23,C23-D23-F23-G23),C23-D23-F23-G23))","v":0.17191198275905201},0.17191198275905201,0.24121753378554392,0.36326129630165616,{"$f":"SUM(K$16:K23)/$K$137","v":2.8362846164927628E-3},3.3174547607457179E-4,0.36326129630165616,{"$f":"IF(E23<I$3,P23*(1-I$6*D23/C23),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P23*(1-$I$6)+(C23-D23)/C23*(K23-P23*(1-I$6)),P23*(1-$I$6)+(C23-D23)/C23*(K23-P23*(1-I$6))))","v":0.36326129630165616},0.36326129630165616,0.36326129630165616,0.36326129630165616,{"$f":"MIN(K23,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K23-(G23/(C23-G23))*(Q23)*95%,K23-(G23/(C23-G23))*(P23)*84%))","v":0.36326129630165616},0.36326129630165616,0.11497473406925397,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H23/C23*K23,IF(OPFOKLEGHEN!$H$20=\"ja\",O23-(K23-Q23)-(K23-S23),Q23-(K23-O23)-(K23-S23)))","v":0.36326129630165616},{"$f":"IF(H23=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q23-(K23-R23)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O23*80%-(K23-S23)),(Q23-(K23-S23)-(K23-T23))),(N23-(K23-S23))))","v":0.72652259260331231},{"$f":"IF(H23=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q23-(K23-R23)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O23*80%-(K23-S23)),(Q23-(K23-S23)-(K23-N23))),(N23-(K23-S23))))","v":0.72652259260331231},{"$f":"IF(H23=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q23-(K23-R23)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O23-(K23-S23)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N23-(K23-Q23)-(K23-S23)),(Q23-(K23-N23/80%)))))),(O23-(K23-S23))))","v":0.72652259260331231},1,null,null,{"$f":"IF(H23=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P23-(K23-R23),K23-(K23-O23)/I$6-(K23-R23)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K23-O23)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O23-(K23-S23),IF(OPFOKLEGHEN!$H$20=\"nee\",(O23-(K23-S23)),(O23-(K23-S23)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O23*80%-(K23-S23),0+O23-(K23-S23)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O23*80%-(K23-S23)),O23*93%-(K23-S23)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O23-(K23-S23))),O23-(K23-S23))))))))","v":0.36326129630165616},{"$f":"IF(H23=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q23-(K23-R23),N23-(K23-R23)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q23-(K23-N23)-(K23-S23),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q23-(K23-N23)-(K23-S23)),(O23-(K23-S23)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q23*$N$135-(K23-N23)-(K23-S23),(Q23-(K23-N23)-(K23-S23))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N23*95%-(K23-Q23)/I$4-(K23-S23)),N23-(K23-Q23)/I$4-(K23-S23)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N23-(K23-Q23)/I$4-(K23-S23))),N23-(K23-Q23)/I$4-(K23-S23))))))))","v":0.36326129630165616},0,0.24121753378554392,0,0,0.24121753378554392,0,0.17191198275905201,3.3174547607457179E-4,2,8,{"$f":"AO22+8.6","v":83.6},{"$f":"AP22+7.8","v":77.8},80.699999999999989,0.11497473406925397]
[2,9,0.18020324300035601,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C24)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C24<$I$3,C24-D24,MIN($I$3,C24-D24))))","v":0},{"$f":"IF(C24<$I$7,MAX(0,C24-D24-E24-F24,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C24-D24-F24)),MIN(I$7,MAX(0,C24-D24-E24-F24))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C24-D24-E24-F24,MIN(I$7,C24-E24-F24)),MIN(I$7,MAX(0,C24-D24-F24))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C24-F24-G24,C24-D24-F24-G24),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C24-G24,IF(OPFOKLEGHEN!$J$18=\"nee\",C24-D24-G24)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C24-G24,C24-D24-F24-G24),C24-D24-F24-G24))","v":0.18020324300035601},0.18020324300035601,0.24569702131187857,0.38785250431473017,{"$f":"SUM(K$16:K24)/$K$137","v":3.2904754590734938E-3},3.9847860032335289E-4,0.38785250431473017,{"$f":"IF(E24<I$3,P24*(1-I$6*D24/C24),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P24*(1-$I$6)+(C24-D24)/C24*(K24-P24*(1-I$6)),P24*(1-$I$6)+(C24-D24)/C24*(K24-P24*(1-I$6))))","v":0.38785250431473017},0.38785250431473017,0.38785250431473017,0.38785250431473017,{"$f":"MIN(K24,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K24-(G24/(C24-G24))*(Q24)*95%,K24-(G24/(C24-G24))*(P24)*84%))","v":0.38785250431473017},0.38785250431473017,0.14953265104169539,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H24/C24*K24,IF(OPFOKLEGHEN!$H$20=\"ja\",O24-(K24-Q24)-(K24-S24),Q24-(K24-O24)-(K24-S24)))","v":0.38785250431473017},{"$f":"IF(H24=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q24-(K24-R24)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O24*80%-(K24-S24)),(Q24-(K24-S24)-(K24-T24))),(N24-(K24-S24))))","v":0.77570500862946035},{"$f":"IF(H24=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q24-(K24-R24)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O24*80%-(K24-S24)),(Q24-(K24-S24)-(K24-N24))),(N24-(K24-S24))))","v":0.77570500862946035},{"$f":"IF(H24=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q24-(K24-R24)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O24-(K24-S24)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N24-(K24-Q24)-(K24-S24)),(Q24-(K24-N24/80%)))))),(O24-(K24-S24))))","v":0.77570500862946035},1,null,null,{"$f":"IF(H24=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P24-(K24-R24),K24-(K24-O24)/I$6-(K24-R24)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K24-O24)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O24-(K24-S24),IF(OPFOKLEGHEN!$H$20=\"nee\",(O24-(K24-S24)),(O24-(K24-S24)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O24*80%-(K24-S24),0+O24-(K24-S24)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O24*80%-(K24-S24)),O24*93%-(K24-S24)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O24-(K24-S24))),O24-(K24-S24))))))))","v":0.38785250431473017},{"$f":"IF(H24=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q24-(K24-R24),N24-(K24-R24)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q24-(K24-N24)-(K24-S24),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q24-(K24-N24)-(K24-S24)),(O24-(K24-S24)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q24*$N$135-(K24-N24)-(K24-S24),(Q24-(K24-N24)-(K24-S24))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N24*95%-(K24-Q24)/I$4-(K24-S24)),N24-(K24-Q24)/I$4-(K24-S24)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N24-(K24-Q24)/I$4-(K24-S24))),N24-(K24-Q24)/I$4-(K24-S24))))))))","v":0.38785250431473017},0,0.24569702131187857,0,0,0.24569702131187857,0,0.18020324300035601,3.9847860032335289E-4,2,9,92.199999999999989,85.6,88.899999999999991,0.14953265104169539]
[2,10,0.18846227494828399,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C25)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C25<$I$3,C25-D25,MIN($I$3,C25-D25))))","v":0},{"$f":"IF(C25<$I$7,MAX(0,C25-D25-E25-F25,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C25-D25-F25)),MIN(I$7,MAX(0,C25-D25-E25-F25))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C25-D25-E25-F25,MIN(I$7,C25-E25-F25)),MIN(I$7,MAX(0,C25-D25-F25))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C25-F25-G25,C25-D25-F25-G25),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C25-G25,IF(OPFOKLEGHEN!$J$18=\"nee\",C25-D25-G25)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C25-G25,C25-D25-F25-G25),C25-D25-F25-G25))","v":0.18846227494828399},0.18846227494828399,0.25025969436864992,0.41316111923834348,{"$f":"SUM(K$16:K25)/$K$137","v":3.7743037050713218E-3},4.7164511328578025E-4,0.41316111923834348,{"$f":"IF(E25<I$3,P25*(1-I$6*D25/C25),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P25*(1-$I$6)+(C25-D25)/C25*(K25-P25*(1-I$6)),P25*(1-$I$6)+(C25-D25)/C25*(K25-P25*(1-I$6))))","v":0.41316111923834348},0.41316111923834348,0.41316111923834348,0.41316111923834348,{"$f":"MIN(K25,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K25-(G25/(C25-G25))*(Q25)*95%,K25-(G25/(C25-G25))*(P25)*84%))","v":0.41316111923834348},0.41316111923834348,0.18996997314787023,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H25/C25*K25,IF(OPFOKLEGHEN!$H$20=\"ja\",O25-(K25-Q25)-(K25-S25),Q25-(K25-O25)-(K25-S25)))","v":0.41316111923834348},{"$f":"IF(H25=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q25-(K25-R25)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O25*80%-(K25-S25)),(Q25-(K25-S25)-(K25-T25))),(N25-(K25-S25))))","v":0.82632223847668695},{"$f":"IF(H25=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q25-(K25-R25)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O25*80%-(K25-S25)),(Q25-(K25-S25)-(K25-N25))),(N25-(K25-S25))))","v":0.82632223847668695},{"$f":"IF(H25=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q25-(K25-R25)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O25-(K25-S25)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N25-(K25-Q25)-(K25-S25)),(Q25-(K25-N25/80%)))))),(O25-(K25-S25))))","v":0.82632223847668695},1,null,null,{"$f":"IF(H25=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P25-(K25-R25),K25-(K25-O25)/I$6-(K25-R25)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K25-O25)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O25-(K25-S25),IF(OPFOKLEGHEN!$H$20=\"nee\",(O25-(K25-S25)),(O25-(K25-S25)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O25*80%-(K25-S25),0+O25-(K25-S25)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O25*80%-(K25-S25)),O25*93%-(K25-S25)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O25-(K25-S25))),O25-(K25-S25))))))))","v":0.41316111923834348},{"$f":"IF(H25=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q25-(K25-R25),N25-(K25-R25)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q25-(K25-N25)-(K25-S25),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q25-(K25-N25)-(K25-S25)),(O25-(K25-S25)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q25*$N$135-(K25-N25)-(K25-S25),(Q25-(K25-N25)-(K25-S25))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N25*95%-(K25-Q25)/I$4-(K25-S25)),N25-(K25-Q25)/I$4-(K25-S25)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N25-(K25-Q25)/I$4-(K25-S25))),N25-(K25-Q25)/I$4-(K25-S25))))))))","v":0.41316111923834348},0,0.25025969436864992,0,0,0.25025969436864992,0,0.18846227494828399,4.7164511328578025E-4,2,10,100.79999999999998,93.399999999999991,97.1,0.18996997314787023]
[2,11,0.19669034895470799,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C26)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C26<$I$3,C26-D26,MIN($I$3,C26-D26))))","v":0},{"$f":"IF(C26<$I$7,MAX(0,C26-D26-E26-F26,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C26-D26-F26)),MIN(I$7,MAX(0,C26-D26-E26-F26))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C26-D26-E26-F26,MIN(I$7,C26-E26-F26)),MIN(I$7,MAX(0,C26-D26-F26))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C26-F26-G26,C26-D26-F26-G26),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C26-G26,IF(OPFOKLEGHEN!$J$18=\"nee\",C26-D26-G26)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C26-G26,C26-D26-F26-G26),C26-D26-F26-G26))","v":0.19669034895470799},0.19669034895470799,0.25490709773803089,0.43920683020489637,{"$f":"SUM(K$16:K26)/$K$137","v":4.2886325235236555E-3},5.5151542605637674E-4,0.43920683020489637,{"$f":"IF(E26<I$3,P26*(1-I$6*D26/C26),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P26*(1-$I$6)+(C26-D26)/C26*(K26-P26*(1-I$6)),P26*(1-$I$6)+(C26-D26)/C26*(K26-P26*(1-I$6))))","v":0.43920683020489637},0.43920683020489637,0.43920683020489637,0.43920683020489637,{"$f":"MIN(K26,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K26-(G26/(C26-G26))*(Q26)*95%,K26-(G26/(C26-G26))*(P26)*84%))","v":0.43920683020489637},0.43920683020489637,0.23669716593209555,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H26/C26*K26,IF(OPFOKLEGHEN!$H$20=\"ja\",O26-(K26-Q26)-(K26-S26),Q26-(K26-O26)-(K26-S26)))","v":0.43920683020489637},{"$f":"IF(H26=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q26-(K26-R26)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O26*80%-(K26-S26)),(Q26-(K26-S26)-(K26-T26))),(N26-(K26-S26))))","v":0.87841366040979274},{"$f":"IF(H26=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q26-(K26-R26)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O26*80%-(K26-S26)),(Q26-(K26-S26)-(K26-N26))),(N26-(K26-S26))))","v":0.87841366040979274},{"$f":"IF(H26=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q26-(K26-R26)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O26-(K26-S26)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N26-(K26-Q26)-(K26-S26)),(Q26-(K26-N26/80%)))))),(O26-(K26-S26))))","v":0.87841366040979274},1,null,null,{"$f":"IF(H26=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P26-(K26-R26),K26-(K26-O26)/I$6-(K26-R26)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K26-O26)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O26-(K26-S26),IF(OPFOKLEGHEN!$H$20=\"nee\",(O26-(K26-S26)),(O26-(K26-S26)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O26*80%-(K26-S26),0+O26-(K26-S26)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O26*80%-(K26-S26)),O26*93%-(K26-S26)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O26-(K26-S26))),O26-(K26-S26))))))))","v":0.43920683020489637},{"$f":"IF(H26=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q26-(K26-R26),N26-(K26-R26)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q26-(K26-N26)-(K26-S26),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q26-(K26-N26)-(K26-S26)),(O26-(K26-S26)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q26*$N$135-(K26-N26)-(K26-S26),(Q26-(K26-N26)-(K26-S26))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N26*95%-(K26-Q26)/I$4-(K26-S26)),N26-(K26-Q26)/I$4-(K26-S26)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N26-(K26-Q26)/I$4-(K26-S26))),N26-(K26-Q26)/I$4-(K26-S26))))))))","v":0.43920683020489637},0,0.25490709773803089,0,0,0.25490709773803089,0,0.19669034895470799,5.5151542605637674E-4,2,11,109.39999999999998,101.19999999999999,105.29999999999998,0.23669716593209555]
[2,12,0.20488873537149999,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C27)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C27<$I$3,C27-D27,MIN($I$3,C27-D27))))","v":0},{"$f":"IF(C27<$I$7,MAX(0,C27-D27-E27-F27,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C27-D27-F27)),MIN(I$7,MAX(0,C27-D27-E27-F27))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C27-D27-E27-F27,MIN(I$7,C27-E27-F27)),MIN(I$7,MAX(0,C27-D27-F27))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C27-F27-G27,C27-D27-F27-G27),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C27-G27,IF(OPFOKLEGHEN!$J$18=\"nee\",C27-D27-G27)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C27-G27,C27-D27-F27-G27),C27-D27-F27-G27))","v":0.20488873537149999},0.20488873537149999,0.25964080488929814,0.46600989120195435,{"$f":"SUM(K$16:K27)/$K$137","v":4.8343488016999005E-3},6.383697139752799E-4,0.46600989120195435,{"$f":"IF(E27<I$3,P27*(1-I$6*D27/C27),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P27*(1-$I$6)+(C27-D27)/C27*(K27-P27*(1-I$6)),P27*(1-$I$6)+(C27-D27)/C27*(K27-P27*(1-I$6))))","v":0.46600989120195435},0.46600989120195435,0.46600989120195435,0.46600989120195435,{"$f":"MIN(K27,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K27-(G27/(C27-G27))*(Q27)*95%,K27-(G27/(C27-G27))*(P27)*84%))","v":0.46600989120195435},0.46600989120195435,0.29012244928604392,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H27/C27*K27,IF(OPFOKLEGHEN!$H$20=\"ja\",O27-(K27-Q27)-(K27-S27),Q27-(K27-O27)-(K27-S27)))","v":0.46600989120195435},{"$f":"IF(H27=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q27-(K27-R27)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O27*80%-(K27-S27)),(Q27-(K27-S27)-(K27-T27))),(N27-(K27-S27))))","v":0.9320197824039087},{"$f":"IF(H27=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q27-(K27-R27)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O27*80%-(K27-S27)),(Q27-(K27-S27)-(K27-N27))),(N27-(K27-S27))))","v":0.9320197824039087},{"$f":"IF(H27=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q27-(K27-R27)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O27-(K27-S27)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N27-(K27-Q27)-(K27-S27)),(Q27-(K27-N27/80%)))))),(O27-(K27-S27))))","v":0.9320197824039087},1,null,null,{"$f":"IF(H27=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P27-(K27-R27),K27-(K27-O27)/I$6-(K27-R27)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K27-O27)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O27-(K27-S27),IF(OPFOKLEGHEN!$H$20=\"nee\",(O27-(K27-S27)),(O27-(K27-S27)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O27*80%-(K27-S27),0+O27-(K27-S27)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O27*80%-(K27-S27)),O27*93%-(K27-S27)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O27-(K27-S27))),O27-(K27-S27))))))))","v":0.46600989120195435},{"$f":"IF(H27=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q27-(K27-R27),N27-(K27-R27)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q27-(K27-N27)-(K27-S27),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q27-(K27-N27)-(K27-S27)),(O27-(K27-S27)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q27*$N$135-(K27-N27)-(K27-S27),(Q27-(K27-N27)-(K27-S27))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N27*95%-(K27-Q27)/I$4-(K27-S27)),N27-(K27-Q27)/I$4-(K27-S27)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N27-(K27-Q27)/I$4-(K27-S27))),N27-(K27-Q27)/I$4-(K27-S27))))))))","v":0.46600989120195435},0,0.25964080488929814,0,0,0.25964080488929814,0,0.20488873537149999,6.383697139752799E-4,2,12,117.99999999999997,108.99999999999999,113.49999999999997,0.29012244928604392]
[2,13,0.213058704550532,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C28)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C28<$I$3,C28-D28,MIN($I$3,C28-D28))))","v":0},{"$f":"IF(C28<$I$7,MAX(0,C28-D28-E28-F28,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C28-D28-F28)),MIN(I$7,MAX(0,C28-D28-E28-F28))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C28-D28-E28-F28,MIN(I$7,C28-E28-F28)),MIN(I$7,MAX(0,C28-D28-F28))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C28-F28-G28,C28-D28-F28-G28),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C28-G28,IF(OPFOKLEGHEN!$J$18=\"nee\",C28-D28-G28)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C28-G28,C28-D28-F28-G28),C28-D28-F28-G28))","v":0.213058704550532},0.213058704550532,0.26446241851156127,0.49359113774367519,{"$f":"SUM(K$16:K28)/$K$137","v":5.4123638260924279E-3},7.324982637748604E-4,0.49359113774367519,{"$f":"IF(E28<I$3,P28*(1-I$6*D28/C28),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P28*(1-$I$6)+(C28-D28)/C28*(K28-P28*(1-I$6)),P28*(1-$I$6)+(C28-D28)/C28*(K28-P28*(1-I$6))))","v":0.49359113774367519},0.49359113774367519,0.49359113774367519,0.49359113774367519,{"$f":"MIN(K28,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K28-(G28/(C28-G28))*(Q28)*95%,K28-(G28/(C28-G28))*(P28)*84%))","v":0.49359113774367519},0.49359113774367519,0.35065201594926548,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H28/C28*K28,IF(OPFOKLEGHEN!$H$20=\"ja\",O28-(K28-Q28)-(K28-S28),Q28-(K28-O28)-(K28-S28)))","v":0.49359113774367519},{"$f":"IF(H28=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q28-(K28-R28)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O28*80%-(K28-S28)),(Q28-(K28-S28)-(K28-T28))),(N28-(K28-S28))))","v":0.98718227548735038},{"$f":"IF(H28=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q28-(K28-R28)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O28*80%-(K28-S28)),(Q28-(K28-S28)-(K28-N28))),(N28-(K28-S28))))","v":0.98718227548735038},{"$f":"IF(H28=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q28-(K28-R28)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O28-(K28-S28)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N28-(K28-Q28)-(K28-S28)),(Q28-(K28-N28/80%)))))),(O28-(K28-S28))))","v":0.98718227548735038},1,null,null,{"$f":"IF(H28=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P28-(K28-R28),K28-(K28-O28)/I$6-(K28-R28)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K28-O28)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O28-(K28-S28),IF(OPFOKLEGHEN!$H$20=\"nee\",(O28-(K28-S28)),(O28-(K28-S28)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O28*80%-(K28-S28),0+O28-(K28-S28)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O28*80%-(K28-S28)),O28*93%-(K28-S28)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O28-(K28-S28))),O28-(K28-S28))))))))","v":0.49359113774367519},{"$f":"IF(H28=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q28-(K28-R28),N28-(K28-R28)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q28-(K28-N28)-(K28-S28),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q28-(K28-N28)-(K28-S28)),(O28-(K28-S28)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q28*$N$135-(K28-N28)-(K28-S28),(Q28-(K28-N28)-(K28-S28))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N28*95%-(K28-Q28)/I$4-(K28-S28)),N28-(K28-Q28)/I$4-(K28-S28)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N28-(K28-Q28)/I$4-(K28-S28))),N28-(K28-Q28)/I$4-(K28-S28))))))))","v":0.49359113774367519},0,0.26446241851156127,0,0,0.26446241851156127,0,0.213058704550532,7.324982637748604E-4,2,13,126.59999999999997,116.79999999999998,121.69999999999997,0.35065201594926548]
[2,14,0.22130066726499997,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C29)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C29<$I$3,C29-D29,MIN($I$3,C29-D29))))","v":0},{"$f":"IF(C29<$I$7,MAX(0,C29-D29-E29-F29,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C29-D29-F29)),MIN(I$7,MAX(0,C29-D29-E29-F29))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C29-D29-E29-F29,MIN(I$7,C29-E29-F29)),MIN(I$7,MAX(0,C29-D29-F29))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C29-F29-G29,C29-D29-F29-G29),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C29-G29,IF(OPFOKLEGHEN!$J$18=\"nee\",C29-D29-G29)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C29-G29,C29-D29-F29-G29),C29-D29-F29-G29))","v":0.22130066726499997},0.22130066726499997,0.26937357105638443,0.52220594692060374,{"$f":"SUM(K$16:K29)/$K$137","v":6.023887940011961E-3},8.3457571425667263E-4,0.52220594692060374,{"$f":"IF(E29<I$3,P29*(1-I$6*D29/C29),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P29*(1-$I$6)+(C29-D29)/C29*(K29-P29*(1-I$6)),P29*(1-$I$6)+(C29-D29)/C29*(K29-P29*(1-I$6))))","v":0.52220594692060374},0.52220594692060374,0.52220594692060374,0.52220594692060374,{"$f":"MIN(K29,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K29-(G29/(C29-G29))*(Q29)*95%,K29-(G29/(C29-G29))*(P29)*84%))","v":0.52220594692060374},0.52220594692060374,0.41825826113084996,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H29/C29*K29,IF(OPFOKLEGHEN!$H$20=\"ja\",O29-(K29-Q29)-(K29-S29),Q29-(K29-O29)-(K29-S29)))","v":0.52220594692060374},{"$f":"IF(H29=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q29-(K29-R29)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O29*80%-(K29-S29)),(Q29-(K29-S29)-(K29-T29))),(N29-(K29-S29))))","v":1.0444118938412075},{"$f":"IF(H29=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q29-(K29-R29)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O29*80%-(K29-S29)),(Q29-(K29-S29)-(K29-N29))),(N29-(K29-S29))))","v":1.0444118938412075},{"$f":"IF(H29=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q29-(K29-R29)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O29-(K29-S29)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N29-(K29-Q29)-(K29-S29)),(Q29-(K29-N29/80%)))))),(O29-(K29-S29))))","v":1.0444118938412075},1,null,null,{"$f":"IF(H29=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P29-(K29-R29),K29-(K29-O29)/I$6-(K29-R29)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K29-O29)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O29-(K29-S29),IF(OPFOKLEGHEN!$H$20=\"nee\",(O29-(K29-S29)),(O29-(K29-S29)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O29*80%-(K29-S29),0+O29-(K29-S29)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O29*80%-(K29-S29)),O29*93%-(K29-S29)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O29-(K29-S29))),O29-(K29-S29))))))))","v":0.52220594692060374},{"$f":"IF(H29=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q29-(K29-R29),N29-(K29-R29)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q29-(K29-N29)-(K29-S29),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q29-(K29-N29)-(K29-S29)),(O29-(K29-S29)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q29*$N$135-(K29-N29)-(K29-S29),(Q29-(K29-N29)-(K29-S29))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N29*95%-(K29-Q29)/I$4-(K29-S29)),N29-(K29-Q29)/I$4-(K29-S29)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N29-(K29-Q29)/I$4-(K29-S29))),N29-(K29-Q29)/I$4-(K29-S29))))))))","v":0.52220594692060374},0,0.26937357105638443,0,0,0.26937357105638443,0,0.22130066726499997,8.3457571425667263E-4,2,14,135,125,130,0.41825826113084996]
[3,15,0.23084996955784598,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C30)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C30<$I$3,C30-D30,MIN($I$3,C30-D30))))","v":0},{"$f":"IF(C30<$I$7,MAX(0,C30-D30-E30-F30,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C30-D30-F30)),MIN(I$7,MAX(0,C30-D30-E30-F30))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C30-D30-E30-F30,MIN(I$7,C30-E30-F30)),MIN(I$7,MAX(0,C30-D30-F30))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C30-F30-G30,C30-D30-F30-G30),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C30-G30,IF(OPFOKLEGHEN!$J$18=\"nee\",C30-D30-G30)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C30-G30,C30-D30-F30-G30),C30-D30-F30-G30))","v":0.23084996955784598},0.23084996955784598,0.27437592529048455,0.55485554424625627,{"$f":"SUM(K$16:K30)/$K$137","v":6.6736460422499666E-3},9.5009511001071265E-4,0.55485554424625627,{"$f":"IF(E30<I$3,P30*(1-I$6*D30/C30),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P30*(1-$I$6)+(C30-D30)/C30*(K30-P30*(1-I$6)),P30*(1-$I$6)+(C30-D30)/C30*(K30-P30*(1-I$6))))","v":0.55485554424625627},0.55485554424625627,0.55485554424625627,0.55485554424625627,{"$f":"MIN(K30,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K30-(G30/(C30-G30))*(Q30)*95%,K30-(G30/(C30-G30))*(P30)*84%))","v":0.55485554424625627},0.55485554424625627,0.5020986837883149,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H30/C30*K30,IF(OPFOKLEGHEN!$H$20=\"ja\",O30-(K30-Q30)-(K30-S30),Q30-(K30-O30)-(K30-S30)))","v":0.55485554424625627},{"$f":"IF(H30=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q30-(K30-R30)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O30*80%-(K30-S30)),(Q30-(K30-S30)-(K30-T30))),(N30-(K30-S30))))","v":1.1097110884925125},{"$f":"IF(H30=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q30-(K30-R30)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O30*80%-(K30-S30)),(Q30-(K30-S30)-(K30-N30))),(N30-(K30-S30))))","v":1.1097110884925125},{"$f":"IF(H30=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q30-(K30-R30)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O30-(K30-S30)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N30-(K30-Q30)-(K30-S30)),(Q30-(K30-N30/80%)))))),(O30-(K30-S30))))","v":1.1097110884925125},1,null,null,{"$f":"IF(H30=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P30-(K30-R30),K30-(K30-O30)/I$6-(K30-R30)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K30-O30)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O30-(K30-S30),IF(OPFOKLEGHEN!$H$20=\"nee\",(O30-(K30-S30)),(O30-(K30-S30)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O30*80%-(K30-S30),0+O30-(K30-S30)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O30*80%-(K30-S30)),O30*93%-(K30-S30)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O30-(K30-S30))),O30-(K30-S30))))))))","v":0.55485554424625627},{"$f":"IF(H30=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q30-(K30-R30),N30-(K30-R30)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q30-(K30-N30)-(K30-S30),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q30-(K30-N30)-(K30-S30)),(O30-(K30-S30)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q30*$N$135-(K30-N30)-(K30-S30),(Q30-(K30-N30)-(K30-S30))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N30*95%-(K30-Q30)/I$4-(K30-S30)),N30-(K30-Q30)/I$4-(K30-S30)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N30-(K30-Q30)/I$4-(K30-S30))),N30-(K30-Q30)/I$4-(K30-S30))))))))","v":0.55485554424625627},0,0.27437592529048455,0,0,0.27437592529048455,0,0.23084996955784598,9.5009511001071265E-4,3,15,145,{"$f":"AP29+9.3","v":134.30000000000001},139.65,0.5020986837883149]
[3,16,0.24036552664062802,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C31)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C31<$I$3,C31-D31,MIN($I$3,C31-D31))))","v":0},{"$f":"IF(C31<$I$7,MAX(0,C31-D31-E31-F31,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C31-D31-F31)),MIN(I$7,MAX(0,C31-D31-E31-F31))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C31-D31-E31-F31,MIN(I$7,C31-E31-F31)),MIN(I$7,MAX(0,C31-D31-F31))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C31-F31-G31,C31-D31-F31-G31),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C31-G31,IF(OPFOKLEGHEN!$J$18=\"nee\",C31-D31-G31)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C31-G31,C31-D31-F31-G31),C31-D31-F31-G31))","v":0.24036552664062802},0.24036552664062802,0.27947117485869366,0.58845506846187623,{"$f":"SUM(K$16:K31)/$K$137","v":7.362750535304159E-3},1.0748037780125592E-3,0.58845506846187623,{"$f":"IF(E31<I$3,P31*(1-I$6*D31/C31),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P31*(1-$I$6)+(C31-D31)/C31*(K31-P31*(1-I$6)),P31*(1-$I$6)+(C31-D31)/C31*(K31-P31*(1-I$6))))","v":0.58845506846187623},0.58845506846187623,0.58845506846187623,0.58845506846187623,{"$f":"MIN(K31,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K31-(G31/(C31-G31))*(Q31)*95%,K31-(G31/(C31-G31))*(P31)*84%))","v":0.58845506846187623},0.58845506846187623,0.59610650606875748,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H31/C31*K31,IF(OPFOKLEGHEN!$H$20=\"ja\",O31-(K31-Q31)-(K31-S31),Q31-(K31-O31)-(K31-S31)))","v":0.58845506846187623},{"$f":"IF(H31=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q31-(K31-R31)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O31*80%-(K31-S31)),(Q31-(K31-S31)-(K31-T31))),(N31-(K31-S31))))","v":1.1769101369237525},{"$f":"IF(H31=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q31-(K31-R31)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O31*80%-(K31-S31)),(Q31-(K31-S31)-(K31-N31))),(N31-(K31-S31))))","v":1.1769101369237525},{"$f":"IF(H31=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q31-(K31-R31)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O31-(K31-S31)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N31-(K31-Q31)-(K31-S31)),(Q31-(K31-N31/80%)))))),(O31-(K31-S31))))","v":1.1769101369237525},1,null,null,{"$f":"IF(H31=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P31-(K31-R31),K31-(K31-O31)/I$6-(K31-R31)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K31-O31)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O31-(K31-S31),IF(OPFOKLEGHEN!$H$20=\"nee\",(O31-(K31-S31)),(O31-(K31-S31)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O31*80%-(K31-S31),0+O31-(K31-S31)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O31*80%-(K31-S31)),O31*93%-(K31-S31)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O31-(K31-S31))),O31-(K31-S31))))))))","v":0.58845506846187623},{"$f":"IF(H31=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q31-(K31-R31),N31-(K31-R31)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q31-(K31-N31)-(K31-S31),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q31-(K31-N31)-(K31-S31)),(O31-(K31-S31)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q31*$N$135-(K31-N31)-(K31-S31),(Q31-(K31-N31)-(K31-S31))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N31*95%-(K31-Q31)/I$4-(K31-S31)),N31-(K31-Q31)/I$4-(K31-S31)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N31-(K31-Q31)/I$4-(K31-S31))),N31-(K31-Q31)/I$4-(K31-S31))))))))","v":0.58845506846187623},0,0.27947117485869366,0,0,0.27947117485869366,0,0.24036552664062802,1.0748037780125592E-3,3,16,155,143.60000000000002,149.30000000000001,0.59610650606875748]
[3,17,0.24984940896176203,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C32)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C32<$I$3,C32-D32,MIN($I$3,C32-D32))))","v":0},{"$f":"IF(C32<$I$7,MAX(0,C32-D32-E32-F32,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C32-D32-F32)),MIN(I$7,MAX(0,C32-D32-E32-F32))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C32-D32-E32-F32,MIN(I$7,C32-E32-F32)),MIN(I$7,MAX(0,C32-D32-F32))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C32-F32-G32,C32-D32-F32-G32),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C32-G32,IF(OPFOKLEGHEN!$J$18=\"nee\",C32-D32-G32)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C32-G32,C32-D32-F32-G32),C32-D32-F32-G32))","v":0.24984940896176203},0.24984940896176203,0.28466104485737542,0.62303216979358322,{"$f":"SUM(K$16:K32)/$K$137","v":8.092346201196322E-3},1.2090806948048989E-3,0.62303216979358322,{"$f":"IF(E32<I$3,P32*(1-I$6*D32/C32),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P32*(1-$I$6)+(C32-D32)/C32*(K32-P32*(1-I$6)),P32*(1-$I$6)+(C32-D32)/C32*(K32-P32*(1-I$6))))","v":0.62303216979358322},0.62303216979358322,0.62303216979358322,0.62303216979358322,{"$f":"MIN(K32,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K32-(G32/(C32-G32))*(Q32)*95%,K32-(G32/(C32-G32))*(P32)*84%))","v":0.62303216979358322},0.62303216979358322,0.70082759213774248,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H32/C32*K32,IF(OPFOKLEGHEN!$H$20=\"ja\",O32-(K32-Q32)-(K32-S32),Q32-(K32-O32)-(K32-S32)))","v":0.62303216979358322},{"$f":"IF(H32=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q32-(K32-R32)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O32*80%-(K32-S32)),(Q32-(K32-S32)-(K32-T32))),(N32-(K32-S32))))","v":1.2460643395871664},{"$f":"IF(H32=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q32-(K32-R32)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O32*80%-(K32-S32)),(Q32-(K32-S32)-(K32-N32))),(N32-(K32-S32))))","v":1.2460643395871664},{"$f":"IF(H32=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q32-(K32-R32)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O32-(K32-S32)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N32-(K32-Q32)-(K32-S32)),(Q32-(K32-N32/80%)))))),(O32-(K32-S32))))","v":1.2460643395871664},1,null,null,{"$f":"IF(H32=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P32-(K32-R32),K32-(K32-O32)/I$6-(K32-R32)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K32-O32)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O32-(K32-S32),IF(OPFOKLEGHEN!$H$20=\"nee\",(O32-(K32-S32)),(O32-(K32-S32)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O32*80%-(K32-S32),0+O32-(K32-S32)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O32*80%-(K32-S32)),O32*93%-(K32-S32)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O32-(K32-S32))),O32-(K32-S32))))))))","v":0.62303216979358322},{"$f":"IF(H32=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q32-(K32-R32),N32-(K32-R32)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q32-(K32-N32)-(K32-S32),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q32-(K32-N32)-(K32-S32)),(O32-(K32-S32)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q32*$N$135-(K32-N32)-(K32-S32),(Q32-(K32-N32)-(K32-S32))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N32*95%-(K32-Q32)/I$4-(K32-S32)),N32-(K32-Q32)/I$4-(K32-S32)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N32-(K32-Q32)/I$4-(K32-S32))),N32-(K32-Q32)/I$4-(K32-S32))))))))","v":0.62303216979358322},0,0.28466104485737542,0,0,0.28466104485737542,0,0.24984940896176203,1.2090806948048989E-3,3,17,165,152.90000000000003,158.95000000000002,0.70082759213774248]
[3,18,0.25930368696966399,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C33)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C33<$I$3,C33-D33,MIN($I$3,C33-D33))))","v":0},{"$f":"IF(C33<$I$7,MAX(0,C33-D33-E33-F33,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C33-D33-F33)),MIN(I$7,MAX(0,C33-D33-E33-F33))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C33-D33-E33-F33,MIN(I$7,C33-E33-F33)),MIN(I$7,MAX(0,C33-D33-F33))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C33-F33-G33,C33-D33-F33-G33),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C33-G33,IF(OPFOKLEGHEN!$J$18=\"nee\",C33-D33-G33)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C33-G33,C33-D33-F33-G33),C33-D33-F33-G33))","v":0.25930368696966399},0.25930368696966399,0.28994729241849049,0.65861536109063634,{"$f":"SUM(K$16:K33)/$K$137","v":8.8636112116386116E-3},1.353319235117746E-3,0.65861536109063634,{"$f":"IF(E33<I$3,P33*(1-I$6*D33/C33),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P33*(1-$I$6)+(C33-D33)/C33*(K33-P33*(1-I$6)),P33*(1-$I$6)+(C33-D33)/C33*(K33-P33*(1-I$6))))","v":0.65861536109063634},0.65861536109063634,0.65861536109063634,0.65861536109063634,{"$f":"MIN(K33,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K33-(G33/(C33-G33))*(Q33)*95%,K33-(G33/(C33-G33))*(P33)*84%))","v":0.65861536109063634},0.65861536109063634,0.81680661395444154,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H33/C33*K33,IF(OPFOKLEGHEN!$H$20=\"ja\",O33-(K33-Q33)-(K33-S33),Q33-(K33-O33)-(K33-S33)))","v":0.65861536109063634},{"$f":"IF(H33=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q33-(K33-R33)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O33*80%-(K33-S33)),(Q33-(K33-S33)-(K33-T33))),(N33-(K33-S33))))","v":1.3172307221812727},{"$f":"IF(H33=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q33-(K33-R33)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O33*80%-(K33-S33)),(Q33-(K33-S33)-(K33-N33))),(N33-(K33-S33))))","v":1.3172307221812727},{"$f":"IF(H33=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q33-(K33-R33)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O33-(K33-S33)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N33-(K33-Q33)-(K33-S33)),(Q33-(K33-N33/80%)))))),(O33-(K33-S33))))","v":1.3172307221812727},1,null,null,{"$f":"IF(H33=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P33-(K33-R33),K33-(K33-O33)/I$6-(K33-R33)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K33-O33)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O33-(K33-S33),IF(OPFOKLEGHEN!$H$20=\"nee\",(O33-(K33-S33)),(O33-(K33-S33)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O33*80%-(K33-S33),0+O33-(K33-S33)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O33*80%-(K33-S33)),O33*93%-(K33-S33)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O33-(K33-S33))),O33-(K33-S33))))))))","v":0.65861536109063634},{"$f":"IF(H33=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q33-(K33-R33),N33-(K33-R33)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q33-(K33-N33)-(K33-S33),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q33-(K33-N33)-(K33-S33)),(O33-(K33-S33)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q33*$N$135-(K33-N33)-(K33-S33),(Q33-(K33-N33)-(K33-S33))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N33*95%-(K33-Q33)/I$4-(K33-S33)),N33-(K33-Q33)/I$4-(K33-S33)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N33-(K33-Q33)/I$4-(K33-S33))),N33-(K33-Q33)/I$4-(K33-S33))))))))","v":0.65861536109063634},0,0.28994729241849049,0,0,0.28994729241849049,0,0.25930368696966399,1.353319235117746E-3,3,18,175,162.20000000000005,168.60000000000002,0.81680661395444154]
[3,19,0.26873043111275002,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C34)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C34<$I$3,C34-D34,MIN($I$3,C34-D34))))","v":0},{"$f":"IF(C34<$I$7,MAX(0,C34-D34-E34-F34,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C34-D34-F34)),MIN(I$7,MAX(0,C34-D34-E34-F34))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C34-D34-E34-F34,MIN(I$7,C34-E34-F34)),MIN(I$7,MAX(0,C34-D34-F34))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C34-F34-G34,C34-D34-F34-G34),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C34-G34,IF(OPFOKLEGHEN!$J$18=\"nee\",C34-D34-G34)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C34-G34,C34-D34-F34-G34),C34-D34-F34-G34))","v":0.26873043111275002},0.26873043111275002,0.29533170730450725,0.69523404514079346,{"$f":"SUM(K$16:K34)/$K$137","v":9.6777581701872409E-3},1.5079277234788899E-3,0.69523404514079346,{"$f":"IF(E34<I$3,P34*(1-I$6*D34/C34),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P34*(1-$I$6)+(C34-D34)/C34*(K34-P34*(1-I$6)),P34*(1-$I$6)+(C34-D34)/C34*(K34-P34*(1-I$6))))","v":0.69523404514079346},0.69523404514079346,0.69523404514079346,0.69523404514079346,{"$f":"MIN(K34,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K34-(G34/(C34-G34))*(Q34)*95%,K34-(G34/(C34-G34))*(P34)*84%))","v":0.69523404514079346},0.69523404514079346,0.94458746536131633,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H34/C34*K34,IF(OPFOKLEGHEN!$H$20=\"ja\",O34-(K34-Q34)-(K34-S34),Q34-(K34-O34)-(K34-S34)))","v":0.69523404514079346},{"$f":"IF(H34=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q34-(K34-R34)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O34*80%-(K34-S34)),(Q34-(K34-S34)-(K34-T34))),(N34-(K34-S34))))","v":1.3904680902815869},{"$f":"IF(H34=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q34-(K34-R34)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O34*80%-(K34-S34)),(Q34-(K34-S34)-(K34-N34))),(N34-(K34-S34))))","v":1.3904680902815869},{"$f":"IF(H34=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q34-(K34-R34)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O34-(K34-S34)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N34-(K34-Q34)-(K34-S34)),(Q34-(K34-N34/80%)))))),(O34-(K34-S34))))","v":1.3904680902815869},1,null,null,{"$f":"IF(H34=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P34-(K34-R34),K34-(K34-O34)/I$6-(K34-R34)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K34-O34)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O34-(K34-S34),IF(OPFOKLEGHEN!$H$20=\"nee\",(O34-(K34-S34)),(O34-(K34-S34)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O34*80%-(K34-S34),0+O34-(K34-S34)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O34*80%-(K34-S34)),O34*93%-(K34-S34)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O34-(K34-S34))),O34-(K34-S34))))))))","v":0.69523404514079346},{"$f":"IF(H34=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q34-(K34-R34),N34-(K34-R34)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q34-(K34-N34)-(K34-S34),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q34-(K34-N34)-(K34-S34)),(O34-(K34-S34)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q34*$N$135-(K34-N34)-(K34-S34),(Q34-(K34-N34)-(K34-S34))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N34*95%-(K34-Q34)/I$4-(K34-S34)),N34-(K34-Q34)/I$4-(K34-S34)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N34-(K34-Q34)/I$4-(K34-S34))),N34-(K34-Q34)/I$4-(K34-S34))))))))","v":0.69523404514079346},0,0.29533170730450725,0,0,0.29533170730450725,0,0.26873043111275002,1.5079277234788899E-3,3,19,185,171.50000000000006,178.25000000000003,0.94458746536131633]
[3,20,0.27813171183943602,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C35)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C35<$I$3,C35-D35,MIN($I$3,C35-D35))))","v":0},{"$f":"IF(C35<$I$7,MAX(0,C35-D35-E35-F35,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C35-D35-F35)),MIN(I$7,MAX(0,C35-D35-E35-F35))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C35-D35-E35-F35,MIN(I$7,C35-E35-F35)),MIN(I$7,MAX(0,C35-D35-F35))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C35-F35-G35,C35-D35-F35-G35),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C35-G35,IF(OPFOKLEGHEN!$J$18=\"nee\",C35-D35-G35)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C35-G35,C35-D35-F35-G35),C35-D35-F35-G35))","v":0.27813171183943602},0.27813171183943602,0.30081611251436158,0.73291854282513302,{"$f":"SUM(K$16:K35)/$K$137","v":1.0536035187366595E-2},1.6733300064500755E-3,0.73291854282513302,{"$f":"IF(E35<I$3,P35*(1-I$6*D35/C35),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P35*(1-$I$6)+(C35-D35)/C35*(K35-P35*(1-I$6)),P35*(1-$I$6)+(C35-D35)/C35*(K35-P35*(1-I$6))))","v":0.73291854282513302},0.73291854282513302,0.73291854282513302,0.73291854282513302,{"$f":"MIN(K35,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K35-(G35/(C35-G35))*(Q35)*95%,K35-(G35/(C35-G35))*(P35)*84%))","v":0.73291854282513302},0.73291854282513302,1.0847136761738005,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H35/C35*K35,IF(OPFOKLEGHEN!$H$20=\"ja\",O35-(K35-Q35)-(K35-S35),Q35-(K35-O35)-(K35-S35)))","v":0.73291854282513302},{"$f":"IF(H35=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q35-(K35-R35)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O35*80%-(K35-S35)),(Q35-(K35-S35)-(K35-T35))),(N35-(K35-S35))))","v":1.465837085650266},{"$f":"IF(H35=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q35-(K35-R35)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O35*80%-(K35-S35)),(Q35-(K35-S35)-(K35-N35))),(N35-(K35-S35))))","v":1.465837085650266},{"$f":"IF(H35=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q35-(K35-R35)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O35-(K35-S35)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N35-(K35-Q35)-(K35-S35)),(Q35-(K35-N35/80%)))))),(O35-(K35-S35))))","v":1.465837085650266},1,null,null,{"$f":"IF(H35=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P35-(K35-R35),K35-(K35-O35)/I$6-(K35-R35)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K35-O35)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O35-(K35-S35),IF(OPFOKLEGHEN!$H$20=\"nee\",(O35-(K35-S35)),(O35-(K35-S35)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O35*80%-(K35-S35),0+O35-(K35-S35)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O35*80%-(K35-S35)),O35*93%-(K35-S35)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O35-(K35-S35))),O35-(K35-S35))))))))","v":0.73291854282513302},{"$f":"IF(H35=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q35-(K35-R35),N35-(K35-R35)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q35-(K35-N35)-(K35-S35),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q35-(K35-N35)-(K35-S35)),(O35-(K35-S35)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q35*$N$135-(K35-N35)-(K35-S35),(Q35-(K35-N35)-(K35-S35))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N35*95%-(K35-Q35)/I$4-(K35-S35)),N35-(K35-Q35)/I$4-(K35-S35)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N35-(K35-Q35)/I$4-(K35-S35))),N35-(K35-Q35)/I$4-(K35-S35))))))))","v":0.73291854282513302},0,0.30081611251436158,0,0,0.30081611251436158,0,0.27813171183943602,1.6733300064500755E-3,3,20,195,180.80000000000007,187.90000000000003,1.0847136761738005]
[3,21,0.28746106624750001,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C36)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C36<$I$3,C36-D36,MIN($I$3,C36-D36))))","v":0},{"$f":"IF(C36<$I$7,MAX(0,C36-D36-E36-F36,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C36-D36-F36)),MIN(I$7,MAX(0,C36-D36-E36-F36))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C36-D36-E36-F36,MIN(I$7,C36-E36-F36)),MIN(I$7,MAX(0,C36-D36-F36))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C36-F36-G36,C36-D36-F36-G36),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C36-G36,IF(OPFOKLEGHEN!$J$18=\"nee\",C36-D36-G36)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C36-G36,C36-D36-F36-G36),C36-D36-F36-G36))","v":0.28746106624750001},0.28746106624750001,0.30640236490066852,0.77156985451229132,{"$f":"SUM(K$16:K36)/$K$137","v":1.1439574441161018E-2},1.8496537608171369E-3,0.77156985451229132,{"$f":"IF(E36<I$3,P36*(1-I$6*D36/C36),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P36*(1-$I$6)+(C36-D36)/C36*(K36-P36*(1-I$6)),P36*(1-$I$6)+(C36-D36)/C36*(K36-P36*(1-I$6))))","v":0.77156985451229132},0.77156985451229132,0.77156985451229132,0.77156985451229132,{"$f":"MIN(K36,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K36-(G36/(C36-G36))*(Q36)*95%,K36-(G36/(C36-G36))*(P36)*84%))","v":0.77156985451229132},0.77156985451229132,1.2375198901954876,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H36/C36*K36,IF(OPFOKLEGHEN!$H$20=\"ja\",O36-(K36-Q36)-(K36-S36),Q36-(K36-O36)-(K36-S36)))","v":0.77156985451229132},{"$f":"IF(H36=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q36-(K36-R36)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O36*80%-(K36-S36)),(Q36-(K36-S36)-(K36-T36))),(N36-(K36-S36))))","v":1.5431397090245826},{"$f":"IF(H36=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q36-(K36-R36)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O36*80%-(K36-S36)),(Q36-(K36-S36)-(K36-N36))),(N36-(K36-S36))))","v":1.5431397090245826},{"$f":"IF(H36=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q36-(K36-R36)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O36-(K36-S36)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N36-(K36-Q36)-(K36-S36)),(Q36-(K36-N36/80%)))))),(O36-(K36-S36))))","v":1.5431397090245826},1,null,null,{"$f":"IF(H36=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P36-(K36-R36),K36-(K36-O36)/I$6-(K36-R36)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K36-O36)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O36-(K36-S36),IF(OPFOKLEGHEN!$H$20=\"nee\",(O36-(K36-S36)),(O36-(K36-S36)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O36*80%-(K36-S36),0+O36-(K36-S36)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O36*80%-(K36-S36)),O36*93%-(K36-S36)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O36-(K36-S36))),O36-(K36-S36))))))))","v":0.77156985451229132},{"$f":"IF(H36=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q36-(K36-R36),N36-(K36-R36)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q36-(K36-N36)-(K36-S36),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q36-(K36-N36)-(K36-S36)),(O36-(K36-S36)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q36*$N$135-(K36-N36)-(K36-S36),(Q36-(K36-N36)-(K36-S36))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N36*95%-(K36-Q36)/I$4-(K36-S36)),N36-(K36-Q36)/I$4-(K36-S36)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N36-(K36-Q36)/I$4-(K36-S36))),N36-(K36-Q36)/I$4-(K36-S36))))))))","v":0.77156985451229132},0,0.30640236490066852,0,0,0.30640236490066852,0,0.28746106624750001,1.8496537608171369E-3,3,21,205,190,197.5,1.2375198901954876,"(($Z35/1000)*(1-$F$9)*$D35*$B35)+H35*(1-F$6)*C35/D35"]
[4,22,0.29783462082875195,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C37)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C37<$I$3,C37-D37,MIN($I$3,C37-D37))))","v":0},{"$f":"IF(C37<$I$7,MAX(0,C37-D37-E37-F37,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C37-D37-F37)),MIN(I$7,MAX(0,C37-D37-E37-F37))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C37-D37-E37-F37,MIN(I$7,C37-E37-F37)),MIN(I$7,MAX(0,C37-D37-F37))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C37-F37-G37,C37-D37-F37-G37),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C37-G37,IF(OPFOKLEGHEN!$J$18=\"nee\",C37-D37-G37)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C37-G37,C37-D37-F37-G37),C37-D37-F37-G37))","v":0.29783462082875195},0.29783462082875195,0.31209235579839589,0.8142587180462405,{"$f":"SUM(K$16:K37)/$K$137","v":1.2393104066763288E-2},2.0449419859608778E-3,0.8142587180462405,{"$f":"IF(E37<I$3,P37*(1-I$6*D37/C37),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P37*(1-$I$6)+(C37-D37)/C37*(K37-P37*(1-I$6)),P37*(1-$I$6)+(C37-D37)/C37*(K37-P37*(1-I$6))))","v":0.8142587180462405},0.8142587180462405,0.8142587180462405,0.8142587180462405,{"$f":"MIN(K37,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K37-(G37/(C37-G37))*(Q37)*95%,K37-(G37/(C37-G37))*(P37)*84%))","v":0.8142587180462405},0.8142587180462405,1.4225177160022848,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H37/C37*K37,IF(OPFOKLEGHEN!$H$20=\"ja\",O37-(K37-Q37)-(K37-S37),Q37-(K37-O37)-(K37-S37)))","v":0.8142587180462405},{"$f":"IF(H37=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q37-(K37-R37)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O37*80%-(K37-S37)),(Q37-(K37-S37)-(K37-T37))),(N37-(K37-S37))))","v":1.628517436092481},{"$f":"IF(H37=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q37-(K37-R37)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O37*80%-(K37-S37)),(Q37-(K37-S37)-(K37-N37))),(N37-(K37-S37))))","v":1.628517436092481},{"$f":"IF(H37=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q37-(K37-R37)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O37-(K37-S37)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N37-(K37-Q37)-(K37-S37)),(Q37-(K37-N37/80%)))))),(O37-(K37-S37))))","v":1.628517436092481},1,null,null,{"$f":"IF(H37=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P37-(K37-R37),K37-(K37-O37)/I$6-(K37-R37)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K37-O37)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O37-(K37-S37),IF(OPFOKLEGHEN!$H$20=\"nee\",(O37-(K37-S37)),(O37-(K37-S37)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O37*80%-(K37-S37),0+O37-(K37-S37)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O37*80%-(K37-S37)),O37*93%-(K37-S37)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O37-(K37-S37))),O37-(K37-S37))))))))","v":0.8142587180462405},{"$f":"IF(H37=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q37-(K37-R37),N37-(K37-R37)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q37-(K37-N37)-(K37-S37),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q37-(K37-N37)-(K37-S37)),(O37-(K37-S37)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q37*$N$135-(K37-N37)-(K37-S37),(Q37-(K37-N37)-(K37-S37))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N37*95%-(K37-Q37)/I$4-(K37-S37)),N37-(K37-Q37)/I$4-(K37-S37)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N37-(K37-Q37)/I$4-(K37-S37))),N37-(K37-Q37)/I$4-(K37-S37))))))))","v":0.8142587180462405},0,0.31209235579839589,0,0,0.31209235579839589,0,0.29783462082875195,2.0449419859608778E-3,4,22,{"$f":"AO36+12.1","v":217.1},{"$f":"AP36+9.3","v":199.3},208.2,1.4225177160022848,{"$f":"(($AP36/1000)*(1-$I$10)*$D36*$B36)","v":0}]
[4,23,0.30818476962395602,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C38)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C38<$I$3,C38-D38,MIN($I$3,C38-D38))))","v":0},{"$f":"IF(C38<$I$7,MAX(0,C38-D38-E38-F38,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C38-D38-F38)),MIN(I$7,MAX(0,C38-D38-E38-F38))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C38-D38-E38-F38,MIN(I$7,C38-E38-F38)),MIN(I$7,MAX(0,C38-D38-F38))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C38-F38-G38,C38-D38-F38-G38),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C38-G38,IF(OPFOKLEGHEN!$J$18=\"nee\",C38-D38-G38)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C38-G38,C38-D38-F38-G38),C38-D38-F38-G38))","v":0.30818476962395602},0.30818476962395602,0.31788801166521291,0.85820181429744713,{"$f":"SUM(K$16:K38)/$K$137","v":1.3398092821003144E-2},2.2532696037490048E-3,0.85820181429744713,{"$f":"IF(E38<I$3,P38*(1-I$6*D38/C38),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P38*(1-$I$6)+(C38-D38)/C38*(K38-P38*(1-I$6)),P38*(1-$I$6)+(C38-D38)/C38*(K38-P38*(1-I$6))))","v":0.85820181429744713},0.85820181429744713,0.85820181429744713,0.85820181429744713,{"$f":"MIN(K38,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K38-(G38/(C38-G38))*(Q38)*95%,K38-(G38/(C38-G38))*(P38)*84%))","v":0.85820181429744713},0.85820181429744713,1.6246268315496464,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H38/C38*K38,IF(OPFOKLEGHEN!$H$20=\"ja\",O38-(K38-Q38)-(K38-S38),Q38-(K38-O38)-(K38-S38)))","v":0.85820181429744713},{"$f":"IF(H38=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q38-(K38-R38)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O38*80%-(K38-S38)),(Q38-(K38-S38)-(K38-T38))),(N38-(K38-S38))))","v":1.7164036285948943},{"$f":"IF(H38=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q38-(K38-R38)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O38*80%-(K38-S38)),(Q38-(K38-S38)-(K38-N38))),(N38-(K38-S38))))","v":1.7164036285948943},{"$f":"IF(H38=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q38-(K38-R38)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O38-(K38-S38)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N38-(K38-Q38)-(K38-S38)),(Q38-(K38-N38/80%)))))),(O38-(K38-S38))))","v":1.7164036285948943},1,null,null,{"$f":"IF(H38=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P38-(K38-R38),K38-(K38-O38)/I$6-(K38-R38)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K38-O38)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O38-(K38-S38),IF(OPFOKLEGHEN!$H$20=\"nee\",(O38-(K38-S38)),(O38-(K38-S38)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O38*80%-(K38-S38),0+O38-(K38-S38)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O38*80%-(K38-S38)),O38*93%-(K38-S38)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O38-(K38-S38))),O38-(K38-S38))))))))","v":0.85820181429744713},{"$f":"IF(H38=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q38-(K38-R38),N38-(K38-R38)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q38-(K38-N38)-(K38-S38),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q38-(K38-N38)-(K38-S38)),(O38-(K38-S38)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q38*$N$135-(K38-N38)-(K38-S38),(Q38-(K38-N38)-(K38-S38))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N38*95%-(K38-Q38)/I$4-(K38-S38)),N38-(K38-Q38)/I$4-(K38-S38)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N38-(K38-Q38)/I$4-(K38-S38))),N38-(K38-Q38)/I$4-(K38-S38))))))))","v":0.85820181429744713},0,0.31788801166521291,0,0,0.31788801166521291,0,0.30818476962395602,2.2532696037490048E-3,4,23,229.2,208.60000000000002,218.9,1.6246268315496464,{"$f":"(($AQ36/1000)*(1-$I$10)*$E36*$B36)","v":0}]
[4,24,0.31851433513218397,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C39)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C39<$I$3,C39-D39,MIN($I$3,C39-D39))))","v":0},{"$f":"IF(C39<$I$7,MAX(0,C39-D39-E39-F39,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C39-D39-F39)),MIN(I$7,MAX(0,C39-D39-E39-F39))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C39-D39-E39-F39,MIN(I$7,C39-E39-F39)),MIN(I$7,MAX(0,C39-D39-F39))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C39-F39-G39,C39-D39-F39-G39),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C39-G39,IF(OPFOKLEGHEN!$J$18=\"nee\",C39-D39-G39)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C39-G39,C39-D39-F39-G39),C39-D39-F39-G39))","v":0.31851433513218397},0.31851433513218397,0.32379129473372997,0.90343780012203834,{"$f":"SUM(K$16:K39)/$K$137","v":1.4456054729439703E-2},2.4751720551288727E-3,0.90343780012203834,{"$f":"IF(E39<I$3,P39*(1-I$6*D39/C39),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P39*(1-$I$6)+(C39-D39)/C39*(K39-P39*(1-I$6)),P39*(1-$I$6)+(C39-D39)/C39*(K39-P39*(1-I$6))))","v":0.90343780012203834},0.90343780012203834,0.90343780012203834,0.90343780012203834,{"$f":"MIN(K39,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K39-(G39/(C39-G39))*(Q39)*95%,K39-(G39/(C39-G39))*(P39)*84%))","v":0.90343780012203834},0.90343780012203834,1.8445802176175037,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H39/C39*K39,IF(OPFOKLEGHEN!$H$20=\"ja\",O39-(K39-Q39)-(K39-S39),Q39-(K39-O39)-(K39-S39)))","v":0.90343780012203834},{"$f":"IF(H39=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q39-(K39-R39)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O39*80%-(K39-S39)),(Q39-(K39-S39)-(K39-T39))),(N39-(K39-S39))))","v":1.8068756002440767},{"$f":"IF(H39=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q39-(K39-R39)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O39*80%-(K39-S39)),(Q39-(K39-S39)-(K39-N39))),(N39-(K39-S39))))","v":1.8068756002440767},{"$f":"IF(H39=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q39-(K39-R39)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O39-(K39-S39)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N39-(K39-Q39)-(K39-S39)),(Q39-(K39-N39/80%)))))),(O39-(K39-S39))))","v":1.8068756002440767},1,null,null,{"$f":"IF(H39=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P39-(K39-R39),K39-(K39-O39)/I$6-(K39-R39)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K39-O39)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O39-(K39-S39),IF(OPFOKLEGHEN!$H$20=\"nee\",(O39-(K39-S39)),(O39-(K39-S39)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O39*80%-(K39-S39),0+O39-(K39-S39)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O39*80%-(K39-S39)),O39*93%-(K39-S39)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O39-(K39-S39))),O39-(K39-S39))))))))","v":0.90343780012203834},{"$f":"IF(H39=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q39-(K39-R39),N39-(K39-R39)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q39-(K39-N39)-(K39-S39),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q39-(K39-N39)-(K39-S39)),(O39-(K39-S39)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q39*$N$135-(K39-N39)-(K39-S39),(Q39-(K39-N39)-(K39-S39))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N39*95%-(K39-Q39)/I$4-(K39-S39)),N39-(K39-Q39)/I$4-(K39-S39)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N39-(K39-Q39)/I$4-(K39-S39))),N39-(K39-Q39)/I$4-(K39-S39))))))))","v":0.90343780012203834},0,0.32379129473372997,0,0,0.32379129473372997,0,0.31851433513218397,2.4751720551288727E-3,4,24,241.29999999999998,217.90000000000003,229.60000000000002,1.8445802176175037,"(($Y35/1000)*(1-$F$9)*$F35*$B35)"]
[4,25,0.32882613985250797,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C40)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C40<$I$3,C40-D40,MIN($I$3,C40-D40))))","v":0},{"$f":"IF(C40<$I$7,MAX(0,C40-D40-E40-F40,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C40-D40-F40)),MIN(I$7,MAX(0,C40-D40-E40-F40))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C40-D40-E40-F40,MIN(I$7,C40-E40-F40)),MIN(I$7,MAX(0,C40-D40-F40))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C40-F40-G40,C40-D40-F40-G40),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C40-G40,IF(OPFOKLEGHEN!$J$18=\"nee\",C40-D40-G40)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C40-G40,C40-D40-F40-G40),C40-D40-F40-G40))","v":0.32882613985250797},0.32882613985250797,0.32980420367585112,0.95000661044829737,{"$f":"SUM(K$16:K40)/$K$137","v":1.5568550583035225E-2},2.7112060800465109E-3,0.95000661044829737,{"$f":"IF(E40<I$3,P40*(1-I$6*D40/C40),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P40*(1-$I$6)+(C40-D40)/C40*(K40-P40*(1-I$6)),P40*(1-$I$6)+(C40-D40)/C40*(K40-P40*(1-I$6))))","v":0.95000661044829737},0.95000661044829737,0.95000661044829737,0.95000661044829737,{"$f":"MIN(K40,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K40-(G40/(C40-G40))*(Q40)*95%,K40-(G40/(C40-G40))*(P40)*84%))","v":0.95000661044829737},0.95000661044829737,2.0831135959656377,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H40/C40*K40,IF(OPFOKLEGHEN!$H$20=\"ja\",O40-(K40-Q40)-(K40-S40),Q40-(K40-O40)-(K40-S40)))","v":0.95000661044829737},{"$f":"IF(H40=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q40-(K40-R40)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O40*80%-(K40-S40)),(Q40-(K40-S40)-(K40-T40))),(N40-(K40-S40))))","v":1.9000132208965947},{"$f":"IF(H40=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q40-(K40-R40)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O40*80%-(K40-S40)),(Q40-(K40-S40)-(K40-N40))),(N40-(K40-S40))))","v":1.9000132208965947},{"$f":"IF(H40=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q40-(K40-R40)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O40-(K40-S40)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N40-(K40-Q40)-(K40-S40)),(Q40-(K40-N40/80%)))))),(O40-(K40-S40))))","v":1.9000132208965947},1,null,null,{"$f":"IF(H40=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P40-(K40-R40),K40-(K40-O40)/I$6-(K40-R40)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K40-O40)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O40-(K40-S40),IF(OPFOKLEGHEN!$H$20=\"nee\",(O40-(K40-S40)),(O40-(K40-S40)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O40*80%-(K40-S40),0+O40-(K40-S40)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O40*80%-(K40-S40)),O40*93%-(K40-S40)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O40-(K40-S40))),O40-(K40-S40))))))))","v":0.95000661044829737},{"$f":"IF(H40=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q40-(K40-R40),N40-(K40-R40)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q40-(K40-N40)-(K40-S40),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q40-(K40-N40)-(K40-S40)),(O40-(K40-S40)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q40*$N$135-(K40-N40)-(K40-S40),(Q40-(K40-N40)-(K40-S40))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N40*95%-(K40-Q40)/I$4-(K40-S40)),N40-(K40-Q40)/I$4-(K40-S40)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N40-(K40-Q40)/I$4-(K40-S40))),N40-(K40-Q40)/I$4-(K40-S40))))))))","v":0.95000661044829737},0,0.32980420367585112,0,0,0.32980420367585112,0,0.32882613985250797,2.7112060800465109E-3,4,25,253.39999999999998,227.20000000000005,240.3,2.0831135959656377]
[4,26,0.33912300628400005,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C41)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C41<$I$3,C41-D41,MIN($I$3,C41-D41))))","v":0},{"$f":"IF(C41<$I$7,MAX(0,C41-D41-E41-F41,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C41-D41-F41)),MIN(I$7,MAX(0,C41-D41-E41-F41))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C41-D41-E41-F41,MIN(I$7,C41-E41-F41)),MIN(I$7,MAX(0,C41-D41-F41))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C41-F41-G41,C41-D41-F41-G41),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C41-G41,IF(OPFOKLEGHEN!$J$18=\"nee\",C41-D41-G41)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C41-G41,C41-D41-F41-G41),C41-D41-F41-G41))","v":0.33912300628400005},0.33912300628400005,0.33592877427946305,0.99794950027912899,{"$f":"SUM(K$16:K41)/$K$137","v":1.6737189484015456E-2},2.9619505716047207E-3,0.99794950027912899,{"$f":"IF(E41<I$3,P41*(1-I$6*D41/C41),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P41*(1-$I$6)+(C41-D41)/C41*(K41-P41*(1-I$6)),P41*(1-$I$6)+(C41-D41)/C41*(K41-P41*(1-I$6))))","v":0.99794950027912899},0.99794950027912899,0.99794950027912899,0.99794950027912899,{"$f":"MIN(K41,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K41-(G41/(C41-G41))*(Q41)*95%,K41-(G41/(C41-G41))*(P41)*84%))","v":0.99794950027912899},0.99794950027912899,2.3409661123784526,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H41/C41*K41,IF(OPFOKLEGHEN!$H$20=\"ja\",O41-(K41-Q41)-(K41-S41),Q41-(K41-O41)-(K41-S41)))","v":0.99794950027912899},{"$f":"IF(H41=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q41-(K41-R41)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O41*80%-(K41-S41)),(Q41-(K41-S41)-(K41-T41))),(N41-(K41-S41))))","v":1.995899000558258},{"$f":"IF(H41=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q41-(K41-R41)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O41*80%-(K41-S41)),(Q41-(K41-S41)-(K41-N41))),(N41-(K41-S41))))","v":1.995899000558258},{"$f":"IF(H41=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q41-(K41-R41)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O41-(K41-S41)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N41-(K41-Q41)-(K41-S41)),(Q41-(K41-N41/80%)))))),(O41-(K41-S41))))","v":1.995899000558258},1,null,null,{"$f":"IF(H41=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P41-(K41-R41),K41-(K41-O41)/I$6-(K41-R41)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K41-O41)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O41-(K41-S41),IF(OPFOKLEGHEN!$H$20=\"nee\",(O41-(K41-S41)),(O41-(K41-S41)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O41*80%-(K41-S41),0+O41-(K41-S41)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O41*80%-(K41-S41)),O41*93%-(K41-S41)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O41-(K41-S41))),O41-(K41-S41))))))))","v":0.99794950027912899},{"$f":"IF(H41=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q41-(K41-R41),N41-(K41-R41)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q41-(K41-N41)-(K41-S41),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q41-(K41-N41)-(K41-S41)),(O41-(K41-S41)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q41*$N$135-(K41-N41)-(K41-S41),(Q41-(K41-N41)-(K41-S41))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N41*95%-(K41-Q41)/I$4-(K41-S41)),N41-(K41-Q41)/I$4-(K41-S41)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N41-(K41-Q41)/I$4-(K41-S41))),N41-(K41-Q41)/I$4-(K41-S41))))))))","v":0.99794950027912899},0,0.33592877427946305,0,0,0.33592877427946305,0,0.33912300628400005,2.9619505716047207E-3,4,26,265.5,236.50000000000006,251.00000000000003,2.3409661123784526]
[4,27,0.349407756925732,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C42)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C42<$I$3,C42-D42,MIN($I$3,C42-D42))))","v":0},{"$f":"IF(C42<$I$7,MAX(0,C42-D42-E42-F42,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C42-D42-F42)),MIN(I$7,MAX(0,C42-D42-E42-F42))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C42-D42-E42-F42,MIN(I$7,C42-E42-F42)),MIN(I$7,MAX(0,C42-D42-F42))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C42-F42-G42,C42-D42-F42-G42),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C42-G42,IF(OPFOKLEGHEN!$J$18=\"nee\",C42-D42-G42)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C42-G42,C42-D42-F42-G42),C42-D42-F42-G42))","v":0.349407756925732},0.349407756925732,0.34216708013769137,1.0473090880111044,{"$f":"SUM(K$16:K42)/$K$137","v":1.7963630442458314E-2},3.2280074630479244E-3,1.0473090880111044,{"$f":"IF(E42<I$3,P42*(1-I$6*D42/C42),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P42*(1-$I$6)+(C42-D42)/C42*(K42-P42*(1-I$6)),P42*(1-$I$6)+(C42-D42)/C42*(K42-P42*(1-I$6))))","v":1.0473090880111044},1.0473090880111044,1.0473090880111044,1.0473090880111044,{"$f":"MIN(K42,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K42-(G42/(C42-G42))*(Q42)*95%,K42-(G42/(C42-G42))*(P42)*84%))","v":1.0473090880111044},1.0473090880111044,2.6188810197097467,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H42/C42*K42,IF(OPFOKLEGHEN!$H$20=\"ja\",O42-(K42-Q42)-(K42-S42),Q42-(K42-O42)-(K42-S42)))","v":1.0473090880111044},{"$f":"IF(H42=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q42-(K42-R42)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O42*80%-(K42-S42)),(Q42-(K42-S42)-(K42-T42))),(N42-(K42-S42))))","v":2.0946181760222089},{"$f":"IF(H42=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q42-(K42-R42)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O42*80%-(K42-S42)),(Q42-(K42-S42)-(K42-N42))),(N42-(K42-S42))))","v":2.0946181760222089},{"$f":"IF(H42=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q42-(K42-R42)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O42-(K42-S42)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N42-(K42-Q42)-(K42-S42)),(Q42-(K42-N42/80%)))))),(O42-(K42-S42))))","v":2.0946181760222089},1,null,null,{"$f":"IF(H42=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P42-(K42-R42),K42-(K42-O42)/I$6-(K42-R42)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K42-O42)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O42-(K42-S42),IF(OPFOKLEGHEN!$H$20=\"nee\",(O42-(K42-S42)),(O42-(K42-S42)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O42*80%-(K42-S42),0+O42-(K42-S42)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O42*80%-(K42-S42)),O42*93%-(K42-S42)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O42-(K42-S42))),O42-(K42-S42))))))))","v":1.0473090880111044},{"$f":"IF(H42=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q42-(K42-R42),N42-(K42-R42)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q42-(K42-N42)-(K42-S42),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q42-(K42-N42)-(K42-S42)),(O42-(K42-S42)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q42*$N$135-(K42-N42)-(K42-S42),(Q42-(K42-N42)-(K42-S42))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N42*95%-(K42-Q42)/I$4-(K42-S42)),N42-(K42-Q42)/I$4-(K42-S42)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N42-(K42-Q42)/I$4-(K42-S42))),N42-(K42-Q42)/I$4-(K42-S42))))))))","v":1.0473090880111044},0,0.34216708013769137,0,0,0.34216708013769137,0,0.349407756925732,3.2280074630479244E-3,4,27,277.60000000000002,245.80000000000007,261.70000000000005,2.6188810197097467]
[4,28,0.35977921167249993,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C43)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C43<$I$3,C43-D43,MIN($I$3,C43-D43))))","v":0},{"$f":"IF(C43<$I$7,MAX(0,C43-D43-E43-F43,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C43-D43-F43)),MIN(I$7,MAX(0,C43-D43-E43-F43))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C43-D43-E43-F43,MIN(I$7,C43-E43-F43)),MIN(I$7,MAX(0,C43-D43-F43))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C43-F43-G43,C43-D43-F43-G43),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C43-G43,IF(OPFOKLEGHEN!$J$18=\"nee\",C43-D43-G43)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C43-G43,C43-D43-F43-G43),C43-D43-F43-G43))","v":0.35977921167249993},0.35977921167249993,0.34852123335095586,1.0984224845745363,{"$f":"SUM(K$16:K43)/$K$137","v":1.9249927238865466E-2},3.5109394484117602E-3,1.0984224845745363,{"$f":"IF(E43<I$3,P43*(1-I$6*D43/C43),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P43*(1-$I$6)+(C43-D43)/C43*(K43-P43*(1-I$6)),P43*(1-$I$6)+(C43-D43)/C43*(K43-P43*(1-I$6))))","v":1.0984224845745363},1.0984224845745363,1.0984224845745363,1.0984224845745363,{"$f":"MIN(K43,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K43-(G43/(C43-G43))*(Q43)*95%,K43-(G43/(C43-G43))*(P43)*84%))","v":1.0984224845745363},1.0984224845745363,2.9214071987806993,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H43/C43*K43,IF(OPFOKLEGHEN!$H$20=\"ja\",O43-(K43-Q43)-(K43-S43),Q43-(K43-O43)-(K43-S43)))","v":1.0984224845745363},{"$f":"IF(H43=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q43-(K43-R43)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O43*80%-(K43-S43)),(Q43-(K43-S43)-(K43-T43))),(N43-(K43-S43))))","v":2.1968449691490726},{"$f":"IF(H43=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q43-(K43-R43)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O43*80%-(K43-S43)),(Q43-(K43-S43)-(K43-N43))),(N43-(K43-S43))))","v":2.1968449691490726},{"$f":"IF(H43=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q43-(K43-R43)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O43-(K43-S43)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N43-(K43-Q43)-(K43-S43)),(Q43-(K43-N43/80%)))))),(O43-(K43-S43))))","v":2.1968449691490726},1,null,null,{"$f":"IF(H43=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P43-(K43-R43),K43-(K43-O43)/I$6-(K43-R43)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K43-O43)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O43-(K43-S43),IF(OPFOKLEGHEN!$H$20=\"nee\",(O43-(K43-S43)),(O43-(K43-S43)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O43*80%-(K43-S43),0+O43-(K43-S43)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O43*80%-(K43-S43)),O43*93%-(K43-S43)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O43-(K43-S43))),O43-(K43-S43))))))))","v":1.0984224845745363},{"$f":"IF(H43=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q43-(K43-R43),N43-(K43-R43)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q43-(K43-N43)-(K43-S43),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q43-(K43-N43)-(K43-S43)),(O43-(K43-S43)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q43*$N$135-(K43-N43)-(K43-S43),(Q43-(K43-N43)-(K43-S43))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N43*95%-(K43-Q43)/I$4-(K43-S43)),N43-(K43-Q43)/I$4-(K43-S43)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N43-(K43-Q43)/I$4-(K43-S43))),N43-(K43-Q43)/I$4-(K43-S43))))))))","v":1.0984224845745363},0,0.34852123335095586,0,0,0.34852123335095586,0,0.35977921167249993,3.5109394484117602E-3,4,28,290,255,272.5,2.9214071987806993]
[5,29,0.37067181997969395,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C44)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C44<$I$3,C44-D44,MIN($I$3,C44-D44))))","v":0},{"$f":"IF(C44<$I$7,MAX(0,C44-D44-E44-F44,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C44-D44-F44)),MIN(I$7,MAX(0,C44-D44-E44-F44))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C44-D44-E44-F44,MIN(I$7,C44-E44-F44)),MIN(I$7,MAX(0,C44-D44-F44))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C44-F44-G44,C44-D44-F44-G44),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C44-G44,IF(OPFOKLEGHEN!$J$18=\"nee\",C44-D44-G44)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C44-G44,C44-D44-F44-G44),C44-D44-F44-G44))","v":0.37067181997969395},0.37067181997969395,0.35499338524206325,1.1526937470906311,{"$f":"SUM(K$16:K44)/$K$137","v":2.059977786095606E-2},3.8159952814644186E-3,1.1526937470906311,{"$f":"IF(E44<I$3,P44*(1-I$6*D44/C44),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P44*(1-$I$6)+(C44-D44)/C44*(K44-P44*(1-I$6)),P44*(1-$I$6)+(C44-D44)/C44*(K44-P44*(1-I$6))))","v":1.1526937470906311},1.1526937470906311,1.1526937470906311,1.1526937470906311,{"$f":"MIN(K44,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K44-(G44/(C44-G44))*(Q44)*95%,K44-(G44/(C44-G44))*(P44)*84%))","v":1.1526937470906311},1.1526937470906311,3.2463437993821596,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H44/C44*K44,IF(OPFOKLEGHEN!$H$20=\"ja\",O44-(K44-Q44)-(K44-S44),Q44-(K44-O44)-(K44-S44)))","v":1.1526937470906311},{"$f":"IF(H44=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q44-(K44-R44)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O44*80%-(K44-S44)),(Q44-(K44-S44)-(K44-T44))),(N44-(K44-S44))))","v":2.3053874941812622},{"$f":"IF(H44=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q44-(K44-R44)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O44*80%-(K44-S44)),(Q44-(K44-S44)-(K44-N44))),(N44-(K44-S44))))","v":2.3053874941812622},{"$f":"IF(H44=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q44-(K44-R44)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O44-(K44-S44)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N44-(K44-Q44)-(K44-S44)),(Q44-(K44-N44/80%)))))),(O44-(K44-S44))))","v":2.3053874941812622},1,null,null,{"$f":"IF(H44=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P44-(K44-R44),K44-(K44-O44)/I$6-(K44-R44)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K44-O44)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O44-(K44-S44),IF(OPFOKLEGHEN!$H$20=\"nee\",(O44-(K44-S44)),(O44-(K44-S44)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O44*80%-(K44-S44),0+O44-(K44-S44)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O44*80%-(K44-S44)),O44*93%-(K44-S44)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O44-(K44-S44))),O44-(K44-S44))))))))","v":1.1526937470906311},{"$f":"IF(H44=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q44-(K44-R44),N44-(K44-R44)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q44-(K44-N44)-(K44-S44),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q44-(K44-N44)-(K44-S44)),(O44-(K44-S44)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q44*$N$135-(K44-N44)-(K44-S44),(Q44-(K44-N44)-(K44-S44))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N44*95%-(K44-Q44)/I$4-(K44-S44)),N44-(K44-Q44)/I$4-(K44-S44)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N44-(K44-Q44)/I$4-(K44-S44))),N44-(K44-Q44)/I$4-(K44-S44))))))))","v":1.1526937470906311},0,0.35499338524206325,0,0,0.35499338524206325,0,0.37067181997969395,3.8159952814644186E-3,5,29,{"$f":"AO43+12","v":302},{"$f":"AP43+10.7","v":265.7},283.85000000000002,3.2463437993821596]
[5,30,0.38156054588591193,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C45)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C45<$I$3,C45-D45,MIN($I$3,C45-D45))))","v":0},{"$f":"IF(C45<$I$7,MAX(0,C45-D45-E45-F45,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C45-D45-F45)),MIN(I$7,MAX(0,C45-D45-E45-F45))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C45-D45-E45-F45,MIN(I$7,C45-E45-F45)),MIN(I$7,MAX(0,C45-D45-F45))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C45-F45-G45,C45-D45-F45-G45),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C45-G45,IF(OPFOKLEGHEN!$J$18=\"nee\",C45-D45-G45)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C45-G45,C45-D45-F45-G45),C45-D45-F45-G45))","v":0.38156054588591193},0.38156054588591193,0.36158572708458003,1.2085895833198932,{"$f":"SUM(K$16:K45)/$K$137","v":2.2015084749723537E-2},4.1390054223284017E-3,1.2085895833198932,{"$f":"IF(E45<I$3,P45*(1-I$6*D45/C45),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P45*(1-$I$6)+(C45-D45)/C45*(K45-P45*(1-I$6)),P45*(1-$I$6)+(C45-D45)/C45*(K45-P45*(1-I$6))))","v":1.2085895833198932},1.2085895833198932,1.2085895833198932,1.2085895833198932,{"$f":"MIN(K45,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K45-(G45/(C45-G45))*(Q45)*95%,K45-(G45/(C45-G45))*(P45)*84%))","v":1.2085895833198932},1.2085895833198932,3.5943003422452904,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H45/C45*K45,IF(OPFOKLEGHEN!$H$20=\"ja\",O45-(K45-Q45)-(K45-S45),Q45-(K45-O45)-(K45-S45)))","v":1.2085895833198932},{"$f":"IF(H45=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q45-(K45-R45)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O45*80%-(K45-S45)),(Q45-(K45-S45)-(K45-T45))),(N45-(K45-S45))))","v":2.4171791666397864},{"$f":"IF(H45=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q45-(K45-R45)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O45*80%-(K45-S45)),(Q45-(K45-S45)-(K45-N45))),(N45-(K45-S45))))","v":2.4171791666397864},{"$f":"IF(H45=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q45-(K45-R45)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O45-(K45-S45)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N45-(K45-Q45)-(K45-S45)),(Q45-(K45-N45/80%)))))),(O45-(K45-S45))))","v":2.4171791666397864},1,null,null,{"$f":"IF(H45=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P45-(K45-R45),K45-(K45-O45)/I$6-(K45-R45)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K45-O45)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O45-(K45-S45),IF(OPFOKLEGHEN!$H$20=\"nee\",(O45-(K45-S45)),(O45-(K45-S45)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O45*80%-(K45-S45),0+O45-(K45-S45)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O45*80%-(K45-S45)),O45*93%-(K45-S45)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O45-(K45-S45))),O45-(K45-S45))))))))","v":1.2085895833198932},{"$f":"IF(H45=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q45-(K45-R45),N45-(K45-R45)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q45-(K45-N45)-(K45-S45),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q45-(K45-N45)-(K45-S45)),(O45-(K45-S45)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q45*$N$135-(K45-N45)-(K45-S45),(Q45-(K45-N45)-(K45-S45))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N45*95%-(K45-Q45)/I$4-(K45-S45)),N45-(K45-Q45)/I$4-(K45-S45)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N45-(K45-Q45)/I$4-(K45-S45))),N45-(K45-Q45)/I$4-(K45-S45))))))))","v":1.2085895833198932},0,0.36158572708458003,0,0,0.36158572708458003,0,0.38156054588591193,4.1390054223284017E-3,5,30,314,276.39999999999998,295.2,3.5943003422452904]
[5,31,0.3924487581510579,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C46)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C46<$I$3,C46-D46,MIN($I$3,C46-D46))))","v":0},{"$f":"IF(C46<$I$7,MAX(0,C46-D46-E46-F46,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C46-D46-F46)),MIN(I$7,MAX(0,C46-D46-E46-F46))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C46-D46-E46-F46,MIN(I$7,C46-E46-F46)),MIN(I$7,MAX(0,C46-D46-F46))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C46-F46-G46,C46-D46-F46-G46),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C46-G46,IF(OPFOKLEGHEN!$J$18=\"nee\",C46-D46-G46)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C46-G46,C46-D46-F46-G46),C46-D46-F46-G46))","v":0.3924487581510579},0.3924487581510579,0.36830049084473043,1.2661622554639302,{"$f":"SUM(K$16:K46)/$K$137","v":2.3497811547296108E-2},4.4807111780116255E-3,1.2661622554639302,{"$f":"IF(E46<I$3,P46*(1-I$6*D46/C46),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P46*(1-$I$6)+(C46-D46)/C46*(K46-P46*(1-I$6)),P46*(1-$I$6)+(C46-D46)/C46*(K46-P46*(1-I$6))))","v":1.2661622554639302},1.2661622554639302,1.2661622554639302,1.2661622554639302,{"$f":"MIN(K46,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K46-(G46/(C46-G46))*(Q46)*95%,K46-(G46/(C46-G46))*(P46)*84%))","v":1.2661622554639302},1.2661622554639302,3.9660871498745918,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H46/C46*K46,IF(OPFOKLEGHEN!$H$20=\"ja\",O46-(K46-Q46)-(K46-S46),Q46-(K46-O46)-(K46-S46)))","v":1.2661622554639302},{"$f":"IF(H46=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q46-(K46-R46)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O46*80%-(K46-S46)),(Q46-(K46-S46)-(K46-T46))),(N46-(K46-S46))))","v":2.5323245109278605},{"$f":"IF(H46=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q46-(K46-R46)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O46*80%-(K46-S46)),(Q46-(K46-S46)-(K46-N46))),(N46-(K46-S46))))","v":2.5323245109278605},{"$f":"IF(H46=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q46-(K46-R46)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O46-(K46-S46)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N46-(K46-Q46)-(K46-S46)),(Q46-(K46-N46/80%)))))),(O46-(K46-S46))))","v":2.5323245109278605},1,null,null,{"$f":"IF(H46=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P46-(K46-R46),K46-(K46-O46)/I$6-(K46-R46)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K46-O46)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O46-(K46-S46),IF(OPFOKLEGHEN!$H$20=\"nee\",(O46-(K46-S46)),(O46-(K46-S46)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O46*80%-(K46-S46),0+O46-(K46-S46)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O46*80%-(K46-S46)),O46*93%-(K46-S46)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O46-(K46-S46))),O46-(K46-S46))))))))","v":1.2661622554639302},{"$f":"IF(H46=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q46-(K46-R46),N46-(K46-R46)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q46-(K46-N46)-(K46-S46),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q46-(K46-N46)-(K46-S46)),(O46-(K46-S46)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q46*$N$135-(K46-N46)-(K46-S46),(Q46-(K46-N46)-(K46-S46))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N46*95%-(K46-Q46)/I$4-(K46-S46)),N46-(K46-Q46)/I$4-(K46-S46)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N46-(K46-Q46)/I$4-(K46-S46))),N46-(K46-Q46)/I$4-(K46-S46))))))))","v":1.2661622554639302},0,0.36830049084473043,0,0,0.36830049084473043,0,0.3924487581510579,4.4807111780116255E-3,5,31,326,287.09999999999997,306.54999999999995,3.9660871498745918]
[5,32,0.403339825535036,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C47)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C47<$I$3,C47-D47,MIN($I$3,C47-D47))))","v":0},{"$f":"IF(C47<$I$7,MAX(0,C47-D47-E47-F47,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C47-D47-F47)),MIN(I$7,MAX(0,C47-D47-E47-F47))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C47-D47-E47-F47,MIN(I$7,C47-E47-F47)),MIN(I$7,MAX(0,C47-D47-F47))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C47-F47-G47,C47-D47-F47-G47),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C47-G47,IF(OPFOKLEGHEN!$J$18=\"nee\",C47-D47-G47)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C47-G47,C47-D47-F47-G47),C47-D47-F47-G47))","v":0.403339825535036},0.403339825535036,0.37513994993707267,1.3254658059594475,{"$f":"SUM(K$16:K47)/$K$137","v":2.5049985181663445E-2},4.8418842226829132E-3,1.3254658059594475,{"$f":"IF(E47<I$3,P47*(1-I$6*D47/C47),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P47*(1-$I$6)+(C47-D47)/C47*(K47-P47*(1-I$6)),P47*(1-$I$6)+(C47-D47)/C47*(K47-P47*(1-I$6))))","v":1.3254658059594475},1.3254658059594475,1.3254658059594475,1.3254658059594475,{"$f":"MIN(K47,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K47-(G47/(C47-G47))*(Q47)*95%,K47-(G47/(C47-G47))*(P47)*84%))","v":1.3254658059594475},1.3254658059594475,4.3625235529869499,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H47/C47*K47,IF(OPFOKLEGHEN!$H$20=\"ja\",O47-(K47-Q47)-(K47-S47),Q47-(K47-O47)-(K47-S47)))","v":1.3254658059594475},{"$f":"IF(H47=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q47-(K47-R47)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O47*80%-(K47-S47)),(Q47-(K47-S47)-(K47-T47))),(N47-(K47-S47))))","v":2.650931611918895},{"$f":"IF(H47=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q47-(K47-R47)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O47*80%-(K47-S47)),(Q47-(K47-S47)-(K47-N47))),(N47-(K47-S47))))","v":2.650931611918895},{"$f":"IF(H47=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q47-(K47-R47)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O47-(K47-S47)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N47-(K47-Q47)-(K47-S47)),(Q47-(K47-N47/80%)))))),(O47-(K47-S47))))","v":2.650931611918895},1,null,null,{"$f":"IF(H47=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P47-(K47-R47),K47-(K47-O47)/I$6-(K47-R47)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K47-O47)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O47-(K47-S47),IF(OPFOKLEGHEN!$H$20=\"nee\",(O47-(K47-S47)),(O47-(K47-S47)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O47*80%-(K47-S47),0+O47-(K47-S47)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O47*80%-(K47-S47)),O47*93%-(K47-S47)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O47-(K47-S47))),O47-(K47-S47))))))))","v":1.3254658059594475},{"$f":"IF(H47=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q47-(K47-R47),N47-(K47-R47)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q47-(K47-N47)-(K47-S47),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q47-(K47-N47)-(K47-S47)),(O47-(K47-S47)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q47*$N$135-(K47-N47)-(K47-S47),(Q47-(K47-N47)-(K47-S47))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N47*95%-(K47-Q47)/I$4-(K47-S47)),N47-(K47-Q47)/I$4-(K47-S47)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N47-(K47-Q47)/I$4-(K47-S47))),N47-(K47-Q47)/I$4-(K47-S47))))))))","v":1.3254658059594475},0,0.37513994993707267,0,0,0.37513994993707267,0,0.403339825535036,4.8418842226829132E-3,5,32,338,297.79999999999995,317.89999999999998,4.3625235529869499]
[5,33,0.41423711679774999,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C48)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C48<$I$3,C48-D48,MIN($I$3,C48-D48))))","v":0},{"$f":"IF(C48<$I$7,MAX(0,C48-D48-E48-F48,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C48-D48-F48)),MIN(I$7,MAX(0,C48-D48-E48-F48))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C48-D48-E48-F48,MIN(I$7,C48-E48-F48)),MIN(I$7,MAX(0,C48-D48-F48))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C48-F48-G48,C48-D48-F48-G48),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C48-G48,IF(OPFOKLEGHEN!$J$18=\"nee\",C48-D48-G48)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C48-G48,C48-D48-F48-G48),C48-D48-F48-G48))","v":0.41423711679774999},0.41423711679774999,0.38210641999420758,1.3865561167400018,{"$f":"SUM(K$16:K48)/$K$137","v":2.6673698020801325E-2},5.2233278370342525E-3,{"$f":"(((($K48)*(1-($I$6*(D48)/C48)))))","v":1.3865561167400018},{"$f":"IF(E48<I$3,P48*(1-I$6*D48/C48),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P48*(1-$I$6)+(C48-D48)/C48*(K48-P48*(1-I$6)),P48*(1-$I$6)+(C48-D48)/C48*(K48-P48*(1-I$6))))","v":1.3865561167400018},{"$f":"IF(E48=0,K48,K48-K48*I$4*E48/C48)","v":1.3865561167400018},{"$f":"IF(F48=0,K48,K48-K48*I$4*F48/C48)","v":1.3865561167400018},1.3865561167400018,{"$f":"MIN(K48,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K48-(G48/(C48-G48))*(Q48)*95%,K48-(G48/(C48-G48))*(P48)*84%))","v":1.3865561167400018},1.3865561167400018,4.7844386990140118,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H48/C48*K48,IF(OPFOKLEGHEN!$H$20=\"ja\",O48-(K48-Q48)-(K48-S48),Q48-(K48-O48)-(K48-S48)))","v":1.3865561167400018},{"$f":"IF(H48=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q48-(K48-R48)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O48*80%-(K48-S48)),(Q48-(K48-S48)-(K48-T48))),(N48-(K48-S48))))","v":2.7731122334800036},{"$f":"IF(H48=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q48-(K48-R48)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O48*80%-(K48-S48)),(Q48-(K48-S48)-(K48-N48))),(N48-(K48-S48))))","v":2.7731122334800036},{"$f":"IF(H48=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q48-(K48-R48)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O48-(K48-S48)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N48-(K48-Q48)-(K48-S48)),(Q48-(K48-N48/80%)))))),(O48-(K48-S48))))","v":2.7731122334800036},{"$f":"Q48/K48","v":1},null,null,{"$f":"IF(H48=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P48-(K48-R48),K48-(K48-O48)/I$6-(K48-R48)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K48-O48)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O48-(K48-S48),IF(OPFOKLEGHEN!$H$20=\"nee\",(O48-(K48-S48)),(O48-(K48-S48)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O48*80%-(K48-S48),0+O48-(K48-S48)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O48*80%-(K48-S48)),O48*93%-(K48-S48)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O48-(K48-S48))),O48-(K48-S48))))))))","v":1.3865561167400018},{"$f":"IF(H48=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q48-(K48-R48),N48-(K48-R48)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q48-(K48-N48)-(K48-S48),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q48-(K48-N48)-(K48-S48)),(O48-(K48-S48)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q48*$N$135-(K48-N48)-(K48-S48),(Q48-(K48-N48)-(K48-S48))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N48*95%-(K48-Q48)/I$4-(K48-S48)),N48-(K48-Q48)/I$4-(K48-S48)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N48-(K48-Q48)/I$4-(K48-S48))),N48-(K48-Q48)/I$4-(K48-S48))))))))","v":1.3865561167400018},{"$f":"IF((D48+E48)<$I$3,D48+E48,$I$3)","v":0},{"$f":"IF($I$3>0,(J48*(1-$I$8)*(1-$I$4)),(J48*(1-$I$8)))","v":0.38210641999420758},{"$f":"($AF48/1000)*$B48*$AE48","v":0},{"$f":"D48","v":0},0.38210641999420758,{"$f":"(AI48/1000)*B48*AH48","v":0},{"$f":"IF($I$3>$I$5,C48-AE48,C48-AH48)","v":0.41423711679774999},{"$f":"((($J48/1000)*(1-$I$8))*$B48*$AK48)*(1-$I$9)","v":5.2233278370342525E-3},5,33,350,308.49999999999994,329.25,{"$f":"(($AP48/1000)*(1-$I$10)*$D48*$B48)+(($AQ48/1000)*(1-$I$10)*$E48*$B48)+(($AO48/1000)*(1-$I$10)*$I48*$B48)","v":4.7844386990140118}]
[5,34,0.42514400069910396,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C49)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C49<$I$3,C49-D49,MIN($I$3,C49-D49))))","v":0},{"$f":"IF(C49<$I$7,MAX(0,C49-D49-E49-F49,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C49-D49-F49)),MIN(I$7,MAX(0,C49-D49-E49-F49))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C49-D49-E49-F49,MIN(I$7,C49-E49-F49)),MIN(I$7,MAX(0,C49-D49-F49))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C49-F49-G49,C49-D49-F49-G49),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C49-G49,IF(OPFOKLEGHEN!$J$18=\"nee\",C49-D49-G49)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C49-G49,C49-D49-F49-G49),C49-D49-F49-G49))","v":0.42514400069910396},0.42514400069910396,0.38920225965078159,1.4494909703618071,{"$f":"SUM(K$16:K49)/$K$137","v":2.8371110098376992E-2},5.6258781954682006E-3,1.4494909703618071,{"$f":"IF(E49<I$3,P49*(1-I$6*D49/C49),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P49*(1-$I$6)+(C49-D49)/C49*(K49-P49*(1-I$6)),P49*(1-$I$6)+(C49-D49)/C49*(K49-P49*(1-I$6))))","v":1.4494909703618071},1.4494909703618071,1.4494909703618071,1.4494909703618071,{"$f":"MIN(K49,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K49-(G49/(C49-G49))*(Q49)*95%,K49-(G49/(C49-G49))*(P49)*84%))","v":1.4494909703618071},1.4494909703618071,5.232672360604572,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H49/C49*K49,IF(OPFOKLEGHEN!$H$20=\"ja\",O49-(K49-Q49)-(K49-S49),Q49-(K49-O49)-(K49-S49)))","v":1.4494909703618071},{"$f":"IF(H49=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q49-(K49-R49)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O49*80%-(K49-S49)),(Q49-(K49-S49)-(K49-T49))),(N49-(K49-S49))))","v":2.8989819407236141},{"$f":"IF(H49=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q49-(K49-R49)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O49*80%-(K49-S49)),(Q49-(K49-S49)-(K49-N49))),(N49-(K49-S49))))","v":2.8989819407236141},{"$f":"IF(H49=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q49-(K49-R49)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O49-(K49-S49)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N49-(K49-Q49)-(K49-S49)),(Q49-(K49-N49/80%)))))),(O49-(K49-S49))))","v":2.8989819407236141},1,null,null,{"$f":"IF(H49=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P49-(K49-R49),K49-(K49-O49)/I$6-(K49-R49)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K49-O49)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O49-(K49-S49),IF(OPFOKLEGHEN!$H$20=\"nee\",(O49-(K49-S49)),(O49-(K49-S49)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O49*80%-(K49-S49),0+O49-(K49-S49)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O49*80%-(K49-S49)),O49*93%-(K49-S49)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O49-(K49-S49))),O49-(K49-S49))))))))","v":1.4494909703618071},{"$f":"IF(H49=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q49-(K49-R49),N49-(K49-R49)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q49-(K49-N49)-(K49-S49),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q49-(K49-N49)-(K49-S49)),(O49-(K49-S49)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q49*$N$135-(K49-N49)-(K49-S49),(Q49-(K49-N49)-(K49-S49))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N49*95%-(K49-Q49)/I$4-(K49-S49)),N49-(K49-Q49)/I$4-(K49-S49)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N49-(K49-Q49)/I$4-(K49-S49))),N49-(K49-Q49)/I$4-(K49-S49))))))))","v":1.4494909703618071},0,0.38920225965078159,0,0,0.38920225965078159,0,0.42514400069910396,5.6258781954682006E-3,5,34,362,319.19999999999993,340.59999999999997,5.232672360604572]
[5,35,0.43659338919249996,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C50)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C50<$I$3,C50-D50,MIN($I$3,C50-D50))))","v":0},{"$f":"IF(C50<$I$7,MAX(0,C50-D50-E50-F50,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C50-D50-F50)),MIN(I$7,MAX(0,C50-D50-E50-F50))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C50-D50-E50-F50,MIN(I$7,C50-E50-F50)),MIN(I$7,MAX(0,C50-D50-F50))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C50-F50-G50,C50-D50-F50-G50),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C50-G50,IF(OPFOKLEGHEN!$J$18=\"nee\",C50-D50-G50)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C50-G50,C50-D50-F50-G50),C50-D50-F50-G50))","v":0.43659338919249996},0.43659338919249996,0.39642987134204843,1.5161690712918157,{"$f":"SUM(K$16:K50)/$K$137","v":3.0146604907161499E-2},6.0577531387230078E-3,1.5161690712918157,{"$f":"IF(E50<I$3,P50*(1-I$6*D50/C50),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P50*(1-$I$6)+(C50-D50)/C50*(K50-P50*(1-I$6)),P50*(1-$I$6)+(C50-D50)/C50*(K50-P50*(1-I$6))))","v":1.5161690712918157},1.5161690712918157,1.5161690712918157,1.5161690712918157,{"$f":"MIN(K50,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K50-(G50/(C50-G50))*(Q50)*95%,K50-(G50/(C50-G50))*(P50)*84%))","v":1.5161690712918157},{"$f":"$K50*(1-($I$6*(D50)/C50))-($I$4*F50/C50)","v":1.5161690712918157},5.7302882331515619,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H50/C50*K50,IF(OPFOKLEGHEN!$H$20=\"ja\",O50-(K50-Q50)-(K50-S50),Q50-(K50-O50)-(K50-S50)))","v":1.5161690712918157},{"$f":"IF(H50=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q50-(K50-R50)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O50*80%-(K50-S50)),(Q50-(K50-S50)-(K50-T50))),(N50-(K50-S50))))","v":3.0323381425836313},{"$f":"IF(H50=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q50-(K50-R50)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O50*80%-(K50-S50)),(Q50-(K50-S50)-(K50-N50))),(N50-(K50-S50))))","v":3.0323381425836313},{"$f":"IF(H50=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q50-(K50-R50)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O50-(K50-S50)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N50-(K50-Q50)-(K50-S50)),(Q50-(K50-N50/80%)))))),(O50-(K50-S50))))","v":3.0323381425836313},1,null,null,{"$f":"IF(H50=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P50-(K50-R50),K50-(K50-O50)/I$6-(K50-R50)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K50-O50)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O50-(K50-S50),IF(OPFOKLEGHEN!$H$20=\"nee\",(O50-(K50-S50)),(O50-(K50-S50)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O50*80%-(K50-S50),0+O50-(K50-S50)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O50*80%-(K50-S50)),O50*93%-(K50-S50)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O50-(K50-S50))),O50-(K50-S50))))))))","v":1.5161690712918157},{"$f":"IF(H50=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q50-(K50-R50),N50-(K50-R50)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q50-(K50-N50)-(K50-S50),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q50-(K50-N50)-(K50-S50)),(O50-(K50-S50)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q50*$N$135-(K50-N50)-(K50-S50),(Q50-(K50-N50)-(K50-S50))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N50*95%-(K50-Q50)/I$4-(K50-S50)),N50-(K50-Q50)/I$4-(K50-S50)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N50-(K50-Q50)/I$4-(K50-S50))),N50-(K50-Q50)/I$4-(K50-S50))))))))","v":1.5161690712918157},0,0.39642987134204843,0,0,0.39642987134204843,0,0.43659338919249996,6.0577531387230078E-3,5,35,375,330,352.5,5.7302882331515619]
[6,36,0.44757866387335593,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C51)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C51<$I$3,C51-D51,MIN($I$3,C51-D51))))","v":0},{"$f":"IF(C51<$I$7,MAX(0,C51-D51-E51-F51,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C51-D51-F51)),MIN(I$7,MAX(0,C51-D51-E51-F51))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C51-D51-E51-F51,MIN(I$7,C51-E51-F51)),MIN(I$7,MAX(0,C51-D51-F51))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C51-F51-G51,C51-D51-F51-G51),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C51-G51,IF(OPFOKLEGHEN!$J$18=\"nee\",C51-D51-G51)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C51-G51,C51-D51-F51-G51),C51-D51-F51-G51))","v":0.44757866387335593},0.44757866387335593,0.40379170211726045,1.5831821025270945,{"$f":"SUM(K$16:K51)/$K$137","v":3.2000574663979195E-2},6.5062278186044965E-3,1.5831821025270945,{"$f":"IF(E51<I$3,P51*(1-I$6*D51/C51),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P51*(1-$I$6)+(C51-D51)/C51*(K51-P51*(1-I$6)),P51*(1-$I$6)+(C51-D51)/C51*(K51-P51*(1-I$6))))","v":1.5831821025270945},1.5831821025270945,1.5831821025270945,1.5831821025270945,{"$f":"MIN(K51,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K51-(G51/(C51-G51))*(Q51)*95%,K51-(G51/(C51-G51))*(P51)*84%))","v":1.5831821025270945},1.5831821025270945,6.2372772282735394,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H51/C51*K51,IF(OPFOKLEGHEN!$H$20=\"ja\",O51-(K51-Q51)-(K51-S51),Q51-(K51-O51)-(K51-S51)))","v":1.5831821025270945},{"$f":"IF(H51=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q51-(K51-R51)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O51*80%-(K51-S51)),(Q51-(K51-S51)-(K51-T51))),(N51-(K51-S51))))","v":3.1663642050541889},{"$f":"IF(H51=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q51-(K51-R51)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O51*80%-(K51-S51)),(Q51-(K51-S51)-(K51-N51))),(N51-(K51-S51))))","v":3.1663642050541889},{"$f":"IF(H51=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q51-(K51-R51)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O51-(K51-S51)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N51-(K51-Q51)-(K51-S51)),(Q51-(K51-N51/80%)))))),(O51-(K51-S51))))","v":3.1663642050541889},1,null,null,{"$f":"IF(H51=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P51-(K51-R51),K51-(K51-O51)/I$6-(K51-R51)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K51-O51)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O51-(K51-S51),IF(OPFOKLEGHEN!$H$20=\"nee\",(O51-(K51-S51)),(O51-(K51-S51)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O51*80%-(K51-S51),0+O51-(K51-S51)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O51*80%-(K51-S51)),O51*93%-(K51-S51)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O51-(K51-S51))),O51-(K51-S51))))))))","v":1.5831821025270945},{"$f":"IF(H51=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q51-(K51-R51),N51-(K51-R51)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q51-(K51-N51)-(K51-S51),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q51-(K51-N51)-(K51-S51)),(O51-(K51-S51)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q51*$N$135-(K51-N51)-(K51-S51),(Q51-(K51-N51)-(K51-S51))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N51*95%-(K51-Q51)/I$4-(K51-S51)),N51-(K51-Q51)/I$4-(K51-S51)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N51-(K51-Q51)/I$4-(K51-S51))),N51-(K51-Q51)/I$4-(K51-S51))))))))","v":1.5831821025270945},0,0.40379170211726045,0,0,0.40379170211726045,0,0.44757866387335593,6.5062278186044965E-3,6,36,{"$f":"AO50+12.1","v":387.1},{"$f":"AP50+10.7","v":340.7},363.9,6.2372772282735394]
[6,37,0.45858399107030801,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C52)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C52<$I$3,C52-D52,MIN($I$3,C52-D52))))","v":0},{"$f":"IF(C52<$I$7,MAX(0,C52-D52-E52-F52,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C52-D52-F52)),MIN(I$7,MAX(0,C52-D52-E52-F52))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C52-D52-E52-F52,MIN(I$7,C52-E52-F52)),MIN(I$7,MAX(0,C52-D52-F52))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C52-F52-G52,C52-D52-F52-G52),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C52-G52,IF(OPFOKLEGHEN!$J$18=\"nee\",C52-D52-G52)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C52-G52,C52-D52-F52-G52),C52-D52-F52-G52))","v":0.45858399107030801},0.45858399107030801,0.4112902444681652,1.652233426937286,{"$f":"SUM(K$16:K52)/$K$137","v":3.393540629191099E-2},6.9786115064702729E-3,1.652233426937286,{"$f":"IF(E52<I$3,P52*(1-I$6*D52/C52),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P52*(1-$I$6)+(C52-D52)/C52*(K52-P52*(1-I$6)),P52*(1-$I$6)+(C52-D52)/C52*(K52-P52*(1-I$6))))","v":1.652233426937286},1.652233426937286,1.652233426937286,1.652233426937286,{"$f":"MIN(K52,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K52-(G52/(C52-G52))*(Q52)*95%,K52-(G52/(C52-G52))*(P52)*84%))","v":1.652233426937286},1.652233426937286,6.7734689817048785,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H52/C52*K52,IF(OPFOKLEGHEN!$H$20=\"ja\",O52-(K52-Q52)-(K52-S52),Q52-(K52-O52)-(K52-S52)))","v":1.652233426937286},{"$f":"IF(H52=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q52-(K52-R52)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O52*80%-(K52-S52)),(Q52-(K52-S52)-(K52-T52))),(N52-(K52-S52))))","v":3.3044668538745721},{"$f":"IF(H52=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q52-(K52-R52)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O52*80%-(K52-S52)),(Q52-(K52-S52)-(K52-N52))),(N52-(K52-S52))))","v":3.3044668538745721},{"$f":"IF(H52=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q52-(K52-R52)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O52-(K52-S52)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N52-(K52-Q52)-(K52-S52)),(Q52-(K52-N52/80%)))))),(O52-(K52-S52))))","v":3.3044668538745721},1,null,null,{"$f":"IF(H52=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P52-(K52-R52),K52-(K52-O52)/I$6-(K52-R52)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K52-O52)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O52-(K52-S52),IF(OPFOKLEGHEN!$H$20=\"nee\",(O52-(K52-S52)),(O52-(K52-S52)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O52*80%-(K52-S52),0+O52-(K52-S52)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O52*80%-(K52-S52)),O52*93%-(K52-S52)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O52-(K52-S52))),O52-(K52-S52))))))))","v":1.652233426937286},{"$f":"IF(H52=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q52-(K52-R52),N52-(K52-R52)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q52-(K52-N52)-(K52-S52),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q52-(K52-N52)-(K52-S52)),(O52-(K52-S52)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q52*$N$135-(K52-N52)-(K52-S52),(Q52-(K52-N52)-(K52-S52))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N52*95%-(K52-Q52)/I$4-(K52-S52)),N52-(K52-Q52)/I$4-(K52-S52)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N52-(K52-Q52)/I$4-(K52-S52))),N52-(K52-Q52)/I$4-(K52-S52))))))))","v":1.652233426937286},0,0.4112902444681652,0,0,0.4112902444681652,0,0.45858399107030801,6.9786115064702729E-3,6,37,399.20000000000005,351.4,375.3,6.7734689817048785]
[6,38,0.469612784260732,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C53)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C53<$I$3,C53-D53,MIN($I$3,C53-D53))))","v":0},{"$f":"IF(C53<$I$7,MAX(0,C53-D53-E53-F53,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C53-D53-F53)),MIN(I$7,MAX(0,C53-D53-E53-F53))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C53-D53-E53-F53,MIN(I$7,C53-E53-F53)),MIN(I$7,MAX(0,C53-D53-F53))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C53-F53-G53,C53-D53-F53-G53),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C53-G53,IF(OPFOKLEGHEN!$J$18=\"nee\",C53-D53-G53)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C53-G53,C53-D53-F53-G53),C53-D53-F53-G53))","v":0.469612784260732},0.469612784260732,0.41892803717288729,1.723389506608793,{"$f":"SUM(K$16:K53)/$K$137","v":3.595356454380734E-2},7.4758905537824346E-3,1.723389506608793,{"$f":"IF(E53<I$3,P53*(1-I$6*D53/C53),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P53*(1-$I$6)+(C53-D53)/C53*(K53-P53*(1-I$6)),P53*(1-$I$6)+(C53-D53)/C53*(K53-P53*(1-I$6))))","v":1.723389506608793},1.723389506608793,1.723389506608793,1.723389506608793,{"$f":"MIN(K53,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K53-(G53/(C53-G53))*(Q53)*95%,K53-(G53/(C53-G53))*(P53)*84%))","v":1.723389506608793},1.723389506608793,7.3397660503246858,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H53/C53*K53,IF(OPFOKLEGHEN!$H$20=\"ja\",O53-(K53-Q53)-(K53-S53),Q53-(K53-O53)-(K53-S53)))","v":1.723389506608793},{"$f":"IF(H53=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q53-(K53-R53)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O53*80%-(K53-S53)),(Q53-(K53-S53)-(K53-T53))),(N53-(K53-S53))))","v":3.446779013217586},{"$f":"IF(H53=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q53-(K53-R53)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O53*80%-(K53-S53)),(Q53-(K53-S53)-(K53-N53))),(N53-(K53-S53))))","v":3.446779013217586},{"$f":"IF(H53=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q53-(K53-R53)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O53-(K53-S53)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N53-(K53-Q53)-(K53-S53)),(Q53-(K53-N53/80%)))))),(O53-(K53-S53))))","v":3.446779013217586},1,null,null,{"$f":"IF(H53=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P53-(K53-R53),K53-(K53-O53)/I$6-(K53-R53)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K53-O53)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O53-(K53-S53),IF(OPFOKLEGHEN!$H$20=\"nee\",(O53-(K53-S53)),(O53-(K53-S53)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O53*80%-(K53-S53),0+O53-(K53-S53)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O53*80%-(K53-S53)),O53*93%-(K53-S53)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O53-(K53-S53))),O53-(K53-S53))))))))","v":1.723389506608793},{"$f":"IF(H53=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q53-(K53-R53),N53-(K53-R53)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q53-(K53-N53)-(K53-S53),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q53-(K53-N53)-(K53-S53)),(O53-(K53-S53)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q53*$N$135-(K53-N53)-(K53-S53),(Q53-(K53-N53)-(K53-S53))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N53*95%-(K53-Q53)/I$4-(K53-S53)),N53-(K53-Q53)/I$4-(K53-S53)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N53-(K53-Q53)/I$4-(K53-S53))),N53-(K53-Q53)/I$4-(K53-S53))))))))","v":1.723389506608793},0,0.41892803717288729,0,0,0.41892803717288729,0,0.469612784260732,7.4758905537824346E-3,6,38,411.30000000000007,362.09999999999997,386.70000000000005,7.3397660503246858]
[6,39,0.48066845692200399,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C54)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C54<$I$3,C54-D54,MIN($I$3,C54-D54))))","v":0},{"$f":"IF(C54<$I$7,MAX(0,C54-D54-E54-F54,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C54-D54-F54)),MIN(I$7,MAX(0,C54-D54-E54-F54))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C54-D54-E54-F54,MIN(I$7,C54-E54-F54)),MIN(I$7,MAX(0,C54-D54-F54))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C54-F54-G54,C54-D54-F54-G54),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C54-G54,IF(OPFOKLEGHEN!$J$18=\"nee\",C54-D54-G54)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C54-G54,C54-D54-F54-G54),C54-D54-F54-G54))","v":0.48066845692200399},0.48066845692200399,0.42670766615548111,1.796719059322244,{"$f":"SUM(K$16:K54)/$K$137","v":3.8057594643796662E-2},7.999091702462045E-3,1.796719059322244,{"$f":"IF(E54<I$3,P54*(1-I$6*D54/C54),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P54*(1-$I$6)+(C54-D54)/C54*(K54-P54*(1-I$6)),P54*(1-$I$6)+(C54-D54)/C54*(K54-P54*(1-I$6))))","v":1.796719059322244},1.796719059322244,1.796719059322244,1.796719059322244,{"$f":"MIN(K54,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K54-(G54/(C54-G54))*(Q54)*95%,K54-(G54/(C54-G54))*(P54)*84%))","v":1.796719059322244},1.796719059322244,7.9370859617702845,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H54/C54*K54,IF(OPFOKLEGHEN!$H$20=\"ja\",O54-(K54-Q54)-(K54-S54),Q54-(K54-O54)-(K54-S54)))","v":1.796719059322244},{"$f":"IF(H54=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q54-(K54-R54)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O54*80%-(K54-S54)),(Q54-(K54-S54)-(K54-T54))),(N54-(K54-S54))))","v":3.5934381186444879},{"$f":"IF(H54=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q54-(K54-R54)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O54*80%-(K54-S54)),(Q54-(K54-S54)-(K54-N54))),(N54-(K54-S54))))","v":3.5934381186444879},{"$f":"IF(H54=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q54-(K54-R54)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O54-(K54-S54)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N54-(K54-Q54)-(K54-S54)),(Q54-(K54-N54/80%)))))),(O54-(K54-S54))))","v":3.5934381186444879},1,null,null,{"$f":"IF(H54=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P54-(K54-R54),K54-(K54-O54)/I$6-(K54-R54)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K54-O54)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O54-(K54-S54),IF(OPFOKLEGHEN!$H$20=\"nee\",(O54-(K54-S54)),(O54-(K54-S54)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O54*80%-(K54-S54),0+O54-(K54-S54)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O54*80%-(K54-S54)),O54*93%-(K54-S54)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O54-(K54-S54))),O54-(K54-S54))))))))","v":1.796719059322244},{"$f":"IF(H54=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q54-(K54-R54),N54-(K54-R54)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q54-(K54-N54)-(K54-S54),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q54-(K54-N54)-(K54-S54)),(O54-(K54-S54)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q54*$N$135-(K54-N54)-(K54-S54),(Q54-(K54-N54)-(K54-S54))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N54*95%-(K54-Q54)/I$4-(K54-S54)),N54-(K54-Q54)/I$4-(K54-S54)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N54-(K54-Q54)/I$4-(K54-S54))),N54-(K54-Q54)/I$4-(K54-S54))))))))","v":1.796719059322244},0,0.42670766615548111,0,0,0.42670766615548111,0,0.48066845692200399,7.999091702462045E-3,6,39,423.40000000000009,372.79999999999995,398.1,7.9370859617702845]
[6,40,0.49175442253149998,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C55)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C55<$I$3,C55-D55,MIN($I$3,C55-D55))))","v":0},{"$f":"IF(C55<$I$7,MAX(0,C55-D55-E55-F55,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C55-D55-F55)),MIN(I$7,MAX(0,C55-D55-E55-F55))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C55-D55-E55-F55,MIN(I$7,C55-E55-F55)),MIN(I$7,MAX(0,C55-D55-F55))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C55-F55-G55,C55-D55-F55-G55),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C55-G55,IF(OPFOKLEGHEN!$J$18=\"nee\",C55-D55-G55)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C55-G55,C55-D55-F55-G55),C55-D55-F55-G55))","v":0.49175442253149998},0.49175442253149998,0.43463176536144604,1.8722931328330794,{"$f":"SUM(K$16:K55)/$K$137","v":4.0250125015779299E-2},8.5492837115665708E-3,1.8722931328330794,{"$f":"IF(E55<I$3,P55*(1-I$6*D55/C55),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P55*(1-$I$6)+(C55-D55)/C55*(K55-P55*(1-I$6)),P55*(1-$I$6)+(C55-D55)/C55*(K55-P55*(1-I$6))))","v":1.8722931328330794},1.8722931328330794,1.8722931328330794,1.8722931328330794,{"$f":"MIN(K55,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K55-(G55/(C55-G55))*(Q55)*95%,K55-(G55/(C55-G55))*(P55)*84%))","v":1.8722931328330794},1.8722931328330794,8.5663620404987313,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H55/C55*K55,IF(OPFOKLEGHEN!$H$20=\"ja\",O55-(K55-Q55)-(K55-S55),Q55-(K55-O55)-(K55-S55)))","v":1.8722931328330794},{"$f":"IF(H55=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q55-(K55-R55)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O55*80%-(K55-S55)),(Q55-(K55-S55)-(K55-T55))),(N55-(K55-S55))))","v":3.7445862656661588},{"$f":"IF(H55=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q55-(K55-R55)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O55*80%-(K55-S55)),(Q55-(K55-S55)-(K55-N55))),(N55-(K55-S55))))","v":3.7445862656661588},{"$f":"IF(H55=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q55-(K55-R55)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O55-(K55-S55)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N55-(K55-Q55)-(K55-S55)),(Q55-(K55-N55/80%)))))),(O55-(K55-S55))))","v":3.7445862656661588},1,null,null,{"$f":"IF(H55=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P55-(K55-R55),K55-(K55-O55)/I$6-(K55-R55)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K55-O55)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O55-(K55-S55),IF(OPFOKLEGHEN!$H$20=\"nee\",(O55-(K55-S55)),(O55-(K55-S55)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O55*80%-(K55-S55),0+O55-(K55-S55)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O55*80%-(K55-S55)),O55*93%-(K55-S55)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O55-(K55-S55))),O55-(K55-S55))))))))","v":1.8722931328330794},{"$f":"IF(H55=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q55-(K55-R55),N55-(K55-R55)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q55-(K55-N55)-(K55-S55),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q55-(K55-N55)-(K55-S55)),(O55-(K55-S55)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q55*$N$135-(K55-N55)-(K55-S55),(Q55-(K55-N55)-(K55-S55))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N55*95%-(K55-Q55)/I$4-(K55-S55)),N55-(K55-Q55)/I$4-(K55-S55)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N55-(K55-Q55)/I$4-(K55-S55))),N55-(K55-Q55)/I$4-(K55-S55))))))))","v":1.8722931328330794},0,0.43463176536144604,0,0,0.43463176536144604,0,0.49175442253149998,8.5492837115665708E-3,6,40,435.50000000000011,383.49999999999994,409.5,8.5663620404987313]
[6,41,0.50287409456659604,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C56)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C56<$I$3,C56-D56,MIN($I$3,C56-D56))))","v":0},{"$f":"IF(C56<$I$7,MAX(0,C56-D56-E56-F56,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C56-D56-F56)),MIN(I$7,MAX(0,C56-D56-E56-F56))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C56-D56-E56-F56,MIN(I$7,C56-E56-F56)),MIN(I$7,MAX(0,C56-D56-F56))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C56-F56-G56,C56-D56-F56-G56),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C56-G56,IF(OPFOKLEGHEN!$J$18=\"nee\",C56-D56-G56)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C56-G56,C56-D56-F56-G56),C56-D56-F56-G56))","v":0.50287409456659604},0.50287409456659604,0.44270301764950043,1.9501851814625564,{"$f":"SUM(K$16:K56)/$K$137","v":4.2533870101612678E-2},9.1275790456580852E-3,1.9501851814625564,{"$f":"IF(E56<I$3,P56*(1-I$6*D56/C56),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P56*(1-$I$6)+(C56-D56)/C56*(K56-P56*(1-I$6)),P56*(1-$I$6)+(C56-D56)/C56*(K56-P56*(1-I$6))))","v":1.9501851814625564},1.9501851814625564,1.9501851814625564,1.9501851814625564,{"$f":"MIN(K56,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K56-(G56/(C56-G56))*(Q56)*95%,K56-(G56/(C56-G56))*(P56)*84%))","v":1.9501851814625564},1.9501851814625564,9.2285442338483463,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H56/C56*K56,IF(OPFOKLEGHEN!$H$20=\"ja\",O56-(K56-Q56)-(K56-S56),Q56-(K56-O56)-(K56-S56)))","v":1.9501851814625564},{"$f":"IF(H56=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q56-(K56-R56)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O56*80%-(K56-S56)),(Q56-(K56-S56)-(K56-T56))),(N56-(K56-S56))))","v":3.9003703629251127},{"$f":"IF(H56=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q56-(K56-R56)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O56*80%-(K56-S56)),(Q56-(K56-S56)-(K56-N56))),(N56-(K56-S56))))","v":3.9003703629251127},{"$f":"IF(H56=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q56-(K56-R56)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O56-(K56-S56)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N56-(K56-Q56)-(K56-S56)),(Q56-(K56-N56/80%)))))),(O56-(K56-S56))))","v":3.9003703629251127},1,null,null,{"$f":"IF(H56=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P56-(K56-R56),K56-(K56-O56)/I$6-(K56-R56)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K56-O56)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O56-(K56-S56),IF(OPFOKLEGHEN!$H$20=\"nee\",(O56-(K56-S56)),(O56-(K56-S56)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O56*80%-(K56-S56),0+O56-(K56-S56)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O56*80%-(K56-S56)),O56*93%-(K56-S56)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O56-(K56-S56))),O56-(K56-S56))))))))","v":1.9501851814625564},{"$f":"IF(H56=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q56-(K56-R56),N56-(K56-R56)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q56-(K56-N56)-(K56-S56),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q56-(K56-N56)-(K56-S56)),(O56-(K56-S56)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q56*$N$135-(K56-N56)-(K56-S56),(Q56-(K56-N56)-(K56-S56))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N56*95%-(K56-Q56)/I$4-(K56-S56)),N56-(K56-Q56)/I$4-(K56-S56)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N56-(K56-Q56)/I$4-(K56-S56))),N56-(K56-Q56)/I$4-(K56-S56))))))))","v":1.9501851814625564},0,0.44270301764950043,0,0,0.44270301764950043,0,0.50287409456659604,9.1275790456580852E-3,6,41,447.60000000000014,394.19999999999993,420.90000000000003,9.2285442338483463]
[6,42,0.51422697151249996,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C57)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C57<$I$3,C57-D57,MIN($I$3,C57-D57))))","v":0},{"$f":"IF(C57<$I$7,MAX(0,C57-D57-E57-F57,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C57-D57-F57)),MIN(I$7,MAX(0,C57-D57-E57-F57))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C57-D57-E57-F57,MIN(I$7,C57-E57-F57)),MIN(I$7,MAX(0,C57-D57-F57))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C57-F57-G57,C57-D57-F57-G57),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C57-G57,IF(OPFOKLEGHEN!$J$18=\"nee\",C57-D57-G57)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C57-G57,C57-D57-F57-G57),C57-D57-F57-G57))","v":0.51422697151249996},0.51422697151249996,0.45092415569991562,2.0312456995944115,{"$f":"SUM(K$16:K57)/$K$137","v":4.4912540306198061E-2},9.7388492446307418E-3,2.0312456995944115,{"$f":"IF(E57<I$3,P57*(1-I$6*D57/C57),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P57*(1-$I$6)+(C57-D57)/C57*(K57-P57*(1-I$6)),P57*(1-$I$6)+(C57-D57)/C57*(K57-P57*(1-I$6))))","v":2.0312456995944115},2.0312456995944115,2.0312456995944115,2.0312456995944115,{"$f":"MIN(K57,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K57-(G57/(C57-G57))*(Q57)*95%,K57-(G57/(C57-G57))*(P57)*84%))","v":2.0312456995944115},2.0312456995944115,9.9348650896214998,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H57/C57*K57,IF(OPFOKLEGHEN!$H$20=\"ja\",O57-(K57-Q57)-(K57-S57),Q57-(K57-O57)-(K57-S57)))","v":2.0312456995944115},{"$f":"IF(H57=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q57-(K57-R57)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O57*80%-(K57-S57)),(Q57-(K57-S57)-(K57-T57))),(N57-(K57-S57))))","v":4.062491399188823},{"$f":"IF(H57=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q57-(K57-R57)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O57*80%-(K57-S57)),(Q57-(K57-S57)-(K57-N57))),(N57-(K57-S57))))","v":4.062491399188823},{"$f":"IF(H57=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q57-(K57-R57)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O57-(K57-S57)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N57-(K57-Q57)-(K57-S57)),(Q57-(K57-N57/80%)))))),(O57-(K57-S57))))","v":4.062491399188823},1,null,null,{"$f":"IF(H57=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P57-(K57-R57),K57-(K57-O57)/I$6-(K57-R57)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K57-O57)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O57-(K57-S57),IF(OPFOKLEGHEN!$H$20=\"nee\",(O57-(K57-S57)),(O57-(K57-S57)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O57*80%-(K57-S57),0+O57-(K57-S57)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O57*80%-(K57-S57)),O57*93%-(K57-S57)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O57-(K57-S57))),O57-(K57-S57))))))))","v":2.0312456995944115},{"$f":"IF(H57=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q57-(K57-R57),N57-(K57-R57)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q57-(K57-N57)-(K57-S57),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q57-(K57-N57)-(K57-S57)),(O57-(K57-S57)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q57*$N$135-(K57-N57)-(K57-S57),(Q57-(K57-N57)-(K57-S57))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N57*95%-(K57-Q57)/I$4-(K57-S57)),N57-(K57-Q57)/I$4-(K57-S57)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N57-(K57-Q57)/I$4-(K57-S57))),N57-(K57-Q57)/I$4-(K57-S57))))))))","v":2.0312456995944115},0,0.45092415569991562,0,0,0.45092415569991562,0,0.51422697151249996,9.7388492446307418E-3,6,42,460,405,432.5,9.9348650896214998]
[7,43,0.52616325889844595,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C58)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C58<$I$3,C58-D58,MIN($I$3,C58-D58))))","v":0},{"$f":"IF(C58<$I$7,MAX(0,C58-D58-E58-F58,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C58-D58-F58)),MIN(I$7,MAX(0,C58-D58-E58-F58))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C58-D58-E58-F58,MIN(I$7,C58-E58-F58)),MIN(I$7,MAX(0,C58-D58-F58))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C58-F58-G58,C58-D58-F58-G58),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C58-G58,IF(OPFOKLEGHEN!$J$18=\"nee\",C58-D58-G58)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C58-G58,C58-D58-F58-G58),C58-D58-F58-G58))","v":0.52616325889844595},0.52616325889844595,0.45929796293971847,2.1169916457554323,{"$f":"SUM(K$16:K58)/$K$137","v":4.7391622453729555E-2},1.0391625658388538E-2,2.1169916457554323,{"$f":"IF(E58<I$3,P58*(1-I$6*D58/C58),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P58*(1-$I$6)+(C58-D58)/C58*(K58-P58*(1-I$6)),P58*(1-$I$6)+(C58-D58)/C58*(K58-P58*(1-I$6))))","v":2.1169916457554323},2.1169916457554323,2.1169916457554323,2.1169916457554323,{"$f":"MIN(K58,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K58-(G58/(C58-G58))*(Q58)*95%,K58-(G58/(C58-G58))*(P58)*84%))","v":2.1169916457554323},2.1169916457554323,10.699372020722228,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H58/C58*K58,IF(OPFOKLEGHEN!$H$20=\"ja\",O58-(K58-Q58)-(K58-S58),Q58-(K58-O58)-(K58-S58)))","v":2.1169916457554323},{"$f":"IF(H58=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q58-(K58-R58)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O58*80%-(K58-S58)),(Q58-(K58-S58)-(K58-T58))),(N58-(K58-S58))))","v":4.2339832915108646},{"$f":"IF(H58=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q58-(K58-R58)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O58*80%-(K58-S58)),(Q58-(K58-S58)-(K58-N58))),(N58-(K58-S58))))","v":4.2339832915108646},{"$f":"IF(H58=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q58-(K58-R58)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O58-(K58-S58)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N58-(K58-Q58)-(K58-S58)),(Q58-(K58-N58/80%)))))),(O58-(K58-S58))))","v":4.2339832915108646},1,null,null,{"$f":"IF(H58=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P58-(K58-R58),K58-(K58-O58)/I$6-(K58-R58)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K58-O58)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O58-(K58-S58),IF(OPFOKLEGHEN!$H$20=\"nee\",(O58-(K58-S58)),(O58-(K58-S58)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O58*80%-(K58-S58),0+O58-(K58-S58)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O58*80%-(K58-S58)),O58*93%-(K58-S58)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O58-(K58-S58))),O58-(K58-S58))))))))","v":2.1169916457554323},{"$f":"IF(H58=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q58-(K58-R58),N58-(K58-R58)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q58-(K58-N58)-(K58-S58),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q58-(K58-N58)-(K58-S58)),(O58-(K58-S58)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q58*$N$135-(K58-N58)-(K58-S58),(Q58-(K58-N58)-(K58-S58))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N58*95%-(K58-Q58)/I$4-(K58-S58)),N58-(K58-Q58)/I$4-(K58-S58)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N58-(K58-Q58)/I$4-(K58-S58))),N58-(K58-Q58)/I$4-(K58-S58))))))))","v":2.1169916457554323},0,0.45929796293971847,0,0,0.45929796293971847,0,0.52616325889844595,1.0391625658388538E-2,7,43,{"$f":"AO57+12.9","v":472.9},{"$f":"AP57+11.4","v":416.4},444.65,10.699372020722228]
[7,44,0.53814978895272791,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C59)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C59<$I$3,C59-D59,MIN($I$3,C59-D59))))","v":0},{"$f":"IF(C59<$I$7,MAX(0,C59-D59-E59-F59,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C59-D59-F59)),MIN(I$7,MAX(0,C59-D59-E59-F59))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C59-D59-E59-F59,MIN(I$7,C59-E59-F59)),MIN(I$7,MAX(0,C59-D59-F59))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C59-F59-G59,C59-D59-F59-G59),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C59-G59,IF(OPFOKLEGHEN!$J$18=\"nee\",C59-D59-G59)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C59-G59,C59-D59-F59-G59),C59-D59-F59-G59))","v":0.53814978895272791},0.53814978895272791,0.46782727448507472,2.2054276655069422,{"$f":"SUM(K$16:K59)/$K$137","v":4.9974266728303102E-2},1.1077490557340806E-2,2.2054276655069422,{"$f":"IF(E59<I$3,P59*(1-I$6*D59/C59),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P59*(1-$I$6)+(C59-D59)/C59*(K59-P59*(1-I$6)),P59*(1-$I$6)+(C59-D59)/C59*(K59-P59*(1-I$6))))","v":2.2054276655069422},2.2054276655069422,2.2054276655069422,2.2054276655069422,{"$f":"MIN(K59,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K59-(G59/(C59-G59))*(Q59)*95%,K59-(G59/(C59-G59))*(P59)*84%))","v":2.2054276655069422},2.2054276655069422,11.503059368822349,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H59/C59*K59,IF(OPFOKLEGHEN!$H$20=\"ja\",O59-(K59-Q59)-(K59-S59),Q59-(K59-O59)-(K59-S59)))","v":2.2054276655069422},{"$f":"IF(H59=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q59-(K59-R59)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O59*80%-(K59-S59)),(Q59-(K59-S59)-(K59-T59))),(N59-(K59-S59))))","v":4.4108553310138845},{"$f":"IF(H59=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q59-(K59-R59)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O59*80%-(K59-S59)),(Q59-(K59-S59)-(K59-N59))),(N59-(K59-S59))))","v":4.4108553310138845},{"$f":"IF(H59=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q59-(K59-R59)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O59-(K59-S59)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N59-(K59-Q59)-(K59-S59)),(Q59-(K59-N59/80%)))))),(O59-(K59-S59))))","v":4.4108553310138845},1,null,null,{"$f":"IF(H59=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P59-(K59-R59),K59-(K59-O59)/I$6-(K59-R59)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K59-O59)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O59-(K59-S59),IF(OPFOKLEGHEN!$H$20=\"nee\",(O59-(K59-S59)),(O59-(K59-S59)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O59*80%-(K59-S59),0+O59-(K59-S59)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O59*80%-(K59-S59)),O59*93%-(K59-S59)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O59-(K59-S59))),O59-(K59-S59))))))))","v":2.2054276655069422},{"$f":"IF(H59=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q59-(K59-R59),N59-(K59-R59)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q59-(K59-N59)-(K59-S59),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q59-(K59-N59)-(K59-S59)),(O59-(K59-S59)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q59*$N$135-(K59-N59)-(K59-S59),(Q59-(K59-N59)-(K59-S59))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N59*95%-(K59-Q59)/I$4-(K59-S59)),N59-(K59-Q59)/I$4-(K59-S59)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N59-(K59-Q59)/I$4-(K59-S59))),N59-(K59-Q59)/I$4-(K59-S59))))))))","v":2.2054276655069422},0,0.46782727448507472,0,0,0.46782727448507472,0,0.53814978895272791,1.1077490557340806E-2,7,44,485.79999999999995,427.79999999999995,456.79999999999995,11.503059368822349]
[7,45,0.55019069416056188,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C60)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C60<$I$3,C60-D60,MIN($I$3,C60-D60))))","v":0},{"$f":"IF(C60<$I$7,MAX(0,C60-D60-E60-F60,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C60-D60-F60)),MIN(I$7,MAX(0,C60-D60-E60-F60))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C60-D60-E60-F60,MIN(I$7,C60-E60-F60)),MIN(I$7,MAX(0,C60-D60-F60))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C60-F60-G60,C60-D60-F60-G60),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C60-G60,IF(OPFOKLEGHEN!$J$18=\"nee\",C60-D60-G60)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C60-G60,C60-D60-F60-G60),C60-D60-F60-G60))","v":0.55019069416056188},0.55019069416056188,0.47651497810117321,2.2966451736354521,{"$f":"SUM(K$16:K60)/$K$137","v":5.2663730364397095E-2},1.1797834796072526E-2,2.2966451736354521,{"$f":"IF(E60<I$3,P60*(1-I$6*D60/C60),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P60*(1-$I$6)+(C60-D60)/C60*(K60-P60*(1-I$6)),P60*(1-$I$6)+(C60-D60)/C60*(K60-P60*(1-I$6))))","v":2.2966451736354521},2.2966451736354521,2.2966451736354521,2.2966451736354521,{"$f":"MIN(K60,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K60-(G60/(C60-G60))*(Q60)*95%,K60-(G60/(C60-G60))*(P60)*84%))","v":2.2966451736354521},2.2966451736354521,12.347104463004246,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H60/C60*K60,IF(OPFOKLEGHEN!$H$20=\"ja\",O60-(K60-Q60)-(K60-S60),Q60-(K60-O60)-(K60-S60)))","v":2.2966451736354521},{"$f":"IF(H60=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q60-(K60-R60)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O60*80%-(K60-S60)),(Q60-(K60-S60)-(K60-T60))),(N60-(K60-S60))))","v":4.5932903472709041},{"$f":"IF(H60=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q60-(K60-R60)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O60*80%-(K60-S60)),(Q60-(K60-S60)-(K60-N60))),(N60-(K60-S60))))","v":4.5932903472709041},{"$f":"IF(H60=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q60-(K60-R60)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O60-(K60-S60)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N60-(K60-Q60)-(K60-S60)),(Q60-(K60-N60/80%)))))),(O60-(K60-S60))))","v":4.5932903472709041},1,null,null,{"$f":"IF(H60=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P60-(K60-R60),K60-(K60-O60)/I$6-(K60-R60)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K60-O60)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O60-(K60-S60),IF(OPFOKLEGHEN!$H$20=\"nee\",(O60-(K60-S60)),(O60-(K60-S60)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O60*80%-(K60-S60),0+O60-(K60-S60)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O60*80%-(K60-S60)),O60*93%-(K60-S60)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O60-(K60-S60))),O60-(K60-S60))))))))","v":2.2966451736354521},{"$f":"IF(H60=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q60-(K60-R60),N60-(K60-R60)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q60-(K60-N60)-(K60-S60),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q60-(K60-N60)-(K60-S60)),(O60-(K60-S60)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q60*$N$135-(K60-N60)-(K60-S60),(Q60-(K60-N60)-(K60-S60))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N60*95%-(K60-Q60)/I$4-(K60-S60)),N60-(K60-Q60)/I$4-(K60-S60)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N60-(K60-Q60)/I$4-(K60-S60))),N60-(K60-Q60)/I$4-(K60-S60))))))))","v":2.2966451736354521},0,0.47651497810117321,0,0,0.47651497810117321,0,0.55019069416056188,1.1797834796072526E-2,7,45,498.69999999999993,439.19999999999993,468.94999999999993,12.347104463004246]
[7,46,0.56229010700716398,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C61)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C61<$I$3,C61-D61,MIN($I$3,C61-D61))))","v":0},{"$f":"IF(C61<$I$7,MAX(0,C61-D61-E61-F61,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C61-D61-F61)),MIN(I$7,MAX(0,C61-D61-E61-F61))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C61-D61-E61-F61,MIN(I$7,C61-E61-F61)),MIN(I$7,MAX(0,C61-D61-F61))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C61-F61-G61,C61-D61-F61-G61),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C61-G61,IF(OPFOKLEGHEN!$J$18=\"nee\",C61-D61-G61)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C61-G61,C61-D61-F61-G61),C61-D61-F61-G61))","v":0.56229010700716398},0.56229010700716398,0.48536401517993538,2.3907387641286646,{"$f":"SUM(K$16:K61)/$K$137","v":5.546338136984446E-2},1.2554107665515821E-2,2.3907387641286646,{"$f":"IF(E61<I$3,P61*(1-I$6*D61/C61),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P61*(1-$I$6)+(C61-D61)/C61*(K61-P61*(1-I$6)),P61*(1-$I$6)+(C61-D61)/C61*(K61-P61*(1-I$6))))","v":2.3907387641286646},2.3907387641286646,2.3907387641286646,2.3907387641286646,{"$f":"MIN(K61,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K61-(G61/(C61-G61))*(Q61)*95%,K61-(G61/(C61-G61))*(P61)*84%))","v":2.3907387641286646},2.3907387641286646,13.232710462263793,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H61/C61*K61,IF(OPFOKLEGHEN!$H$20=\"ja\",O61-(K61-Q61)-(K61-S61),Q61-(K61-O61)-(K61-S61)))","v":2.3907387641286646},{"$f":"IF(H61=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q61-(K61-R61)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O61*80%-(K61-S61)),(Q61-(K61-S61)-(K61-T61))),(N61-(K61-S61))))","v":4.7814775282573292},{"$f":"IF(H61=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q61-(K61-R61)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O61*80%-(K61-S61)),(Q61-(K61-S61)-(K61-N61))),(N61-(K61-S61))))","v":4.7814775282573292},{"$f":"IF(H61=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q61-(K61-R61)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O61-(K61-S61)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N61-(K61-Q61)-(K61-S61)),(Q61-(K61-N61/80%)))))),(O61-(K61-S61))))","v":4.7814775282573292},1,null,null,{"$f":"IF(H61=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P61-(K61-R61),K61-(K61-O61)/I$6-(K61-R61)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K61-O61)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O61-(K61-S61),IF(OPFOKLEGHEN!$H$20=\"nee\",(O61-(K61-S61)),(O61-(K61-S61)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O61*80%-(K61-S61),0+O61-(K61-S61)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O61*80%-(K61-S61)),O61*93%-(K61-S61)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O61-(K61-S61))),O61-(K61-S61))))))))","v":2.3907387641286646},{"$f":"IF(H61=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q61-(K61-R61),N61-(K61-R61)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q61-(K61-N61)-(K61-S61),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q61-(K61-N61)-(K61-S61)),(O61-(K61-S61)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q61*$N$135-(K61-N61)-(K61-S61),(Q61-(K61-N61)-(K61-S61))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N61*95%-(K61-Q61)/I$4-(K61-S61)),N61-(K61-Q61)/I$4-(K61-S61)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N61-(K61-Q61)/I$4-(K61-S61))),N61-(K61-Q61)/I$4-(K61-S61))))))))","v":2.3907387641286646},0,0.48536401517993538,0,0,0.48536401517993538,0,0.56229010700716398,1.2554107665515821E-2,7,46,511.59999999999991,450.59999999999991,481.09999999999991,13.232710462263793]
[7,47,0.5744521599777499,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C62)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C62<$I$3,C62-D62,MIN($I$3,C62-D62))))","v":0},{"$f":"IF(C62<$I$7,MAX(0,C62-D62-E62-F62,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C62-D62-F62)),MIN(I$7,MAX(0,C62-D62-E62-F62))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C62-D62-E62-F62,MIN(I$7,C62-E62-F62)),MIN(I$7,MAX(0,C62-D62-F62))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C62-F62-G62,C62-D62-F62-G62),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C62-G62,IF(OPFOKLEGHEN!$J$18=\"nee\",C62-D62-G62)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C62-G62,C62-D62-F62-G62),C62-D62-F62-G62))","v":0.5744521599777499},0.5744521599777499,0.49437738173588069,2.4878063158931343,{"$f":"SUM(K$16:K62)/$K$137","v":5.8376702372604457E-2},1.3347819274769098E-2,2.4878063158931343,{"$f":"IF(E62<I$3,P62*(1-I$6*D62/C62),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P62*(1-$I$6)+(C62-D62)/C62*(K62-P62*(1-I$6)),P62*(1-$I$6)+(C62-D62)/C62*(K62-P62*(1-I$6))))","v":2.4878063158931343},2.4878063158931343,2.4878063158931343,2.4878063158931343,{"$f":"MIN(K62,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K62-(G62/(C62-G62))*(Q62)*95%,K62-(G62/(C62-G62))*(P62)*84%))","v":2.4878063158931343},2.4878063158931343,14.161107421691499,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H62/C62*K62,IF(OPFOKLEGHEN!$H$20=\"ja\",O62-(K62-Q62)-(K62-S62),Q62-(K62-O62)-(K62-S62)))","v":2.4878063158931343},{"$f":"IF(H62=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q62-(K62-R62)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O62*80%-(K62-S62)),(Q62-(K62-S62)-(K62-T62))),(N62-(K62-S62))))","v":4.9756126317862686},{"$f":"IF(H62=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q62-(K62-R62)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O62*80%-(K62-S62)),(Q62-(K62-S62)-(K62-N62))),(N62-(K62-S62))))","v":4.9756126317862686},{"$f":"IF(H62=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q62-(K62-R62)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O62-(K62-S62)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N62-(K62-Q62)-(K62-S62)),(Q62-(K62-N62/80%)))))),(O62-(K62-S62))))","v":4.9756126317862686},1,null,null,{"$f":"IF(H62=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P62-(K62-R62),K62-(K62-O62)/I$6-(K62-R62)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K62-O62)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O62-(K62-S62),IF(OPFOKLEGHEN!$H$20=\"nee\",(O62-(K62-S62)),(O62-(K62-S62)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O62*80%-(K62-S62),0+O62-(K62-S62)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O62*80%-(K62-S62)),O62*93%-(K62-S62)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O62-(K62-S62))),O62-(K62-S62))))))))","v":2.4878063158931343},{"$f":"IF(H62=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q62-(K62-R62),N62-(K62-R62)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q62-(K62-N62)-(K62-S62),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q62-(K62-N62)-(K62-S62)),(O62-(K62-S62)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q62*$N$135-(K62-N62)-(K62-S62),(Q62-(K62-N62)-(K62-S62))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N62*95%-(K62-Q62)/I$4-(K62-S62)),N62-(K62-Q62)/I$4-(K62-S62)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N62-(K62-Q62)/I$4-(K62-S62))),N62-(K62-Q62)/I$4-(K62-S62))))))))","v":2.4878063158931343},0,0.49437738173588069,0,0,0.49437738173588069,0,0.5744521599777499,1.3347819274769098E-2,7,47,524.49999999999989,461.99999999999989,493.24999999999989,14.161107421691499]
[7,48,0.58668098555753589,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C63)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C63<$I$3,C63-D63,MIN($I$3,C63-D63))))","v":0},{"$f":"IF(C63<$I$7,MAX(0,C63-D63-E63-F63,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C63-D63-F63)),MIN(I$7,MAX(0,C63-D63-E63-F63))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C63-D63-E63-F63,MIN(I$7,C63-E63-F63)),MIN(I$7,MAX(0,C63-D63-F63))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C63-F63-G63,C63-D63-F63-G63),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C63-G63,IF(OPFOKLEGHEN!$J$18=\"nee\",C63-D63-G63)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C63-G63,C63-D63-F63-G63),C63-D63-F63-G63))","v":0.58668098555753589},0.58668098555753589,0.50355812942048617,2.5879491017683391,{"$f":"SUM(K$16:K63)/$K$137","v":6.1407294595194277E-2},1.4180543023388162E-2,2.5879491017683391,{"$f":"IF(E63<I$3,P63*(1-I$6*D63/C63),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P63*(1-$I$6)+(C63-D63)/C63*(K63-P63*(1-I$6)),P63*(1-$I$6)+(C63-D63)/C63*(K63-P63*(1-I$6))))","v":2.5879491017683391},2.5879491017683391,2.5879491017683391,2.5879491017683391,{"$f":"MIN(K63,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K63-(G63/(C63-G63))*(Q63)*95%,K63-(G63/(C63-G63))*(P63)*84%))","v":2.5879491017683391},2.5879491017683391,15.133553358653746,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H63/C63*K63,IF(OPFOKLEGHEN!$H$20=\"ja\",O63-(K63-Q63)-(K63-S63),Q63-(K63-O63)-(K63-S63)))","v":2.5879491017683391},{"$f":"IF(H63=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q63-(K63-R63)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O63*80%-(K63-S63)),(Q63-(K63-S63)-(K63-T63))),(N63-(K63-S63))))","v":5.1758982035366783},{"$f":"IF(H63=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q63-(K63-R63)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O63*80%-(K63-S63)),(Q63-(K63-S63)-(K63-N63))),(N63-(K63-S63))))","v":5.1758982035366783},{"$f":"IF(H63=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q63-(K63-R63)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O63-(K63-S63)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N63-(K63-Q63)-(K63-S63)),(Q63-(K63-N63/80%)))))),(O63-(K63-S63))))","v":5.1758982035366783},1,null,null,{"$f":"IF(H63=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P63-(K63-R63),K63-(K63-O63)/I$6-(K63-R63)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K63-O63)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O63-(K63-S63),IF(OPFOKLEGHEN!$H$20=\"nee\",(O63-(K63-S63)),(O63-(K63-S63)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O63*80%-(K63-S63),0+O63-(K63-S63)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O63*80%-(K63-S63)),O63*93%-(K63-S63)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O63-(K63-S63))),O63-(K63-S63))))))))","v":2.5879491017683391},{"$f":"IF(H63=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q63-(K63-R63),N63-(K63-R63)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q63-(K63-N63)-(K63-S63),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q63-(K63-N63)-(K63-S63)),(O63-(K63-S63)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q63*$N$135-(K63-N63)-(K63-S63),(Q63-(K63-N63)-(K63-S63))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N63*95%-(K63-Q63)/I$4-(K63-S63)),N63-(K63-Q63)/I$4-(K63-S63)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N63-(K63-Q63)/I$4-(K63-S63))),N63-(K63-Q63)/I$4-(K63-S63))))))))","v":2.5879491017683391},0,0.50355812942048617,0,0,0.50355812942048617,0,0.58668098555753589,1.4180543023388162E-2,7,48,537.39999999999986,473.39999999999986,505.39999999999986,15.133553358653746]
[7,49,0.59892994912749997,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C64)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C64<$I$3,C64-D64,MIN($I$3,C64-D64))))","v":0},{"$f":"IF(C64<$I$7,MAX(0,C64-D64-E64-F64,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C64-D64-F64)),MIN(I$7,MAX(0,C64-D64-E64-F64))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C64-D64-E64-F64,MIN(I$7,C64-E64-F64)),MIN(I$7,MAX(0,C64-D64-F64))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C64-F64-G64,C64-D64-F64-G64),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C64-G64,IF(OPFOKLEGHEN!$J$18=\"nee\",C64-D64-G64)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C64-G64,C64-D64-F64-G64),C64-D64-F64-G64))","v":0.59892994912749997},0.59892994912749997,0.51290936655538244,2.6910437999659731,{"$f":"SUM(K$16:K64)/$K$137","v":6.4558614845369539E-2},1.505264226008364E-2,2.6910437999659731,{"$f":"IF(E64<I$3,P64*(1-I$6*D64/C64),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P64*(1-$I$6)+(C64-D64)/C64*(K64-P64*(1-I$6)),P64*(1-$I$6)+(C64-D64)/C64*(K64-P64*(1-I$6))))","v":2.6910437999659731},2.6910437999659731,2.6910437999659731,2.6910437999659731,{"$f":"MIN(K64,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K64-(G64/(C64-G64))*(Q64)*95%,K64-(G64/(C64-G64))*(P64)*84%))","v":2.6910437999659731},2.6910437999659731,16.141162128986124,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H64/C64*K64,IF(OPFOKLEGHEN!$H$20=\"ja\",O64-(K64-Q64)-(K64-S64),Q64-(K64-O64)-(K64-S64)))","v":2.6910437999659731},{"$f":"IF(H64=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q64-(K64-R64)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O64*80%-(K64-S64)),(Q64-(K64-S64)-(K64-T64))),(N64-(K64-S64))))","v":5.3820875999319462},{"$f":"IF(H64=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q64-(K64-R64)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O64*80%-(K64-S64)),(Q64-(K64-S64)-(K64-N64))),(N64-(K64-S64))))","v":5.3820875999319462},{"$f":"IF(H64=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q64-(K64-R64)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O64-(K64-S64)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N64-(K64-Q64)-(K64-S64)),(Q64-(K64-N64/80%)))))),(O64-(K64-S64))))","v":5.3820875999319462},1,null,null,{"$f":"IF(H64=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P64-(K64-R64),K64-(K64-O64)/I$6-(K64-R64)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K64-O64)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O64-(K64-S64),IF(OPFOKLEGHEN!$H$20=\"nee\",(O64-(K64-S64)),(O64-(K64-S64)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O64*80%-(K64-S64),0+O64-(K64-S64)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O64*80%-(K64-S64)),O64*93%-(K64-S64)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O64-(K64-S64))),O64-(K64-S64))))))))","v":2.6910437999659731},{"$f":"IF(H64=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q64-(K64-R64),N64-(K64-R64)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q64-(K64-N64)-(K64-S64),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q64-(K64-N64)-(K64-S64)),(O64-(K64-S64)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q64*$N$135-(K64-N64)-(K64-S64),(Q64-(K64-N64)-(K64-S64))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N64*95%-(K64-Q64)/I$4-(K64-S64)),N64-(K64-Q64)/I$4-(K64-S64)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N64-(K64-Q64)/I$4-(K64-S64))),N64-(K64-Q64)/I$4-(K64-S64))))))))","v":2.6910437999659731},0,0.51290936655538244,0,0,0.51290936655538244,0,0.59892994912749997,1.505264226008364E-2,7,49,550,485,517.5,16.141162128986124]
[8,50,0.61125331708818398,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C65)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C65<$I$3,C65-D65,MIN($I$3,C65-D65))))","v":0},{"$f":"IF(C65<$I$7,MAX(0,C65-D65-E65-F65,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C65-D65-F65)),MIN(I$7,MAX(0,C65-D65-E65-F65))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C65-D65-E65-F65,MIN(I$7,C65-E65-F65)),MIN(I$7,MAX(0,C65-D65-F65))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C65-F65-G65,C65-D65-F65-G65),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C65-G65,IF(OPFOKLEGHEN!$J$18=\"nee\",C65-D65-G65)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C65-G65,C65-D65-F65-G65),C65-D65-F65-G65))","v":0.61125331708818398},0.61125331708818398,0.52243425918473718,2.797415543251685,{"$f":"SUM(K$16:K65)/$K$137","v":6.7834500674398238E-2},1.5966983694358932E-2,2.797415543251685,{"$f":"IF(E65<I$3,P65*(1-I$6*D65/C65),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P65*(1-$I$6)+(C65-D65)/C65*(K65-P65*(1-I$6)),P65*(1-$I$6)+(C65-D65)/C65*(K65-P65*(1-I$6))))","v":2.797415543251685},2.797415543251685,2.797415543251685,2.797415543251685,{"$f":"MIN(K65,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K65-(G65/(C65-G65))*(Q65)*95%,K65-(G65/(C65-G65))*(P65)*84%))","v":2.797415543251685},2.797415543251685,17.17927447676341,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H65/C65*K65,IF(OPFOKLEGHEN!$H$20=\"ja\",O65-(K65-Q65)-(K65-S65),Q65-(K65-O65)-(K65-S65)))","v":2.797415543251685},{"$f":"IF(H65=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q65-(K65-R65)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O65*80%-(K65-S65)),(Q65-(K65-S65)-(K65-T65))),(N65-(K65-S65))))","v":5.5948310865033699},{"$f":"IF(H65=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q65-(K65-R65)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O65*80%-(K65-S65)),(Q65-(K65-S65)-(K65-N65))),(N65-(K65-S65))))","v":5.5948310865033699},{"$f":"IF(H65=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q65-(K65-R65)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O65-(K65-S65)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N65-(K65-Q65)-(K65-S65)),(Q65-(K65-N65/80%)))))),(O65-(K65-S65))))","v":5.5948310865033699},1,null,null,{"$f":"IF(H65=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P65-(K65-R65),K65-(K65-O65)/I$6-(K65-R65)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K65-O65)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O65-(K65-S65),IF(OPFOKLEGHEN!$H$20=\"nee\",(O65-(K65-S65)),(O65-(K65-S65)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O65*80%-(K65-S65),0+O65-(K65-S65)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O65*80%-(K65-S65)),O65*93%-(K65-S65)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O65-(K65-S65))),O65-(K65-S65))))))))","v":2.797415543251685},{"$f":"IF(H65=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q65-(K65-R65),N65-(K65-R65)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q65-(K65-N65)-(K65-S65),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q65-(K65-N65)-(K65-S65)),(O65-(K65-S65)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q65*$N$135-(K65-N65)-(K65-S65),(Q65-(K65-N65)-(K65-S65))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N65*95%-(K65-Q65)/I$4-(K65-S65)),N65-(K65-Q65)/I$4-(K65-S65)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N65-(K65-Q65)/I$4-(K65-S65))),N65-(K65-Q65)/I$4-(K65-S65))))))))","v":2.797415543251685},0,0.52243425918473718,0,0,0.52243425918473718,0,0.61125331708818398,1.5966983694358932E-2,8,50,{"$f":"AO64+12.1","v":562.1},{"$f":"AP64+12.1","v":497.1},529.6,17.17927447676341]
[8,51,0.623655171116132,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C66)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C66<$I$3,C66-D66,MIN($I$3,C66-D66))))","v":0},{"$f":"IF(C66<$I$7,MAX(0,C66-D66-E66-F66,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C66-D66-F66)),MIN(I$7,MAX(0,C66-D66-E66-F66))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C66-D66-E66-F66,MIN(I$7,C66-E66-F66)),MIN(I$7,MAX(0,C66-D66-F66))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C66-F66-G66,C66-D66-F66-G66),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C66-G66,IF(OPFOKLEGHEN!$J$18=\"nee\",C66-D66-G66)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C66-G66,C66-D66-F66-G66),C66-D66-F66-G66))","v":0.623655171116132},0.623655171116132,0.53213603214718075,2.907175840507692,{"$f":"SUM(K$16:K66)/$K$137","v":7.1238920214923007E-2},1.6925338797476285E-2,2.907175840507692,{"$f":"IF(E66<I$3,P66*(1-I$6*D66/C66),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P66*(1-$I$6)+(C66-D66)/C66*(K66-P66*(1-I$6)),P66*(1-$I$6)+(C66-D66)/C66*(K66-P66*(1-I$6))))","v":2.907175840507692},2.907175840507692,2.907175840507692,2.907175840507692,{"$f":"MIN(K66,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K66-(G66/(C66-G66))*(Q66)*95%,K66-(G66/(C66-G66))*(P66)*84%))","v":2.907175840507692},2.907175840507692,18.263242761999035,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H66/C66*K66,IF(OPFOKLEGHEN!$H$20=\"ja\",O66-(K66-Q66)-(K66-S66),Q66-(K66-O66)-(K66-S66)))","v":2.907175840507692},{"$f":"IF(H66=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q66-(K66-R66)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O66*80%-(K66-S66)),(Q66-(K66-S66)-(K66-T66))),(N66-(K66-S66))))","v":5.8143516810153839},{"$f":"IF(H66=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q66-(K66-R66)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O66*80%-(K66-S66)),(Q66-(K66-S66)-(K66-N66))),(N66-(K66-S66))))","v":5.8143516810153839},{"$f":"IF(H66=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q66-(K66-R66)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O66-(K66-S66)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N66-(K66-Q66)-(K66-S66)),(Q66-(K66-N66/80%)))))),(O66-(K66-S66))))","v":5.8143516810153839},1,null,null,{"$f":"IF(H66=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P66-(K66-R66),K66-(K66-O66)/I$6-(K66-R66)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K66-O66)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O66-(K66-S66),IF(OPFOKLEGHEN!$H$20=\"nee\",(O66-(K66-S66)),(O66-(K66-S66)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O66*80%-(K66-S66),0+O66-(K66-S66)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O66*80%-(K66-S66)),O66*93%-(K66-S66)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O66-(K66-S66))),O66-(K66-S66))))))))","v":2.907175840507692},{"$f":"IF(H66=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q66-(K66-R66),N66-(K66-R66)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q66-(K66-N66)-(K66-S66),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q66-(K66-N66)-(K66-S66)),(O66-(K66-S66)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q66*$N$135-(K66-N66)-(K66-S66),(Q66-(K66-N66)-(K66-S66))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N66*95%-(K66-Q66)/I$4-(K66-S66)),N66-(K66-Q66)/I$4-(K66-S66)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N66-(K66-Q66)/I$4-(K66-S66))),N66-(K66-Q66)/I$4-(K66-S66))))))))","v":2.907175840507692},0,0.53213603214718075,0,0,0.53213603214718075,0,0.623655171116132,1.6925338797476285E-2,8,51,{"$f":"AO65+12.1","v":574.20000000000005},509.20000000000005,541.70000000000005,18.263242761999035]
[8,52,0.63613959288788802,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C67)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C67<$I$3,C67-D67,MIN($I$3,C67-D67))))","v":0},{"$f":"IF(C67<$I$7,MAX(0,C67-D67-E67-F67,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C67-D67-F67)),MIN(I$7,MAX(0,C67-D67-E67-F67))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C67-D67-E67-F67,MIN(I$7,C67-E67-F67)),MIN(I$7,MAX(0,C67-D67-F67))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C67-F67-G67,C67-D67-F67-G67),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C67-G67,IF(OPFOKLEGHEN!$J$18=\"nee\",C67-D67-G67)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C67-G67,C67-D67-F67-G67),C67-D67-F67-G67))","v":0.63613959288788802},0.63613959288788802,0.54201797016763897,3.0204400361119648,{"$f":"SUM(K$16:K67)/$K$137","v":7.477597667248051E-2},1.7929552725778786E-2,3.0204400361119648,{"$f":"IF(E67<I$3,P67*(1-I$6*D67/C67),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P67*(1-$I$6)+(C67-D67)/C67*(K67-P67*(1-I$6)),P67*(1-$I$6)+(C67-D67)/C67*(K67-P67*(1-I$6))))","v":3.0204400361119648},3.0204400361119648,3.0204400361119648,3.0204400361119648,{"$f":"MIN(K67,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K67-(G67/(C67-G67))*(Q67)*95%,K67-(G67/(C67-G67))*(P67)*84%))","v":3.0204400361119648},3.0204400361119648,19.394369452128775,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H67/C67*K67,IF(OPFOKLEGHEN!$H$20=\"ja\",O67-(K67-Q67)-(K67-S67),Q67-(K67-O67)-(K67-S67)))","v":3.0204400361119648},{"$f":"IF(H67=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q67-(K67-R67)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O67*80%-(K67-S67)),(Q67-(K67-S67)-(K67-T67))),(N67-(K67-S67))))","v":6.0408800722239295},{"$f":"IF(H67=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q67-(K67-R67)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O67*80%-(K67-S67)),(Q67-(K67-S67)-(K67-N67))),(N67-(K67-S67))))","v":6.0408800722239295},{"$f":"IF(H67=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q67-(K67-R67)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O67-(K67-S67)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N67-(K67-Q67)-(K67-S67)),(Q67-(K67-N67/80%)))))),(O67-(K67-S67))))","v":6.0408800722239295},1,null,null,{"$f":"IF(H67=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P67-(K67-R67),K67-(K67-O67)/I$6-(K67-R67)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K67-O67)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O67-(K67-S67),IF(OPFOKLEGHEN!$H$20=\"nee\",(O67-(K67-S67)),(O67-(K67-S67)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O67*80%-(K67-S67),0+O67-(K67-S67)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O67*80%-(K67-S67)),O67*93%-(K67-S67)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O67-(K67-S67))),O67-(K67-S67))))))))","v":3.0204400361119648},{"$f":"IF(H67=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q67-(K67-R67),N67-(K67-R67)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q67-(K67-N67)-(K67-S67),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q67-(K67-N67)-(K67-S67)),(O67-(K67-S67)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q67*$N$135-(K67-N67)-(K67-S67),(Q67-(K67-N67)-(K67-S67))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N67*95%-(K67-Q67)/I$4-(K67-S67)),N67-(K67-Q67)/I$4-(K67-S67)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N67-(K67-Q67)/I$4-(K67-S67))),N67-(K67-Q67)/I$4-(K67-S67))))))))","v":3.0204400361119648},0,0.54201797016763897,0,0,0.54201797016763897,0,0.63613959288788802,1.7929552725778786E-2,8,52,586.30000000000007,521.30000000000007,553.80000000000007,19.394369452128775]
[8,53,0.648710664079996,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C68)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C68<$I$3,C68-D68,MIN($I$3,C68-D68))))","v":0},{"$f":"IF(C68<$I$7,MAX(0,C68-D68-E68-F68,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C68-D68-F68)),MIN(I$7,MAX(0,C68-D68-E68-F68))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C68-D68-E68-F68,MIN(I$7,C68-E68-F68)),MIN(I$7,MAX(0,C68-D68-F68))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C68-F68-G68,C68-D68-F68-G68),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C68-G68,IF(OPFOKLEGHEN!$J$18=\"nee\",C68-D68-G68)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C68-G68,C68-D68-F68-G68),C68-D68-F68-G68))","v":0.648710664079996},0.648710664079996,0.55208341896944024,3.1373274358016494,{"$f":"SUM(K$16:K68)/$K$137","v":7.8449912964411977E-2},1.8981547271402676E-2,3.1373274358016494,{"$f":"IF(E68<I$3,P68*(1-I$6*D68/C68),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P68*(1-$I$6)+(C68-D68)/C68*(K68-P68*(1-I$6)),P68*(1-$I$6)+(C68-D68)/C68*(K68-P68*(1-I$6))))","v":3.1373274358016494},3.1373274358016494,3.1373274358016494,3.1373274358016494,{"$f":"MIN(K68,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K68-(G68/(C68-G68))*(Q68)*95%,K68-(G68/(C68-G68))*(P68)*84%))","v":3.1373274358016494},3.1373274358016494,20.573988453429891,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H68/C68*K68,IF(OPFOKLEGHEN!$H$20=\"ja\",O68-(K68-Q68)-(K68-S68),Q68-(K68-O68)-(K68-S68)))","v":3.1373274358016494},{"$f":"IF(H68=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q68-(K68-R68)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O68*80%-(K68-S68)),(Q68-(K68-S68)-(K68-T68))),(N68-(K68-S68))))","v":6.2746548716032988},{"$f":"IF(H68=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q68-(K68-R68)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O68*80%-(K68-S68)),(Q68-(K68-S68)-(K68-N68))),(N68-(K68-S68))))","v":6.2746548716032988},{"$f":"IF(H68=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q68-(K68-R68)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O68-(K68-S68)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N68-(K68-Q68)-(K68-S68)),(Q68-(K68-N68/80%)))))),(O68-(K68-S68))))","v":6.2746548716032988},1,null,null,{"$f":"IF(H68=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P68-(K68-R68),K68-(K68-O68)/I$6-(K68-R68)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K68-O68)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O68-(K68-S68),IF(OPFOKLEGHEN!$H$20=\"nee\",(O68-(K68-S68)),(O68-(K68-S68)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O68*80%-(K68-S68),0+O68-(K68-S68)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O68*80%-(K68-S68)),O68*93%-(K68-S68)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O68-(K68-S68))),O68-(K68-S68))))))))","v":3.1373274358016494},{"$f":"IF(H68=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q68-(K68-R68),N68-(K68-R68)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q68-(K68-N68)-(K68-S68),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q68-(K68-N68)-(K68-S68)),(O68-(K68-S68)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q68*$N$135-(K68-N68)-(K68-S68),(Q68-(K68-N68)-(K68-S68))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N68*95%-(K68-Q68)/I$4-(K68-S68)),N68-(K68-Q68)/I$4-(K68-S68)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N68-(K68-Q68)/I$4-(K68-S68))),N68-(K68-Q68)/I$4-(K68-S68))))))))","v":3.1373274358016494},0,0.55208341896944024,0,0,0.55208341896944024,0,0.648710664079996,1.8981547271402676E-2,8,53,598.40000000000009,533.40000000000009,565.90000000000009,20.573988453429891]
[8,54,0.66137246636900004,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C69)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C69<$I$3,C69-D69,MIN($I$3,C69-D69))))","v":0},{"$f":"IF(C69<$I$7,MAX(0,C69-D69-E69-F69,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C69-D69-F69)),MIN(I$7,MAX(0,C69-D69-E69-F69))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C69-D69-E69-F69,MIN(I$7,C69-E69-F69)),MIN(I$7,MAX(0,C69-D69-F69))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C69-F69-G69,C69-D69-F69-G69),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C69-G69,IF(OPFOKLEGHEN!$J$18=\"nee\",C69-D69-G69)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C69-G69,C69-D69-F69-G69),C69-D69-F69-G69))","v":0.66137246636900004},0.66137246636900004,0.56233578640707649,3.2579614364163305,{"$f":"SUM(K$16:K69)/$K$137","v":8.2265116510708294E-2},2.0083323923114366E-2,3.2579614364163305,{"$f":"IF(E69<I$3,P69*(1-I$6*D69/C69),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P69*(1-$I$6)+(C69-D69)/C69*(K69-P69*(1-I$6)),P69*(1-$I$6)+(C69-D69)/C69*(K69-P69*(1-I$6))))","v":3.2579614364163305},3.2579614364163305,3.2579614364163305,3.2579614364163305,{"$f":"MIN(K69,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K69-(G69/(C69-G69))*(Q69)*95%,K69-(G69/(C69-G69))*(P69)*84%))","v":3.2579614364163305},3.2579614364163305,21.803466098786831,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H69/C69*K69,IF(OPFOKLEGHEN!$H$20=\"ja\",O69-(K69-Q69)-(K69-S69),Q69-(K69-O69)-(K69-S69)))","v":3.2579614364163305},{"$f":"IF(H69=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q69-(K69-R69)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O69*80%-(K69-S69)),(Q69-(K69-S69)-(K69-T69))),(N69-(K69-S69))))","v":6.515922872832661},{"$f":"IF(H69=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q69-(K69-R69)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O69*80%-(K69-S69)),(Q69-(K69-S69)-(K69-N69))),(N69-(K69-S69))))","v":6.515922872832661},{"$f":"IF(H69=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q69-(K69-R69)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O69-(K69-S69)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N69-(K69-Q69)-(K69-S69)),(Q69-(K69-N69/80%)))))),(O69-(K69-S69))))","v":6.515922872832661},1,null,null,{"$f":"IF(H69=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P69-(K69-R69),K69-(K69-O69)/I$6-(K69-R69)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K69-O69)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O69-(K69-S69),IF(OPFOKLEGHEN!$H$20=\"nee\",(O69-(K69-S69)),(O69-(K69-S69)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O69*80%-(K69-S69),0+O69-(K69-S69)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O69*80%-(K69-S69)),O69*93%-(K69-S69)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O69-(K69-S69))),O69-(K69-S69))))))))","v":3.2579614364163305},{"$f":"IF(H69=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q69-(K69-R69),N69-(K69-R69)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q69-(K69-N69)-(K69-S69),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q69-(K69-N69)-(K69-S69)),(O69-(K69-S69)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q69*$N$135-(K69-N69)-(K69-S69),(Q69-(K69-N69)-(K69-S69))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N69*95%-(K69-Q69)/I$4-(K69-S69)),N69-(K69-Q69)/I$4-(K69-S69)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N69-(K69-Q69)/I$4-(K69-S69))),N69-(K69-Q69)/I$4-(K69-S69))))))))","v":3.2579614364163305},0,0.56233578640707649,0,0,0.56233578640707649,0,0.66137246636900004,2.0083323923114366E-2,8,54,610.50000000000011,545.50000000000011,578.00000000000011,21.803466098786831]
[8,55,0.67412908143144412,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C70)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C70<$I$3,C70-D70,MIN($I$3,C70-D70))))","v":0},{"$f":"IF(C70<$I$7,MAX(0,C70-D70-E70-F70,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C70-D70-F70)),MIN(I$7,MAX(0,C70-D70-E70-F70))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C70-D70-E70-F70,MIN(I$7,C70-E70-F70)),MIN(I$7,MAX(0,C70-D70-F70))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C70-F70-G70,C70-D70-F70-G70),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C70-G70,IF(OPFOKLEGHEN!$J$18=\"nee\",C70-D70-G70)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C70-G70,C70-D70-F70-G70),C70-D70-F70-G70))","v":0.67412908143144412},0.67412908143144412,0.5727785436199978,3.3824696596338995,{"$f":"SUM(K$16:K70)/$K$137","v":8.6226124181465094E-2},2.1236967041080419E-2,3.3824696596338995,{"$f":"IF(E70<I$3,P70*(1-I$6*D70/C70),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P70*(1-$I$6)+(C70-D70)/C70*(K70-P70*(1-I$6)),P70*(1-$I$6)+(C70-D70)/C70*(K70-P70*(1-I$6))))","v":3.3824696596338995},3.3824696596338995,3.3824696596338995,3.3824696596338995,{"$f":"MIN(K70,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K70-(G70/(C70-G70))*(Q70)*95%,K70-(G70/(C70-G70))*(P70)*84%))","v":3.3824696596338995},3.3824696596338995,23.084202135456945,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H70/C70*K70,IF(OPFOKLEGHEN!$H$20=\"ja\",O70-(K70-Q70)-(K70-S70),Q70-(K70-O70)-(K70-S70)))","v":3.3824696596338995},{"$f":"IF(H70=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q70-(K70-R70)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O70*80%-(K70-S70)),(Q70-(K70-S70)-(K70-T70))),(N70-(K70-S70))))","v":6.7649393192677989},{"$f":"IF(H70=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q70-(K70-R70)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O70*80%-(K70-S70)),(Q70-(K70-S70)-(K70-N70))),(N70-(K70-S70))))","v":6.7649393192677989},{"$f":"IF(H70=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q70-(K70-R70)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O70-(K70-S70)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N70-(K70-Q70)-(K70-S70)),(Q70-(K70-N70/80%)))))),(O70-(K70-S70))))","v":6.7649393192677989},1,null,null,{"$f":"IF(H70=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P70-(K70-R70),K70-(K70-O70)/I$6-(K70-R70)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K70-O70)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O70-(K70-S70),IF(OPFOKLEGHEN!$H$20=\"nee\",(O70-(K70-S70)),(O70-(K70-S70)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O70*80%-(K70-S70),0+O70-(K70-S70)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O70*80%-(K70-S70)),O70*93%-(K70-S70)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O70-(K70-S70))),O70-(K70-S70))))))))","v":3.3824696596338995},{"$f":"IF(H70=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q70-(K70-R70),N70-(K70-R70)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q70-(K70-N70)-(K70-S70),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q70-(K70-N70)-(K70-S70)),(O70-(K70-S70)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q70*$N$135-(K70-N70)-(K70-S70),(Q70-(K70-N70)-(K70-S70))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N70*95%-(K70-Q70)/I$4-(K70-S70)),N70-(K70-Q70)/I$4-(K70-S70)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N70-(K70-Q70)/I$4-(K70-S70))),N70-(K70-Q70)/I$4-(K70-S70))))))))","v":3.3824696596338995},0,0.5727785436199978,0,0,0.5727785436199978,0,0.67412908143144412,2.1236967041080419E-2,8,55,622.60000000000014,557.60000000000014,590.10000000000014,23.084202135456945]
[8,56,0.68730461394249998,{"$f":"MIN(C71,J$5)","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C71)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C71<$I$3,C71-D71,MIN($I$3,C71-D71))))","v":0},{"$f":"IF(C71<$I$7,MAX(0,C71-D71-E71-F71,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C71-D71-F71)),MIN(I$7,MAX(0,C71-D71-E71-F71))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C71-D71-E71-F71,MIN(I$7,C71-E71-F71)),MIN(I$7,MAX(0,C71-D71-F71))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C71-F71-G71,C71-D71-F71-G71),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C71-G71,IF(OPFOKLEGHEN!$J$18=\"nee\",C71-D71-G71)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C71-G71,C71-D71-F71-G71),C71-D71-F71-G71))","v":0.68730461394249998},0.68730461394249998,0.5834152262078357,3.5126196369165066,{"$f":"SUM(K$16:K71)/$K$137","v":9.0339542697030775E-2},2.2455102701749354E-2,3.5126196369165066,{"$f":"IF(E71<I$3,P71*(1-I$6*D71/C71),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P71*(1-$I$6)+(C71-D71)/C71*(K71-P71*(1-I$6)),P71*(1-$I$6)+(C71-D71)/C71*(K71-P71*(1-I$6))))","v":3.5126196369165066},3.5126196369165066,3.5126196369165066,3.5126196369165066,{"$f":"MIN(K71,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K71-(G71/(C71-G71))*(Q71)*95%,K71-(G71/(C71-G71))*(P71)*84%))","v":3.5126196369165066},3.5126196369165066,24.440552071795299,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H71/C71*K71,IF(OPFOKLEGHEN!$H$20=\"ja\",O71-(K71-Q71)-(K71-S71),Q71-(K71-O71)-(K71-S71)))","v":3.5126196369165066},{"$f":"IF(H71=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q71-(K71-R71)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O71*80%-(K71-S71)),(Q71-(K71-S71)-(K71-T71))),(N71-(K71-S71))))","v":7.0252392738330132},{"$f":"IF(H71=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q71-(K71-R71)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O71*80%-(K71-S71)),(Q71-(K71-S71)-(K71-N71))),(N71-(K71-S71))))","v":7.0252392738330132},{"$f":"IF(H71=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q71-(K71-R71)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O71-(K71-S71)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N71-(K71-Q71)-(K71-S71)),(Q71-(K71-N71/80%)))))),(O71-(K71-S71))))","v":7.0252392738330132},1,null,null,{"$f":"IF(H71=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P71-(K71-R71),K71-(K71-O71)/I$6-(K71-R71)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K71-O71)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O71-(K71-S71),IF(OPFOKLEGHEN!$H$20=\"nee\",(O71-(K71-S71)),(O71-(K71-S71)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O71*80%-(K71-S71),0+O71-(K71-S71)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O71*80%-(K71-S71)),O71*93%-(K71-S71)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O71-(K71-S71))),O71-(K71-S71))))))))","v":3.5126196369165066},{"$f":"IF(H71=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q71-(K71-R71),N71-(K71-R71)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q71-(K71-N71)-(K71-S71),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q71-(K71-N71)-(K71-S71)),(O71-(K71-S71)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q71*$N$135-(K71-N71)-(K71-S71),(Q71-(K71-N71)-(K71-S71))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N71*95%-(K71-Q71)/I$4-(K71-S71)),N71-(K71-Q71)/I$4-(K71-S71)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N71-(K71-Q71)/I$4-(K71-S71))),N71-(K71-Q71)/I$4-(K71-S71))))))))","v":3.5126196369165066},0,0.5834152262078357,0,0,0.5834152262078357,0,0.68730461394249998,2.2455102701749354E-2,8,56,635,570,602.5,24.440552071795299]
[9,57,0.69988931165274992,{"$f":"MIN(C72,J$5)","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C72)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C72<$I$3,C72-D72,MIN($I$3,C72-D72))))","v":0},{"$f":"IF(C72<$I$7,MAX(0,C72-D72-E72-F72,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C72-D72-F72)),MIN(I$7,MAX(0,C72-D72-E72-F72))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C72-D72-E72-F72,MIN(I$7,C72-E72-F72)),MIN(I$7,MAX(0,C72-D72-F72))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C72-F72-G72,C72-D72-F72-G72),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C72-G72,IF(OPFOKLEGHEN!$J$18=\"nee\",C72-D72-G72)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C72-G72,C72-D72-F72-G72),C72-D72-F72-G72))","v":0.69988931165274992},{"$f":"IF(C72-D72-E72<0, 0, C72-D72-E72)","v":0.69988931165274992},0.59424943542744912,3.6433613360074495,{"$f":"SUM(K$16:K72)/$K$137","v":9.4606064987381833E-2},2.3706803213747098E-2,3.6433613360074495,{"$f":"IF(E72<I$3,P72*(1-I$6*D72/C72),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P72*(1-$I$6)+(C72-D72)/C72*(K72-P72*(1-I$6)),P72*(1-$I$6)+(C72-D72)/C72*(K72-P72*(1-I$6))))","v":3.6433613360074495},3.6433613360074495,3.6433613360074495,3.6433613360074495,{"$f":"MIN(K72,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K72-(G72/(C72-G72))*(Q72)*95%,K72-(G72/(C72-G72))*(P72)*84%))","v":3.6433613360074495},3.6433613360074495,{"$f":"AR72","v":0},{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H72/C72*K72,IF(OPFOKLEGHEN!$H$20=\"ja\",O72-(K72-Q72)-(K72-S72),Q72-(K72-O72)-(K72-S72)))","v":3.6433613360074495},{"$f":"IF(H72=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q72-(K72-R72)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O72*80%-(K72-S72)),(Q72-(K72-S72)-(K72-T72))),(N72-(K72-S72))))","v":7.286722672014899},{"$f":"IF(H72=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q72-(K72-R72)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O72*80%-(K72-S72)),(Q72-(K72-S72)-(K72-N72))),(N72-(K72-S72))))","v":7.286722672014899},{"$f":"IF(H72=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q72-(K72-R72)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O72-(K72-S72)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N72-(K72-Q72)-(K72-S72)),(Q72-(K72-N72/80%)))))),(O72-(K72-S72))))","v":7.286722672014899},1,null,null,{"$f":"IF(H72=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P72-(K72-R72),K72-(K72-O72)/I$6-(K72-R72)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K72-O72)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O72-(K72-S72),IF(OPFOKLEGHEN!$H$20=\"nee\",(O72-(K72-S72)),(O72-(K72-S72)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O72*80%-(K72-S72),0+O72-(K72-S72)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O72*80%-(K72-S72)),O72*93%-(K72-S72)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O72-(K72-S72))),O72-(K72-S72))))))))","v":3.6433613360074495},{"$f":"IF(H72=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q72-(K72-R72),N72-(K72-R72)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q72-(K72-N72)-(K72-S72),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q72-(K72-N72)-(K72-S72)),(O72-(K72-S72)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q72*$N$135-(K72-N72)-(K72-S72),(Q72-(K72-N72)-(K72-S72))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N72*95%-(K72-Q72)/I$4-(K72-S72)),N72-(K72-Q72)/I$4-(K72-S72)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N72-(K72-Q72)/I$4-(K72-S72))),N72-(K72-Q72)/I$4-(K72-S72))))))))","v":3.6433613360074495},null,null,null,null,null,null,null,null,9,57,{"$f":"AO71+12.1","v":647.1},{"$f":"AP71+11.4","v":581.4},614.25]
[9,58,0.71257494740899985,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C73)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C73<$I$3,C73-D73,MIN($I$3,C73-D73))))","v":0},{"$f":"IF(C73<$I$7,MAX(0,C73-D73-E73-F73,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C73-D73-F73)),MIN(I$7,MAX(0,C73-D73-E73-F73))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C73-D73-E73-F73,MIN(I$7,C73-E73-F73)),MIN(I$7,MAX(0,C73-D73-F73))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C73-F73-G73,C73-D73-F73-G73),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C73-G73,IF(OPFOKLEGHEN!$J$18=\"nee\",C73-D73-G73)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C73-G73,C73-D73-F73-G73),C73-D73-F73-G73))","v":0.71257494740899985},0.71257494740899985,0.60528483941219946,3.7782827184777297,{"$f":"SUM(K$16:K73)/$K$137","v":9.903058562943777E-2},2.5016027131473551E-2,3.7782827184777297,{"$f":"IF(E73<I$3,P73*(1-I$6*D73/C73),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P73*(1-$I$6)+(C73-D73)/C73*(K73-P73*(1-I$6)),P73*(1-$I$6)+(C73-D73)/C73*(K73-P73*(1-I$6))))","v":3.7782827184777297},3.7782827184777297,3.7782827184777297,3.7782827184777297,{"$f":"MIN(K73,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K73-(G73/(C73-G73))*(Q73)*95%,K73-(G73/(C73-G73))*(P73)*84%))","v":3.7782827184777297},3.7782827184777297,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H73/C73*K73,IF(OPFOKLEGHEN!$H$20=\"ja\",O73-(K73-Q73)-(K73-S73),Q73-(K73-O73)-(K73-S73)))","v":3.7782827184777297},{"$f":"IF(H73=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q73-(K73-R73)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O73*80%-(K73-S73)),(Q73-(K73-S73)-(K73-T73))),(N73-(K73-S73))))","v":7.5565654369554593},{"$f":"IF(H73=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q73-(K73-R73)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O73*80%-(K73-S73)),(Q73-(K73-S73)-(K73-N73))),(N73-(K73-S73))))","v":7.5565654369554593},{"$f":"IF(H73=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q73-(K73-R73)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O73-(K73-S73)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N73-(K73-Q73)-(K73-S73)),(Q73-(K73-N73/80%)))))),(O73-(K73-S73))))","v":7.5565654369554593},1,null,null,{"$f":"IF(H73=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P73-(K73-R73),K73-(K73-O73)/I$6-(K73-R73)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K73-O73)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O73-(K73-S73),IF(OPFOKLEGHEN!$H$20=\"nee\",(O73-(K73-S73)),(O73-(K73-S73)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O73*80%-(K73-S73),0+O73-(K73-S73)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O73*80%-(K73-S73)),O73*93%-(K73-S73)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O73-(K73-S73))),O73-(K73-S73))))))))","v":3.7782827184777297},{"$f":"IF(H73=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q73-(K73-R73),N73-(K73-R73)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q73-(K73-N73)-(K73-S73),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q73-(K73-N73)-(K73-S73)),(O73-(K73-S73)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q73*$N$135-(K73-N73)-(K73-S73),(Q73-(K73-N73)-(K73-S73))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N73*95%-(K73-Q73)/I$4-(K73-S73)),N73-(K73-Q73)/I$4-(K73-S73)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N73-(K73-Q73)/I$4-(K73-S73))),N73-(K73-Q73)/I$4-(K73-S73))))))))","v":3.7782827184777297},null,null,null,null,null,null,null,null,9,58,659.2,592.79999999999995,626]
[9,59,0.72536525883924996,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C74)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C74<$I$3,C74-D74,MIN($I$3,C74-D74))))","v":0},{"$f":"IF(C74<$I$7,MAX(0,C74-D74-E74-F74,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C74-D74-F74)),MIN(I$7,MAX(0,C74-D74-E74-F74))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C74-D74-E74-F74,MIN(I$7,C74-E74-F74)),MIN(I$7,MAX(0,C74-D74-F74))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C74-F74-G74,C74-D74-F74-G74),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C74-G74,IF(OPFOKLEGHEN!$J$18=\"nee\",C74-D74-G74)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C74-G74,C74-D74-F74-G74),C74-D74-F74-G74))","v":0.72536525883924996},0.72536525883924996,0.61652517441387056,3.9175240582239672,{"$f":"SUM(K$16:K74)/$K$137","v":0.10361816346647856},2.6385150620458226E-2,3.9175240582239672,{"$f":"IF(E74<I$3,P74*(1-I$6*D74/C74),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P74*(1-$I$6)+(C74-D74)/C74*(K74-P74*(1-I$6)),P74*(1-$I$6)+(C74-D74)/C74*(K74-P74*(1-I$6))))","v":3.9175240582239672},3.9175240582239672,3.9175240582239672,3.9175240582239672,{"$f":"MIN(K74,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K74-(G74/(C74-G74))*(Q74)*95%,K74-(G74/(C74-G74))*(P74)*84%))","v":3.9175240582239672},3.9175240582239672,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H74/C74*K74,IF(OPFOKLEGHEN!$H$20=\"ja\",O74-(K74-Q74)-(K74-S74),Q74-(K74-O74)-(K74-S74)))","v":3.9175240582239672},{"$f":"IF(H74=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q74-(K74-R74)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O74*80%-(K74-S74)),(Q74-(K74-S74)-(K74-T74))),(N74-(K74-S74))))","v":7.8350481164479344},{"$f":"IF(H74=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q74-(K74-R74)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O74*80%-(K74-S74)),(Q74-(K74-S74)-(K74-N74))),(N74-(K74-S74))))","v":7.8350481164479344},{"$f":"IF(H74=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q74-(K74-R74)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O74-(K74-S74)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N74-(K74-Q74)-(K74-S74)),(Q74-(K74-N74/80%)))))),(O74-(K74-S74))))","v":7.8350481164479344},1,null,null,{"$f":"IF(H74=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P74-(K74-R74),K74-(K74-O74)/I$6-(K74-R74)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K74-O74)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O74-(K74-S74),IF(OPFOKLEGHEN!$H$20=\"nee\",(O74-(K74-S74)),(O74-(K74-S74)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O74*80%-(K74-S74),0+O74-(K74-S74)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O74*80%-(K74-S74)),O74*93%-(K74-S74)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O74-(K74-S74))),O74-(K74-S74))))))))","v":3.9175240582239672},{"$f":"IF(H74=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q74-(K74-R74),N74-(K74-R74)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q74-(K74-N74)-(K74-S74),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q74-(K74-N74)-(K74-S74)),(O74-(K74-S74)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q74*$N$135-(K74-N74)-(K74-S74),(Q74-(K74-N74)-(K74-S74))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N74*95%-(K74-Q74)/I$4-(K74-S74)),N74-(K74-Q74)/I$4-(K74-S74)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N74-(K74-Q74)/I$4-(K74-S74))),N74-(K74-Q74)/I$4-(K74-S74))))))))","v":3.9175240582239672},null,null,null,null,null,null,null,null,9,59,671.30000000000007,604.19999999999993,637.75]
[9,60,0.73826398357149992,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C75)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C75<$I$3,C75-D75,MIN($I$3,C75-D75))))","v":0},{"$f":"IF(C75<$I$7,MAX(0,C75-D75-E75-F75,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C75-D75-F75)),MIN(I$7,MAX(0,C75-D75-E75-F75))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C75-D75-E75-F75,MIN(I$7,C75-E75-F75)),MIN(I$7,MAX(0,C75-D75-F75))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C75-F75-G75,C75-D75-F75-G75),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C75-G75,IF(OPFOKLEGHEN!$J$18=\"nee\",C75-D75-G75)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C75-G75,C75-D75-F75-G75),C75-D75-F75-G75))","v":0.73826398357149992},0.73826398357149992,0.6279742460676484,4.0612303319041718,{"$f":"SUM(K$16:K75)/$K$137","v":0.10837402711526697},2.7816646108932683E-2,4.0612303319041718,{"$f":"IF(E75<I$3,P75*(1-I$6*D75/C75),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P75*(1-$I$6)+(C75-D75)/C75*(K75-P75*(1-I$6)),P75*(1-$I$6)+(C75-D75)/C75*(K75-P75*(1-I$6))))","v":4.0612303319041718},4.0612303319041718,4.0612303319041718,4.0612303319041718,{"$f":"MIN(K75,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K75-(G75/(C75-G75))*(Q75)*95%,K75-(G75/(C75-G75))*(P75)*84%))","v":4.0612303319041718},4.0612303319041718,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H75/C75*K75,IF(OPFOKLEGHEN!$H$20=\"ja\",O75-(K75-Q75)-(K75-S75),Q75-(K75-O75)-(K75-S75)))","v":4.0612303319041718},{"$f":"IF(H75=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q75-(K75-R75)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O75*80%-(K75-S75)),(Q75-(K75-S75)-(K75-T75))),(N75-(K75-S75))))","v":8.1224606638083436},{"$f":"IF(H75=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q75-(K75-R75)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O75*80%-(K75-S75)),(Q75-(K75-S75)-(K75-N75))),(N75-(K75-S75))))","v":8.1224606638083436},{"$f":"IF(H75=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q75-(K75-R75)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O75-(K75-S75)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N75-(K75-Q75)-(K75-S75)),(Q75-(K75-N75/80%)))))),(O75-(K75-S75))))","v":8.1224606638083436},1,null,null,{"$f":"IF(H75=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P75-(K75-R75),K75-(K75-O75)/I$6-(K75-R75)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K75-O75)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O75-(K75-S75),IF(OPFOKLEGHEN!$H$20=\"nee\",(O75-(K75-S75)),(O75-(K75-S75)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O75*80%-(K75-S75),0+O75-(K75-S75)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O75*80%-(K75-S75)),O75*93%-(K75-S75)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O75-(K75-S75))),O75-(K75-S75))))))))","v":4.0612303319041718},{"$f":"IF(H75=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q75-(K75-R75),N75-(K75-R75)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q75-(K75-N75)-(K75-S75),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q75-(K75-N75)-(K75-S75)),(O75-(K75-S75)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q75*$N$135-(K75-N75)-(K75-S75),(Q75-(K75-N75)-(K75-S75))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N75*95%-(K75-Q75)/I$4-(K75-S75)),N75-(K75-Q75)/I$4-(K75-S75)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N75-(K75-Q75)/I$4-(K75-S75))),N75-(K75-Q75)/I$4-(K75-S75))))))))","v":4.0612303319041718},null,null,null,null,null,null,null,null,9,60,683.40000000000009,615.59999999999991,649.5]
[9,61,0.75127485923374993,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C76)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C76<$I$3,C76-D76,MIN($I$3,C76-D76))))","v":0},{"$f":"IF(C76<$I$7,MAX(0,C76-D76-E76-F76,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C76-D76-F76)),MIN(I$7,MAX(0,C76-D76-E76-F76))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C76-D76-E76-F76,MIN(I$7,C76-E76-F76)),MIN(I$7,MAX(0,C76-D76-F76))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C76-F76-G76,C76-D76-F76-G76),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C76-G76,IF(OPFOKLEGHEN!$J$18=\"nee\",C76-D76-G76)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C76-G76,C76-D76-F76-G76),C76-D76-F76-G76))","v":0.75127485923374993},0.75127485923374993,0.63963593068059343,4.2095513695383042,{"$f":"SUM(K$16:K76)/$K$137","v":0.11330358064953008},2.9313086020757599E-2,4.2095513695383042,{"$f":"IF(E76<I$3,P76*(1-I$6*D76/C76),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P76*(1-$I$6)+(C76-D76)/C76*(K76-P76*(1-I$6)),P76*(1-$I$6)+(C76-D76)/C76*(K76-P76*(1-I$6))))","v":4.2095513695383042},4.2095513695383042,4.2095513695383042,4.2095513695383042,{"$f":"MIN(K76,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K76-(G76/(C76-G76))*(Q76)*95%,K76-(G76/(C76-G76))*(P76)*84%))","v":4.2095513695383042},4.2095513695383042,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H76/C76*K76,IF(OPFOKLEGHEN!$H$20=\"ja\",O76-(K76-Q76)-(K76-S76),Q76-(K76-O76)-(K76-S76)))","v":4.2095513695383042},{"$f":"IF(H76=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q76-(K76-R76)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O76*80%-(K76-S76)),(Q76-(K76-S76)-(K76-T76))),(N76-(K76-S76))))","v":8.4191027390766084},{"$f":"IF(H76=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q76-(K76-R76)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O76*80%-(K76-S76)),(Q76-(K76-S76)-(K76-N76))),(N76-(K76-S76))))","v":8.4191027390766084},{"$f":"IF(H76=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q76-(K76-R76)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O76-(K76-S76)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N76-(K76-Q76)-(K76-S76)),(Q76-(K76-N76/80%)))))),(O76-(K76-S76))))","v":8.4191027390766084},1,null,null,{"$f":"IF(H76=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P76-(K76-R76),K76-(K76-O76)/I$6-(K76-R76)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K76-O76)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O76-(K76-S76),IF(OPFOKLEGHEN!$H$20=\"nee\",(O76-(K76-S76)),(O76-(K76-S76)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O76*80%-(K76-S76),0+O76-(K76-S76)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O76*80%-(K76-S76)),O76*93%-(K76-S76)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O76-(K76-S76))),O76-(K76-S76))))))))","v":4.2095513695383042},{"$f":"IF(H76=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q76-(K76-R76),N76-(K76-R76)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q76-(K76-N76)-(K76-S76),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q76-(K76-N76)-(K76-S76)),(O76-(K76-S76)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q76*$N$135-(K76-N76)-(K76-S76),(Q76-(K76-N76)-(K76-S76))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N76*95%-(K76-Q76)/I$4-(K76-S76)),N76-(K76-Q76)/I$4-(K76-S76)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N76-(K76-Q76)/I$4-(K76-S76))),N76-(K76-Q76)/I$4-(K76-S76))))))))","v":4.2095513695383042},null,null,null,null,null,null,null,null,9,61,695.50000000000011,626.99999999999989,661.25]
[9,62,0.76440162345399987,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C77)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C77<$I$3,C77-D77,MIN($I$3,C77-D77))))","v":0},{"$f":"IF(C77<$I$7,MAX(0,C77-D77-E77-F77,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C77-D77-F77)),MIN(I$7,MAX(0,C77-D77-E77-F77))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C77-D77-E77-F77,MIN(I$7,C77-E77-F77)),MIN(I$7,MAX(0,C77-D77-F77))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C77-F77-G77,C77-D77-F77-G77),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C77-G77,IF(OPFOKLEGHEN!$J$18=\"nee\",C77-D77-G77)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C77-G77,C77-D77-F77-G77),C77-D77-F77-G77))","v":0.76440162345399987},0.76440162345399987,0.6515141765440412,4.3626420096611938,{"$f":"SUM(K$16:K77)/$K$137","v":0.1184124094651311},3.0877146643720776E-2,4.3626420096611938,{"$f":"IF(E77<I$3,P77*(1-I$6*D77/C77),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P77*(1-$I$6)+(C77-D77)/C77*(K77-P77*(1-I$6)),P77*(1-$I$6)+(C77-D77)/C77*(K77-P77*(1-I$6))))","v":4.3626420096611938},4.3626420096611938,4.3626420096611938,4.3626420096611938,{"$f":"MIN(K77,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K77-(G77/(C77-G77))*(Q77)*95%,K77-(G77/(C77-G77))*(P77)*84%))","v":4.3626420096611938},4.3626420096611938,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H77/C77*K77,IF(OPFOKLEGHEN!$H$20=\"ja\",O77-(K77-Q77)-(K77-S77),Q77-(K77-O77)-(K77-S77)))","v":4.3626420096611938},{"$f":"IF(H77=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q77-(K77-R77)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O77*80%-(K77-S77)),(Q77-(K77-S77)-(K77-T77))),(N77-(K77-S77))))","v":8.7252840193223875},{"$f":"IF(H77=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q77-(K77-R77)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O77*80%-(K77-S77)),(Q77-(K77-S77)-(K77-N77))),(N77-(K77-S77))))","v":8.7252840193223875},{"$f":"IF(H77=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q77-(K77-R77)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O77-(K77-S77)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N77-(K77-Q77)-(K77-S77)),(Q77-(K77-N77/80%)))))),(O77-(K77-S77))))","v":8.7252840193223875},1,null,null,{"$f":"IF(H77=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P77-(K77-R77),K77-(K77-O77)/I$6-(K77-R77)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K77-O77)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O77-(K77-S77),IF(OPFOKLEGHEN!$H$20=\"nee\",(O77-(K77-S77)),(O77-(K77-S77)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O77*80%-(K77-S77),0+O77-(K77-S77)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O77*80%-(K77-S77)),O77*93%-(K77-S77)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O77-(K77-S77))),O77-(K77-S77))))))))","v":4.3626420096611938},{"$f":"IF(H77=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q77-(K77-R77),N77-(K77-R77)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q77-(K77-N77)-(K77-S77),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q77-(K77-N77)-(K77-S77)),(O77-(K77-S77)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q77*$N$135-(K77-N77)-(K77-S77),(Q77-(K77-N77)-(K77-S77))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N77*95%-(K77-Q77)/I$4-(K77-S77)),N77-(K77-Q77)/I$4-(K77-S77)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N77-(K77-Q77)/I$4-(K77-S77))),N77-(K77-Q77)/I$4-(K77-S77))))))))","v":4.3626420096611938},null,null,null,null,null,null,null,null,9,62,707.60000000000014,638.39999999999986,673]
[9,63,0.77793117900999997,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C78)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C78<$I$3,C78-D78,MIN($I$3,C78-D78))))","v":0},{"$f":"IF(C78<$I$7,MAX(0,C78-D78-E78-F78,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C78-D78-F78)),MIN(I$7,MAX(0,C78-D78-E78-F78))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C78-D78-E78-F78,MIN(I$7,C78-E78-F78)),MIN(I$7,MAX(0,C78-D78-F78))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C78-F78-G78,C78-D78-F78-G78),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C78-G78,IF(OPFOKLEGHEN!$J$18=\"nee\",C78-D78-G78)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C78-G78,C78-D78-F78-G78),C78-D78-F78-G78))","v":0.77793117900999997},0.77793117900999997,0.66361300527037204,4.5223083689440244,{"$f":"SUM(K$16:K78)/$K$137","v":0.12370821399301377},3.2523450598570036E-2,4.5223083689440244,{"$f":"IF(E78<I$3,P78*(1-I$6*D78/C78),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P78*(1-$I$6)+(C78-D78)/C78*(K78-P78*(1-I$6)),P78*(1-$I$6)+(C78-D78)/C78*(K78-P78*(1-I$6))))","v":4.5223083689440244},4.5223083689440244,4.5223083689440244,4.5223083689440244,{"$f":"MIN(K78,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K78-(G78/(C78-G78))*(Q78)*95%,K78-(G78/(C78-G78))*(P78)*84%))","v":4.5223083689440244},4.5223083689440244,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H78/C78*K78,IF(OPFOKLEGHEN!$H$20=\"ja\",O78-(K78-Q78)-(K78-S78),Q78-(K78-O78)-(K78-S78)))","v":4.5223083689440244},{"$f":"IF(H78=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q78-(K78-R78)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O78*80%-(K78-S78)),(Q78-(K78-S78)-(K78-T78))),(N78-(K78-S78))))","v":9.0446167378880489},{"$f":"IF(H78=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q78-(K78-R78)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O78*80%-(K78-S78)),(Q78-(K78-S78)-(K78-N78))),(N78-(K78-S78))))","v":9.0446167378880489},{"$f":"IF(H78=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q78-(K78-R78)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O78-(K78-S78)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N78-(K78-Q78)-(K78-S78)),(Q78-(K78-N78/80%)))))),(O78-(K78-S78))))","v":9.0446167378880489},1,null,null,{"$f":"IF(H78=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P78-(K78-R78),K78-(K78-O78)/I$6-(K78-R78)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K78-O78)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O78-(K78-S78),IF(OPFOKLEGHEN!$H$20=\"nee\",(O78-(K78-S78)),(O78-(K78-S78)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O78*80%-(K78-S78),0+O78-(K78-S78)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O78*80%-(K78-S78)),O78*93%-(K78-S78)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O78-(K78-S78))),O78-(K78-S78))))))))","v":4.5223083689440244},{"$f":"IF(H78=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q78-(K78-R78),N78-(K78-R78)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q78-(K78-N78)-(K78-S78),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q78-(K78-N78)-(K78-S78)),(O78-(K78-S78)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q78*$N$135-(K78-N78)-(K78-S78),(Q78-(K78-N78)-(K78-S78))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N78*95%-(K78-Q78)/I$4-(K78-S78)),N78-(K78-Q78)/I$4-(K78-S78)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N78-(K78-Q78)/I$4-(K78-S78))),N78-(K78-Q78)/I$4-(K78-S78))))))))","v":4.5223083689440244},null,null,null,null,null,null,null,null,9,63,720,650,685]
[10,64,0.79170385806028398,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C79)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C79<$I$3,C79-D79,MIN($I$3,C79-D79))))","v":0},{"$f":"IF(C79<$I$7,MAX(0,C79-D79-E79-F79,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C79-D79-F79)),MIN(I$7,MAX(0,C79-D79-E79-F79))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C79-D79-E79-F79,MIN(I$7,C79-E79-F79)),MIN(I$7,MAX(0,C79-D79-F79))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C79-F79-G79,C79-D79-F79-G79),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C79-G79,IF(OPFOKLEGHEN!$J$18=\"nee\",C79-D79-G79)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C79-G79,C79-D79-F79-G79),C79-D79-F79-G79))","v":0.79170385806028398},0.79170385806028398,0.6759365131546079,4.6878399365504739,{"$f":"SUM(K$16:K79)/$K$137","v":0.12919786262742788},3.4249058897172412E-2,4.6878399365504739,{"$f":"IF(E79<I$3,P79*(1-I$6*D79/C79),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P79*(1-$I$6)+(C79-D79)/C79*(K79-P79*(1-I$6)),P79*(1-$I$6)+(C79-D79)/C79*(K79-P79*(1-I$6))))","v":4.6878399365504739},4.6878399365504739,4.6878399365504739,4.6878399365504739,{"$f":"MIN(K79,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K79-(G79/(C79-G79))*(Q79)*95%,K79-(G79/(C79-G79))*(P79)*84%))","v":4.6878399365504739},4.6878399365504739,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H79/C79*K79,IF(OPFOKLEGHEN!$H$20=\"ja\",O79-(K79-Q79)-(K79-S79),Q79-(K79-O79)-(K79-S79)))","v":4.6878399365504739},{"$f":"IF(H79=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q79-(K79-R79)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O79*80%-(K79-S79)),(Q79-(K79-S79)-(K79-T79))),(N79-(K79-S79))))","v":9.3756798731009479},{"$f":"IF(H79=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q79-(K79-R79)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O79*80%-(K79-S79)),(Q79-(K79-S79)-(K79-N79))),(N79-(K79-S79))))","v":9.3756798731009479},{"$f":"IF(H79=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q79-(K79-R79)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O79-(K79-S79)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N79-(K79-Q79)-(K79-S79)),(Q79-(K79-N79/80%)))))),(O79-(K79-S79))))","v":9.3756798731009479},1,null,null,{"$f":"IF(H79=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P79-(K79-R79),K79-(K79-O79)/I$6-(K79-R79)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K79-O79)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O79-(K79-S79),IF(OPFOKLEGHEN!$H$20=\"nee\",(O79-(K79-S79)),(O79-(K79-S79)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O79*80%-(K79-S79),0+O79-(K79-S79)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O79*80%-(K79-S79)),O79*93%-(K79-S79)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O79-(K79-S79))),O79-(K79-S79))))))))","v":4.6878399365504739},{"$f":"IF(H79=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q79-(K79-R79),N79-(K79-R79)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q79-(K79-N79)-(K79-S79),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q79-(K79-N79)-(K79-S79)),(O79-(K79-S79)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q79*$N$135-(K79-N79)-(K79-S79),(Q79-(K79-N79)-(K79-S79))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N79*95%-(K79-Q79)/I$4-(K79-S79)),N79-(K79-Q79)/I$4-(K79-S79)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N79-(K79-Q79)/I$4-(K79-S79))),N79-(K79-Q79)/I$4-(K79-S79))))))))","v":4.6878399365504739},null,null,null,null,null,null,null,null,10,64,{"$f":"AO78+12.1","v":732.1},{"$f":"AP78+12.1","v":662.1},697.1]
[10,65,0.80561152572503203,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C80)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C80<$I$3,C80-D80,MIN($I$3,C80-D80))))","v":0},{"$f":"IF(C80<$I$7,MAX(0,C80-D80-E80-F80,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C80-D80-F80)),MIN(I$7,MAX(0,C80-D80-E80-F80))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C80-D80-E80-F80,MIN(I$7,C80-E80-F80)),MIN(I$7,MAX(0,C80-D80-F80))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C80-F80-G80,C80-D80-F80-G80),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C80-G80,IF(OPFOKLEGHEN!$J$18=\"nee\",C80-D80-G80)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C80-G80,C80-D80-F80-G80),C80-D80-F80-G80))","v":0.80561152572503203},0.80561152572503203,0.68848887256129243,4.8587740425627759,{"$f":"SUM(K$16:K80)/$K$137","v":0.13488768195758802},3.6052547119472651E-2,{"$f":"(((($K80)*(1-($I$6*(D80)/C80)))))","v":4.8587740425627759},{"$f":"IF(E80<I$3,P80*(1-I$6*D80/C80),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P80*(1-$I$6)+(C80-D80)/C80*(K80-P80*(1-I$6)),P80*(1-$I$6)+(C80-D80)/C80*(K80-P80*(1-I$6))))","v":4.8587740425627759},{"$f":"IF(E80=0,K80,K80-K80*I$4*E80/C80)","v":4.8587740425627759},{"$f":"IF(F80=0,K80,K80-K80*I$4*F80/C80)","v":4.8587740425627759},{"$f":"K80-(G80/C80)*K80*97.25%","v":4.8587740425627759},{"$f":"MIN(K80,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K80-(G80/(C80-G80))*(Q80)*95%,K80-(G80/(C80-G80))*(P80)*84%))","v":4.8587740425627759},4.8587740425627759,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H80/C80*K80,IF(OPFOKLEGHEN!$H$20=\"ja\",O80-(K80-Q80)-(K80-S80),Q80-(K80-O80)-(K80-S80)))","v":4.8587740425627759},{"$f":"IF(H80=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q80-(K80-R80)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O80*80%-(K80-S80)),(Q80-(K80-S80)-(K80-T80))),(N80-(K80-S80))))","v":9.7175480851255518},{"$f":"IF(H80=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q80-(K80-R80)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O80*80%-(K80-S80)),(Q80-(K80-S80)-(K80-N80))),(N80-(K80-S80))))","v":9.7175480851255518},{"$f":"IF(H80=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q80-(K80-R80)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O80-(K80-S80)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N80-(K80-Q80)-(K80-S80)),(Q80-(K80-N80/80%)))))),(O80-(K80-S80))))","v":9.7175480851255518},{"$f":"Q80/K80","v":1},null,null,{"$f":"IF(H80=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P80-(K80-R80),K80-(K80-O80)/I$6-(K80-R80)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K80-O80)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O80-(K80-S80),IF(OPFOKLEGHEN!$H$20=\"nee\",(O80-(K80-S80)),(O80-(K80-S80)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O80*80%-(K80-S80),0+O80-(K80-S80)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O80*80%-(K80-S80)),O80*93%-(K80-S80)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O80-(K80-S80))),O80-(K80-S80))))))))","v":4.8587740425627759},{"$f":"IF(H80=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q80-(K80-R80),N80-(K80-R80)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q80-(K80-N80)-(K80-S80),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q80-(K80-N80)-(K80-S80)),(O80-(K80-S80)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q80*$N$135-(K80-N80)-(K80-S80),(Q80-(K80-N80)-(K80-S80))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N80*95%-(K80-Q80)/I$4-(K80-S80)),N80-(K80-Q80)/I$4-(K80-S80)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N80-(K80-Q80)/I$4-(K80-S80))),N80-(K80-Q80)/I$4-(K80-S80))))))))","v":4.8587740425627759},null,null,null,null,null,null,null,null,10,65,{"$f":"AO79+12.1","v":744.2},674.2,709.2]
[10,66,{"$f":"0.000000000384*AQ81^3-0.000000342064*AQ81^2+0.001060852819*AQ81+0.088327034395","v":0.81965826368078809},0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C81)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C81<$I$3,C81-D81,MIN($I$3,C81-D81))))","v":0},{"$f":"IF(C81<$I$7,MAX(0,C81-D81-E81-F81,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C81-D81-F81)),MIN(I$7,MAX(0,C81-D81-E81-F81))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C81-D81-E81-F81,MIN(I$7,C81-E81-F81)),MIN(I$7,MAX(0,C81-D81-F81))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C81-F81-G81,C81-D81-F81-G81),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C81-G81,IF(OPFOKLEGHEN!$J$18=\"nee\",C81-D81-G81)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C81-G81,C81-D81-F81-G81),C81-D81-F81-G81))","v":0.81965826368078809},0.81965826368078809,0.70127433333712652,{"$f":"(J81/1000)*C81*24*365","v":5.0352944492606193},{"$f":"SUM(K$16:K81)/$K$137","v":0.14078421376571049},{"$f":"(((($J81/1000)*(1-$I$8))*$B81*$C81))","v":3.7937149960182749E-2},5.0352944492606193,{"$f":"IF(E81<I$3,P81*(1-I$6*D81/C81),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P81*(1-$I$6)+(C81-D81)/C81*(K81-P81*(1-I$6)),P81*(1-$I$6)+(C81-D81)/C81*(K81-P81*(1-I$6))))","v":5.0352944492606193},5.0352944492606193,5.0352944492606193,5.0352944492606193,{"$f":"MIN(K81,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K81-(G81/(C81-G81))*(Q81)*95%,K81-(G81/(C81-G81))*(P81)*84%))","v":5.0352944492606193},5.0352944492606193,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H81/C81*K81,IF(OPFOKLEGHEN!$H$20=\"ja\",O81-(K81-Q81)-(K81-S81),Q81-(K81-O81)-(K81-S81)))","v":5.0352944492606193},{"$f":"IF(H81=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q81-(K81-R81)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O81*80%-(K81-S81)),(Q81-(K81-S81)-(K81-T81))),(N81-(K81-S81))))","v":10.070588898521239},{"$f":"IF(H81=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q81-(K81-R81)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O81*80%-(K81-S81)),(Q81-(K81-S81)-(K81-N81))),(N81-(K81-S81))))","v":10.070588898521239},{"$f":"IF(H81=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q81-(K81-R81)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O81-(K81-S81)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N81-(K81-Q81)-(K81-S81)),(Q81-(K81-N81/80%)))))),(O81-(K81-S81))))","v":10.070588898521239},1,null,null,{"$f":"IF(H81=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P81-(K81-R81),K81-(K81-O81)/I$6-(K81-R81)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K81-O81)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O81-(K81-S81),IF(OPFOKLEGHEN!$H$20=\"nee\",(O81-(K81-S81)),(O81-(K81-S81)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O81*80%-(K81-S81),0+O81-(K81-S81)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O81*80%-(K81-S81)),O81*93%-(K81-S81)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O81-(K81-S81))),O81-(K81-S81))))))))","v":5.0352944492606193},{"$f":"IF(H81=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q81-(K81-R81),N81-(K81-R81)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q81-(K81-N81)-(K81-S81),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q81-(K81-N81)-(K81-S81)),(O81-(K81-S81)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q81*$N$135-(K81-N81)-(K81-S81),(Q81-(K81-N81)-(K81-S81))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N81*95%-(K81-Q81)/I$4-(K81-S81)),N81-(K81-Q81)/I$4-(K81-S81)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N81-(K81-Q81)/I$4-(K81-S81))),N81-(K81-Q81)/I$4-(K81-S81))))))))","v":5.0352944492606193},null,null,null,null,null,null,null,null,10,66,756.30000000000007,686.30000000000007,{"$f":"(AO81+AP81)/2","v":721.30000000000007}]
[10,67,0.83384815360409603,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C82)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C82<$I$3,C82-D82,MIN($I$3,C82-D82))))","v":0},{"$f":"IF(C82<$I$7,MAX(0,C82-D82-E82-F82,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C82-D82-F82)),MIN(I$7,MAX(0,C82-D82-E82-F82))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C82-D82-E82-F82,MIN(I$7,C82-E82-F82)),MIN(I$7,MAX(0,C82-D82-F82))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C82-F82-G82,C82-D82-F82-G82),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C82-G82,IF(OPFOKLEGHEN!$J$18=\"nee\",C82-D82-G82)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C82-G82,C82-D82-F82-G82),C82-D82-F82-G82))","v":0.83384815360409603},0.83384815360409603,0.71429722424983755,5.2175910929116602,{"$f":"SUM(K$16:K82)/$K$137","v":0.14689422225700091},3.9906233244872281E-2,5.2175910929116602,{"$f":"IF(E82<I$3,P82*(1-I$6*D82/C82),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P82*(1-$I$6)+(C82-D82)/C82*(K82-P82*(1-I$6)),P82*(1-$I$6)+(C82-D82)/C82*(K82-P82*(1-I$6))))","v":5.2175910929116602},5.2175910929116602,5.2175910929116602,5.2175910929116602,{"$f":"MIN(K82,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K82-(G82/(C82-G82))*(Q82)*95%,K82-(G82/(C82-G82))*(P82)*84%))","v":5.2175910929116602},{"$f":"$K82*(1-($I$6*(D82)/C82))-($I$4*F82/C82)","v":5.2175910929116602},0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H82/C82*K82,IF(OPFOKLEGHEN!$H$20=\"ja\",O82-(K82-Q82)-(K82-S82),Q82-(K82-O82)-(K82-S82)))","v":5.2175910929116602},{"$f":"IF(H82=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q82-(K82-R82)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O82*80%-(K82-S82)),(Q82-(K82-S82)-(K82-T82))),(N82-(K82-S82))))","v":10.43518218582332},{"$f":"IF(H82=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q82-(K82-R82)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O82*80%-(K82-S82)),(Q82-(K82-S82)-(K82-N82))),(N82-(K82-S82))))","v":10.43518218582332},{"$f":"IF(H82=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q82-(K82-R82)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O82-(K82-S82)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N82-(K82-Q82)-(K82-S82)),(Q82-(K82-N82/80%)))))),(O82-(K82-S82))))","v":10.43518218582332},1,null,null,{"$f":"IF(H82=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P82-(K82-R82),K82-(K82-O82)/I$6-(K82-R82)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K82-O82)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O82-(K82-S82),IF(OPFOKLEGHEN!$H$20=\"nee\",(O82-(K82-S82)),(O82-(K82-S82)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O82*80%-(K82-S82),0+O82-(K82-S82)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O82*80%-(K82-S82)),O82*93%-(K82-S82)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O82-(K82-S82))),O82-(K82-S82))))))))","v":5.2175910929116602},{"$f":"IF(H82=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q82-(K82-R82),N82-(K82-R82)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q82-(K82-N82)-(K82-S82),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q82-(K82-N82)-(K82-S82)),(O82-(K82-S82)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q82*$N$135-(K82-N82)-(K82-S82),(Q82-(K82-N82)-(K82-S82))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N82*95%-(K82-Q82)/I$4-(K82-S82)),N82-(K82-Q82)/I$4-(K82-S82)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N82-(K82-Q82)/I$4-(K82-S82))),N82-(K82-Q82)/I$4-(K82-S82))))))))","v":5.2175910929116602},null,null,null,null,null,null,null,null,10,67,768.40000000000009,698.40000000000009,733.40000000000009]
[10,68,0.84818527717150016,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C83)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C83<$I$3,C83-D83,MIN($I$3,C83-D83))))","v":0},{"$f":"IF(C83<$I$7,MAX(0,C83-D83-E83-F83,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C83-D83-F83)),MIN(I$7,MAX(0,C83-D83-E83-F83))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C83-D83-E83-F83,MIN(I$7,C83-E83-F83)),MIN(I$7,MAX(0,C83-D83-F83))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C83-F83-G83,C83-D83-F83-G83),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C83-G83,IF(OPFOKLEGHEN!$J$18=\"nee\",C83-D83-G83)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C83-G83,C83-D83-F83-G83),C83-D83-F83-G83))","v":0.84818527717150016},0.84818527717150016,0.72756195445376759,5.4058602808607912,{"$f":"SUM(K$16:K83)/$K$137","v":0.1532247015204414},4.1963298983850893E-2,5.4058602808607912,{"$f":"IF(E83<I$3,P83*(1-I$6*D83/C83),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P83*(1-$I$6)+(C83-D83)/C83*(K83-P83*(1-I$6)),P83*(1-$I$6)+(C83-D83)/C83*(K83-P83*(1-I$6))))","v":5.4058602808607912},5.4058602808607912,5.4058602808607912,5.4058602808607912,{"$f":"MIN(K83,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K83-(G83/(C83-G83))*(Q83)*95%,K83-(G83/(C83-G83))*(P83)*84%))","v":5.4058602808607912},5.4058602808607912,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H83/C83*K83,IF(OPFOKLEGHEN!$H$20=\"ja\",O83-(K83-Q83)-(K83-S83),Q83-(K83-O83)-(K83-S83)))","v":5.4058602808607912},{"$f":"IF(H83=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q83-(K83-R83)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O83*80%-(K83-S83)),(Q83-(K83-S83)-(K83-T83))),(N83-(K83-S83))))","v":10.811720561721582},{"$f":"IF(H83=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q83-(K83-R83)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O83*80%-(K83-S83)),(Q83-(K83-S83)-(K83-N83))),(N83-(K83-S83))))","v":10.811720561721582},{"$f":"IF(H83=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q83-(K83-R83)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O83-(K83-S83)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N83-(K83-Q83)-(K83-S83)),(Q83-(K83-N83/80%)))))),(O83-(K83-S83))))","v":10.811720561721582},1,null,null,{"$f":"IF(H83=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P83-(K83-R83),K83-(K83-O83)/I$6-(K83-R83)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K83-O83)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O83-(K83-S83),IF(OPFOKLEGHEN!$H$20=\"nee\",(O83-(K83-S83)),(O83-(K83-S83)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O83*80%-(K83-S83),0+O83-(K83-S83)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O83*80%-(K83-S83)),O83*93%-(K83-S83)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O83-(K83-S83))),O83-(K83-S83))))))))","v":5.4058602808607912},{"$f":"IF(H83=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q83-(K83-R83),N83-(K83-R83)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q83-(K83-N83)-(K83-S83),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q83-(K83-N83)-(K83-S83)),(O83-(K83-S83)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q83*$N$135-(K83-N83)-(K83-S83),(Q83-(K83-N83)-(K83-S83))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N83*95%-(K83-Q83)/I$4-(K83-S83)),N83-(K83-Q83)/I$4-(K83-S83)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N83-(K83-Q83)/I$4-(K83-S83))),N83-(K83-Q83)/I$4-(K83-S83))))))))","v":5.4058602808607912},null,null,null,null,null,null,null,null,10,68,780.50000000000011,710.50000000000011,745.50000000000011]
[10,69,0.86267371605954413,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C84)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C84<$I$3,C84-D84,MIN($I$3,C84-D84))))","v":0},{"$f":"IF(C84<$I$7,MAX(0,C84-D84-E84-F84,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C84-D84-F84)),MIN(I$7,MAX(0,C84-D84-E84-F84))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C84-D84-E84-F84,MIN(I$7,C84-E84-F84)),MIN(I$7,MAX(0,C84-D84-F84))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C84-F84-G84,C84-D84-F84-G84),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C84-G84,IF(OPFOKLEGHEN!$J$18=\"nee\",C84-D84-G84)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C84-G84,C84-D84-F84-G84),C84-D84-F84-G84))","v":0.86267371605954413},0.86267371605954413,0.74107301498267952,5.6003048945494509,{"$f":"SUM(K$16:K84)/$K$137","v":0.15978288322732129},4.4111990607752526E-2,5.6003048945494509,{"$f":"IF(E84<I$3,P84*(1-I$6*D84/C84),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P84*(1-$I$6)+(C84-D84)/C84*(K84-P84*(1-I$6)),P84*(1-$I$6)+(C84-D84)/C84*(K84-P84*(1-I$6))))","v":5.6003048945494509},5.6003048945494509,5.6003048945494509,5.6003048945494509,{"$f":"MIN(K84,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K84-(G84/(C84-G84))*(Q84)*95%,K84-(G84/(C84-G84))*(P84)*84%))","v":5.6003048945494509},5.6003048945494509,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H84/C84*K84,IF(OPFOKLEGHEN!$H$20=\"ja\",O84-(K84-Q84)-(K84-S84),Q84-(K84-O84)-(K84-S84)))","v":5.6003048945494509},{"$f":"IF(H84=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q84-(K84-R84)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O84*80%-(K84-S84)),(Q84-(K84-S84)-(K84-T84))),(N84-(K84-S84))))","v":11.200609789098902},{"$f":"IF(H84=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q84-(K84-R84)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O84*80%-(K84-S84)),(Q84-(K84-S84)-(K84-N84))),(N84-(K84-S84))))","v":11.200609789098902},{"$f":"IF(H84=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q84-(K84-R84)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O84-(K84-S84)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N84-(K84-Q84)-(K84-S84)),(Q84-(K84-N84/80%)))))),(O84-(K84-S84))))","v":11.200609789098902},1,null,null,{"$f":"IF(H84=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P84-(K84-R84),K84-(K84-O84)/I$6-(K84-R84)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K84-O84)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O84-(K84-S84),IF(OPFOKLEGHEN!$H$20=\"nee\",(O84-(K84-S84)),(O84-(K84-S84)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O84*80%-(K84-S84),0+O84-(K84-S84)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O84*80%-(K84-S84)),O84*93%-(K84-S84)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O84-(K84-S84))),O84-(K84-S84))))))))","v":5.6003048945494509},{"$f":"IF(H84=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q84-(K84-R84),N84-(K84-R84)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q84-(K84-N84)-(K84-S84),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q84-(K84-N84)-(K84-S84)),(O84-(K84-S84)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q84*$N$135-(K84-N84)-(K84-S84),(Q84-(K84-N84)-(K84-S84))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N84*95%-(K84-Q84)/I$4-(K84-S84)),N84-(K84-Q84)/I$4-(K84-S84)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N84-(K84-Q84)/I$4-(K84-S84))),N84-(K84-Q84)/I$4-(K84-S84))))))))","v":5.6003048945494509},null,null,null,null,null,null,null,null,10,69,792.60000000000014,722.60000000000014,757.60000000000014]
[10,70,0.87768263142499992,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C85)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C85<$I$3,C85-D85,MIN($I$3,C85-D85))))","v":0},{"$f":"IF(C85<$I$7,MAX(0,C85-D85-E85-F85,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C85-D85-F85)),MIN(I$7,MAX(0,C85-D85-E85-F85))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C85-D85-E85-F85,MIN(I$7,C85-E85-F85)),MIN(I$7,MAX(0,C85-D85-F85))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C85-F85-G85,C85-D85-F85-G85),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C85-G85,IF(OPFOKLEGHEN!$J$18=\"nee\",C85-D85-G85)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C85-G85,C85-D85-F85-G85),C85-D85-F85-G85))","v":0.87768263142499992},0.87768263142499992,0.75483498027028362,5.8035486335512818,{"$f":"SUM(K$16:K85)/$K$137","v":0.1665790715063892},4.6375388624268224E-2,5.8035486335512818,{"$f":"IF(E85<I$3,P85*(1-I$6*D85/C85),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P85*(1-$I$6)+(C85-D85)/C85*(K85-P85*(1-I$6)),P85*(1-$I$6)+(C85-D85)/C85*(K85-P85*(1-I$6))))","v":5.8035486335512818},5.8035486335512818,5.8035486335512818,5.8035486335512818,{"$f":"MIN(K85,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K85-(G85/(C85-G85))*(Q85)*95%,K85-(G85/(C85-G85))*(P85)*84%))","v":5.8035486335512818},5.8035486335512818,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H85/C85*K85,IF(OPFOKLEGHEN!$H$20=\"ja\",O85-(K85-Q85)-(K85-S85),Q85-(K85-O85)-(K85-S85)))","v":5.8035486335512818},{"$f":"IF(H85=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q85-(K85-R85)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O85*80%-(K85-S85)),(Q85-(K85-S85)-(K85-T85))),(N85-(K85-S85))))","v":11.607097267102564},{"$f":"IF(H85=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q85-(K85-R85)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O85*80%-(K85-S85)),(Q85-(K85-S85)-(K85-N85))),(N85-(K85-S85))))","v":11.607097267102564},{"$f":"IF(H85=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q85-(K85-R85)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O85-(K85-S85)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N85-(K85-Q85)-(K85-S85)),(Q85-(K85-N85/80%)))))),(O85-(K85-S85))))","v":11.607097267102564},1,null,null,{"$f":"IF(H85=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P85-(K85-R85),K85-(K85-O85)/I$6-(K85-R85)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K85-O85)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O85-(K85-S85),IF(OPFOKLEGHEN!$H$20=\"nee\",(O85-(K85-S85)),(O85-(K85-S85)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O85*80%-(K85-S85),0+O85-(K85-S85)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O85*80%-(K85-S85)),O85*93%-(K85-S85)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O85-(K85-S85))),O85-(K85-S85))))))))","v":5.8035486335512818},{"$f":"IF(H85=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q85-(K85-R85),N85-(K85-R85)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q85-(K85-N85)-(K85-S85),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q85-(K85-N85)-(K85-S85)),(O85-(K85-S85)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q85*$N$135-(K85-N85)-(K85-S85),(Q85-(K85-N85)-(K85-S85))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N85*95%-(K85-Q85)/I$4-(K85-S85)),N85-(K85-Q85)/I$4-(K85-S85)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N85-(K85-Q85)/I$4-(K85-S85))),N85-(K85-Q85)/I$4-(K85-S85))))))))","v":5.8035486335512818},null,null,null,null,null,null,null,null,10,70,805,735,770]
[11,71,0.89119859286431791,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C86)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C86<$I$3,C86-D86,MIN($I$3,C86-D86))))","v":0},{"$f":"IF(C86<$I$7,MAX(0,C86-D86-E86-F86,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C86-D86-F86)),MIN(I$7,MAX(0,C86-D86-E86-F86))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C86-D86-E86-F86,MIN(I$7,C86-E86-F86)),MIN(I$7,MAX(0,C86-D86-F86))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C86-F86-G86,C86-D86-F86-G86),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C86-G86,IF(OPFOKLEGHEN!$J$18=\"nee\",C86-D86-G86)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C86-G86,C86-D86-F86-G86),C86-D86-F86-G86))","v":0.89119859286431791},0.89119859286431791,0.76885250969900243,6.0023544069322039,{"$f":"SUM(K$16:K86)/$K$137","v":0.1736080693218589},4.8649219508240471E-2,6.0023544069322039,{"$f":"IF(E86<I$3,P86*(1-I$6*D86/C86),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P86*(1-$I$6)+(C86-D86)/C86*(K86-P86*(1-I$6)),P86*(1-$I$6)+(C86-D86)/C86*(K86-P86*(1-I$6))))","v":6.0023544069322039},6.0023544069322039,6.0023544069322039,6.0023544069322039,{"$f":"MIN(K86,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K86-(G86/(C86-G86))*(Q86)*95%,K86-(G86/(C86-G86))*(P86)*84%))","v":6.0023544069322039},6.0023544069322039,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H86/C86*K86,IF(OPFOKLEGHEN!$H$20=\"ja\",O86-(K86-Q86)-(K86-S86),Q86-(K86-O86)-(K86-S86)))","v":6.0023544069322039},{"$f":"IF(H86=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q86-(K86-R86)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O86*80%-(K86-S86)),(Q86-(K86-S86)-(K86-T86))),(N86-(K86-S86))))","v":12.004708813864408},{"$f":"IF(H86=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q86-(K86-R86)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O86*80%-(K86-S86)),(Q86-(K86-S86)-(K86-N86))),(N86-(K86-S86))))","v":12.004708813864408},{"$f":"IF(H86=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q86-(K86-R86)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O86-(K86-S86)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N86-(K86-Q86)-(K86-S86)),(Q86-(K86-N86/80%)))))),(O86-(K86-S86))))","v":12.004708813864408},1,null,null,{"$f":"IF(H86=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P86-(K86-R86),K86-(K86-O86)/I$6-(K86-R86)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K86-O86)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O86-(K86-S86),IF(OPFOKLEGHEN!$H$20=\"nee\",(O86-(K86-S86)),(O86-(K86-S86)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O86*80%-(K86-S86),0+O86-(K86-S86)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O86*80%-(K86-S86)),O86*93%-(K86-S86)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O86-(K86-S86))),O86-(K86-S86))))))))","v":6.0023544069322039},{"$f":"IF(H86=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q86-(K86-R86),N86-(K86-R86)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q86-(K86-N86)-(K86-S86),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q86-(K86-N86)-(K86-S86)),(O86-(K86-S86)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q86*$N$135-(K86-N86)-(K86-S86),(Q86-(K86-N86)-(K86-S86))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N86*95%-(K86-Q86)/I$4-(K86-S86)),N86-(K86-Q86)/I$4-(K86-S86)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N86-(K86-Q86)/I$4-(K86-S86))),N86-(K86-Q86)/I$4-(K86-S86))))))))","v":6.0023544069322039},null,null,null,null,null,null,null,null,11,71,{"$f":"AO85+12.1","v":817.1},{"$f":"AP85+10","v":745},781.05]
[11,72,0.90485074879968397,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C87)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C87<$I$3,C87-D87,MIN($I$3,C87-D87))))","v":0},{"$f":"IF(C87<$I$7,MAX(0,C87-D87-E87-F87,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C87-D87-F87)),MIN(I$7,MAX(0,C87-D87-E87-F87))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C87-D87-E87-F87,MIN(I$7,C87-E87-F87)),MIN(I$7,MAX(0,C87-D87-F87))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C87-F87-G87,C87-D87-F87-G87),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C87-G87,IF(OPFOKLEGHEN!$J$18=\"nee\",C87-D87-G87)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C87-G87,C87-D87-F87-G87),C87-D87-F87-G87))","v":0.90485074879968397},0.90485074879968397,0.78313034917749469,6.2074768858624836,{"$f":"SUM(K$16:K87)/$K$137","v":0.18087727378934498},5.102035796599301E-2,6.2074768858624836,{"$f":"IF(E87<I$3,P87*(1-I$6*D87/C87),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P87*(1-$I$6)+(C87-D87)/C87*(K87-P87*(1-I$6)),P87*(1-$I$6)+(C87-D87)/C87*(K87-P87*(1-I$6))))","v":6.2074768858624836},6.2074768858624836,6.2074768858624836,6.2074768858624836,{"$f":"MIN(K87,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K87-(G87/(C87-G87))*(Q87)*95%,K87-(G87/(C87-G87))*(P87)*84%))","v":6.2074768858624836},6.2074768858624836,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H87/C87*K87,IF(OPFOKLEGHEN!$H$20=\"ja\",O87-(K87-Q87)-(K87-S87),Q87-(K87-O87)-(K87-S87)))","v":6.2074768858624836},{"$f":"IF(H87=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q87-(K87-R87)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O87*80%-(K87-S87)),(Q87-(K87-S87)-(K87-T87))),(N87-(K87-S87))))","v":12.414953771724967},{"$f":"IF(H87=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q87-(K87-R87)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O87*80%-(K87-S87)),(Q87-(K87-S87)-(K87-N87))),(N87-(K87-S87))))","v":12.414953771724967},{"$f":"IF(H87=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q87-(K87-R87)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O87-(K87-S87)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N87-(K87-Q87)-(K87-S87)),(Q87-(K87-N87/80%)))))),(O87-(K87-S87))))","v":12.414953771724967},1,null,null,{"$f":"IF(H87=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P87-(K87-R87),K87-(K87-O87)/I$6-(K87-R87)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K87-O87)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O87-(K87-S87),IF(OPFOKLEGHEN!$H$20=\"nee\",(O87-(K87-S87)),(O87-(K87-S87)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O87*80%-(K87-S87),0+O87-(K87-S87)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O87*80%-(K87-S87)),O87*93%-(K87-S87)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O87-(K87-S87))),O87-(K87-S87))))))))","v":6.2074768858624836},{"$f":"IF(H87=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q87-(K87-R87),N87-(K87-R87)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q87-(K87-N87)-(K87-S87),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q87-(K87-N87)-(K87-S87)),(O87-(K87-S87)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q87*$N$135-(K87-N87)-(K87-S87),(Q87-(K87-N87)-(K87-S87))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N87*95%-(K87-Q87)/I$4-(K87-S87)),N87-(K87-Q87)/I$4-(K87-S87)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N87-(K87-Q87)/I$4-(K87-S87))),N87-(K87-Q87)/I$4-(K87-S87))))))))","v":6.2074768858624836},null,null,null,null,null,null,null,null,11,72,829.2,755,792.1]
[11,73,0.91864220786306616,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C88)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C88<$I$3,C88-D88,MIN($I$3,C88-D88))))","v":0},{"$f":"IF(C88<$I$7,MAX(0,C88-D88-E88-F88,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C88-D88-F88)),MIN(I$7,MAX(0,C88-D88-E88-F88))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C88-D88-E88-F88,MIN(I$7,C88-E88-F88)),MIN(I$7,MAX(0,C88-D88-F88))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C88-F88-G88,C88-D88-F88-G88),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C88-G88,IF(OPFOKLEGHEN!$J$18=\"nee\",C88-D88-G88)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C88-G88,C88-D88-F88-G88),C88-D88-F88-G88))","v":0.91864220786306616},0.91864220786306616,0.79767333274747643,6.419121189966015,{"$f":"SUM(K$16:K88)/$K$137","v":0.18839432222777053},5.3492676583050132E-2,6.419121189966015,{"$f":"IF(E88<I$3,P88*(1-I$6*D88/C88),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P88*(1-$I$6)+(C88-D88)/C88*(K88-P88*(1-I$6)),P88*(1-$I$6)+(C88-D88)/C88*(K88-P88*(1-I$6))))","v":6.419121189966015},6.419121189966015,6.419121189966015,6.419121189966015,{"$f":"MIN(K88,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K88-(G88/(C88-G88))*(Q88)*95%,K88-(G88/(C88-G88))*(P88)*84%))","v":6.419121189966015},6.419121189966015,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H88/C88*K88,IF(OPFOKLEGHEN!$H$20=\"ja\",O88-(K88-Q88)-(K88-S88),Q88-(K88-O88)-(K88-S88)))","v":6.419121189966015},{"$f":"IF(H88=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q88-(K88-R88)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O88*80%-(K88-S88)),(Q88-(K88-S88)-(K88-T88))),(N88-(K88-S88))))","v":12.83824237993203},{"$f":"IF(H88=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q88-(K88-R88)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O88*80%-(K88-S88)),(Q88-(K88-S88)-(K88-N88))),(N88-(K88-S88))))","v":12.83824237993203},{"$f":"IF(H88=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q88-(K88-R88)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O88-(K88-S88)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N88-(K88-Q88)-(K88-S88)),(Q88-(K88-N88/80%)))))),(O88-(K88-S88))))","v":12.83824237993203},1,null,null,{"$f":"IF(H88=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P88-(K88-R88),K88-(K88-O88)/I$6-(K88-R88)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K88-O88)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O88-(K88-S88),IF(OPFOKLEGHEN!$H$20=\"nee\",(O88-(K88-S88)),(O88-(K88-S88)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O88*80%-(K88-S88),0+O88-(K88-S88)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O88*80%-(K88-S88)),O88*93%-(K88-S88)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O88-(K88-S88))),O88-(K88-S88))))))))","v":6.419121189966015},{"$f":"IF(H88=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q88-(K88-R88),N88-(K88-R88)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q88-(K88-N88)-(K88-S88),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q88-(K88-N88)-(K88-S88)),(O88-(K88-S88)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q88*$N$135-(K88-N88)-(K88-S88),(Q88-(K88-N88)-(K88-S88))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N88*95%-(K88-Q88)/I$4-(K88-S88)),N88-(K88-Q88)/I$4-(K88-S88)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N88-(K88-Q88)/I$4-(K88-S88))),N88-(K88-Q88)/I$4-(K88-S88))))))))","v":6.419121189966015},null,null,null,null,null,null,null,null,11,73,841.30000000000007,765,803.15000000000009]
[11,74,0.932576078686432,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C89)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C89<$I$3,C89-D89,MIN($I$3,C89-D89))))","v":0},{"$f":"IF(C89<$I$7,MAX(0,C89-D89-E89-F89,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C89-D89-F89)),MIN(I$7,MAX(0,C89-D89-E89-F89))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C89-D89-E89-F89,MIN(I$7,C89-E89-F89)),MIN(I$7,MAX(0,C89-D89-F89))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C89-F89-G89,C89-D89-F89-G89),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C89-G89,IF(OPFOKLEGHEN!$J$18=\"nee\",C89-D89-G89)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C89-G89,C89-D89-F89-G89),C89-D89-F89-G89))","v":0.932576078686432},0.932576078686432,0.81248638422038,6.6374990077574711,{"$f":"SUM(K$16:K89)/$K$137","v":0.19616709985180208},5.6070197097494619E-2,6.6374990077574711,{"$f":"IF(E89<I$3,P89*(1-I$6*D89/C89),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P89*(1-$I$6)+(C89-D89)/C89*(K89-P89*(1-I$6)),P89*(1-$I$6)+(C89-D89)/C89*(K89-P89*(1-I$6))))","v":6.6374990077574711},6.6374990077574711,6.6374990077574711,6.6374990077574711,{"$f":"MIN(K89,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K89-(G89/(C89-G89))*(Q89)*95%,K89-(G89/(C89-G89))*(P89)*84%))","v":6.6374990077574711},6.6374990077574711,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H89/C89*K89,IF(OPFOKLEGHEN!$H$20=\"ja\",O89-(K89-Q89)-(K89-S89),Q89-(K89-O89)-(K89-S89)))","v":6.6374990077574711},{"$f":"IF(H89=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q89-(K89-R89)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O89*80%-(K89-S89)),(Q89-(K89-S89)-(K89-T89))),(N89-(K89-S89))))","v":13.274998015514942},{"$f":"IF(H89=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q89-(K89-R89)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O89*80%-(K89-S89)),(Q89-(K89-S89)-(K89-N89))),(N89-(K89-S89))))","v":13.274998015514942},{"$f":"IF(H89=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q89-(K89-R89)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O89-(K89-S89)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N89-(K89-Q89)-(K89-S89)),(Q89-(K89-N89/80%)))))),(O89-(K89-S89))))","v":13.274998015514942},1,null,null,{"$f":"IF(H89=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P89-(K89-R89),K89-(K89-O89)/I$6-(K89-R89)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K89-O89)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O89-(K89-S89),IF(OPFOKLEGHEN!$H$20=\"nee\",(O89-(K89-S89)),(O89-(K89-S89)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O89*80%-(K89-S89),0+O89-(K89-S89)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O89*80%-(K89-S89)),O89*93%-(K89-S89)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O89-(K89-S89))),O89-(K89-S89))))))))","v":6.6374990077574711},{"$f":"IF(H89=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q89-(K89-R89),N89-(K89-R89)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q89-(K89-N89)-(K89-S89),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q89-(K89-N89)-(K89-S89)),(O89-(K89-S89)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q89*$N$135-(K89-N89)-(K89-S89),(Q89-(K89-N89)-(K89-S89))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N89*95%-(K89-Q89)/I$4-(K89-S89)),N89-(K89-Q89)/I$4-(K89-S89)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N89-(K89-Q89)/I$4-(K89-S89))),N89-(K89-Q89)/I$4-(K89-S89))))))))","v":6.6374990077574711},null,null,null,null,null,null,null,null,11,74,853.40000000000009,775,814.2]
[11,75,0.94665546990174987,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C90)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C90<$I$3,C90-D90,MIN($I$3,C90-D90))))","v":0},{"$f":"IF(C90<$I$7,MAX(0,C90-D90-E90-F90,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C90-D90-F90)),MIN(I$7,MAX(0,C90-D90-E90-F90))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C90-D90-E90-F90,MIN(I$7,C90-E90-F90)),MIN(I$7,MAX(0,C90-D90-F90))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C90-F90-G90,C90-D90-F90-G90),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C90-G90,IF(OPFOKLEGHEN!$J$18=\"nee\",C90-D90-G90)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C90-G90,C90-D90-F90-G90),C90-D90-F90-G90))","v":0.94665546990174987},0.94665546990174987,0.82757451884440647,6.8628287983346077,{"$f":"SUM(K$16:K90)/$K$137","v":0.20420374770047378},5.8757095876152458E-2,6.8628287983346077,{"$f":"IF(E90<I$3,P90*(1-I$6*D90/C90),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P90*(1-$I$6)+(C90-D90)/C90*(K90-P90*(1-I$6)),P90*(1-$I$6)+(C90-D90)/C90*(K90-P90*(1-I$6))))","v":6.8628287983346077},6.8628287983346077,6.8628287983346077,6.8628287983346077,{"$f":"MIN(K90,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K90-(G90/(C90-G90))*(Q90)*95%,K90-(G90/(C90-G90))*(P90)*84%))","v":6.8628287983346077},6.8628287983346077,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H90/C90*K90,IF(OPFOKLEGHEN!$H$20=\"ja\",O90-(K90-Q90)-(K90-S90),Q90-(K90-O90)-(K90-S90)))","v":6.8628287983346077},{"$f":"IF(H90=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q90-(K90-R90)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O90*80%-(K90-S90)),(Q90-(K90-S90)-(K90-T90))),(N90-(K90-S90))))","v":13.725657596669215},{"$f":"IF(H90=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q90-(K90-R90)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O90*80%-(K90-S90)),(Q90-(K90-S90)-(K90-N90))),(N90-(K90-S90))))","v":13.725657596669215},{"$f":"IF(H90=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q90-(K90-R90)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O90-(K90-S90)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N90-(K90-Q90)-(K90-S90)),(Q90-(K90-N90/80%)))))),(O90-(K90-S90))))","v":13.725657596669215},1,null,null,{"$f":"IF(H90=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P90-(K90-R90),K90-(K90-O90)/I$6-(K90-R90)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K90-O90)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O90-(K90-S90),IF(OPFOKLEGHEN!$H$20=\"nee\",(O90-(K90-S90)),(O90-(K90-S90)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O90*80%-(K90-S90),0+O90-(K90-S90)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O90*80%-(K90-S90)),O90*93%-(K90-S90)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O90-(K90-S90))),O90-(K90-S90))))))))","v":6.8628287983346077},{"$f":"IF(H90=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q90-(K90-R90),N90-(K90-R90)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q90-(K90-N90)-(K90-S90),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q90-(K90-N90)-(K90-S90)),(O90-(K90-S90)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q90*$N$135-(K90-N90)-(K90-S90),(Q90-(K90-N90)-(K90-S90))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N90*95%-(K90-Q90)/I$4-(K90-S90)),N90-(K90-Q90)/I$4-(K90-S90)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N90-(K90-Q90)/I$4-(K90-S90))),N90-(K90-Q90)/I$4-(K90-S90))))))))","v":6.8628287983346077},null,null,null,null,null,null,null,null,11,75,865.50000000000011,785,825.25]
[11,76,0.96088349014098806,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C91)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C91<$I$3,C91-D91,MIN($I$3,C91-D91))))","v":0},{"$f":"IF(C91<$I$7,MAX(0,C91-D91-E91-F91,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C91-D91-F91)),MIN(I$7,MAX(0,C91-D91-E91-F91))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C91-D91-E91-F91,MIN(I$7,C91-E91-F91)),MIN(I$7,MAX(0,C91-D91-F91))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C91-F91-G91,C91-D91-F91-G91),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C91-G91,IF(OPFOKLEGHEN!$J$18=\"nee\",C91-D91-G91)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C91-G91,C91-D91-F91-G91),C91-D91-F91-G91))","v":0.96088349014098806},0.96088349014098806,0.84294284500253636,7.095335998963801,{"$f":"SUM(K$16:K91)/$K$137","v":0.21251267080890288},6.1557709580051238E-2,7.095335998963801,{"$f":"IF(E91<I$3,P91*(1-I$6*D91/C91),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P91*(1-$I$6)+(C91-D91)/C91*(K91-P91*(1-I$6)),P91*(1-$I$6)+(C91-D91)/C91*(K91-P91*(1-I$6))))","v":7.095335998963801},7.095335998963801,7.095335998963801,7.095335998963801,{"$f":"MIN(K91,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K91-(G91/(C91-G91))*(Q91)*95%,K91-(G91/(C91-G91))*(P91)*84%))","v":7.095335998963801},7.095335998963801,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H91/C91*K91,IF(OPFOKLEGHEN!$H$20=\"ja\",O91-(K91-Q91)-(K91-S91),Q91-(K91-O91)-(K91-S91)))","v":7.095335998963801},{"$f":"IF(H91=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q91-(K91-R91)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O91*80%-(K91-S91)),(Q91-(K91-S91)-(K91-T91))),(N91-(K91-S91))))","v":14.190671997927602},{"$f":"IF(H91=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q91-(K91-R91)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O91*80%-(K91-S91)),(Q91-(K91-S91)-(K91-N91))),(N91-(K91-S91))))","v":14.190671997927602},{"$f":"IF(H91=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q91-(K91-R91)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O91-(K91-S91)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N91-(K91-Q91)-(K91-S91)),(Q91-(K91-N91/80%)))))),(O91-(K91-S91))))","v":14.190671997927602},1,null,null,{"$f":"IF(H91=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P91-(K91-R91),K91-(K91-O91)/I$6-(K91-R91)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K91-O91)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O91-(K91-S91),IF(OPFOKLEGHEN!$H$20=\"nee\",(O91-(K91-S91)),(O91-(K91-S91)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O91*80%-(K91-S91),0+O91-(K91-S91)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O91*80%-(K91-S91)),O91*93%-(K91-S91)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O91-(K91-S91))),O91-(K91-S91))))))))","v":7.095335998963801},{"$f":"IF(H91=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q91-(K91-R91),N91-(K91-R91)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q91-(K91-N91)-(K91-S91),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q91-(K91-N91)-(K91-S91)),(O91-(K91-S91)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q91*$N$135-(K91-N91)-(K91-S91),(Q91-(K91-N91)-(K91-S91))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N91*95%-(K91-Q91)/I$4-(K91-S91)),N91-(K91-Q91)/I$4-(K91-S91)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N91-(K91-Q91)/I$4-(K91-S91))),N91-(K91-Q91)/I$4-(K91-S91))))))))","v":7.095335998963801},null,null,null,null,null,null,null,null,11,76,877.60000000000014,795,836.30000000000007]
[11,77,0.97545950659749991,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C92)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C92<$I$3,C92-D92,MIN($I$3,C92-D92))))","v":0},{"$f":"IF(C92<$I$7,MAX(0,C92-D92-E92-F92,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C92-D92-F92)),MIN(I$7,MAX(0,C92-D92-E92-F92))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C92-D92-E92-F92,MIN(I$7,C92-E92-F92)),MIN(I$7,MAX(0,C92-D92-F92))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C92-F92-G92,C92-D92-F92-G92),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C92-G92,IF(OPFOKLEGHEN!$J$18=\"nee\",C92-D92-G92)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C92-G92,C92-D92-F92-G92),C92-D92-F92-G92))","v":0.97545950659749991},0.97545950659749991,0.8585965659420719,7.3367293594022129,{"$f":"SUM(K$16:K92)/$K$137","v":0.22110427522672468},6.4489516058672425E-2,7.3367293594022129,{"$f":"IF(E92<I$3,P92*(1-I$6*D92/C92),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P92*(1-$I$6)+(C92-D92)/C92*(K92-P92*(1-I$6)),P92*(1-$I$6)+(C92-D92)/C92*(K92-P92*(1-I$6))))","v":7.3367293594022129},7.3367293594022129,7.3367293594022129,7.3367293594022129,{"$f":"MIN(K92,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K92-(G92/(C92-G92))*(Q92)*95%,K92-(G92/(C92-G92))*(P92)*84%))","v":7.3367293594022129},7.3367293594022129,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H92/C92*K92,IF(OPFOKLEGHEN!$H$20=\"ja\",O92-(K92-Q92)-(K92-S92),Q92-(K92-O92)-(K92-S92)))","v":7.3367293594022129},{"$f":"IF(H92=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q92-(K92-R92)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O92*80%-(K92-S92)),(Q92-(K92-S92)-(K92-T92))),(N92-(K92-S92))))","v":14.673458718804426},{"$f":"IF(H92=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q92-(K92-R92)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O92*80%-(K92-S92)),(Q92-(K92-S92)-(K92-N92))),(N92-(K92-S92))))","v":14.673458718804426},{"$f":"IF(H92=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q92-(K92-R92)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O92-(K92-S92)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N92-(K92-Q92)-(K92-S92)),(Q92-(K92-N92/80%)))))),(O92-(K92-S92))))","v":14.673458718804426},1,null,null,{"$f":"IF(H92=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P92-(K92-R92),K92-(K92-O92)/I$6-(K92-R92)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K92-O92)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O92-(K92-S92),IF(OPFOKLEGHEN!$H$20=\"nee\",(O92-(K92-S92)),(O92-(K92-S92)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O92*80%-(K92-S92),0+O92-(K92-S92)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O92*80%-(K92-S92)),O92*93%-(K92-S92)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O92-(K92-S92))),O92-(K92-S92))))))))","v":7.3367293594022129},{"$f":"IF(H92=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q92-(K92-R92),N92-(K92-R92)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q92-(K92-N92)-(K92-S92),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q92-(K92-N92)-(K92-S92)),(O92-(K92-S92)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q92*$N$135-(K92-N92)-(K92-S92),(Q92-(K92-N92)-(K92-S92))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N92*95%-(K92-Q92)/I$4-(K92-S92)),N92-(K92-Q92)/I$4-(K92-S92)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N92-(K92-Q92)/I$4-(K92-S92))),N92-(K92-Q92)/I$4-(K92-S92))))))))","v":7.3367293594022129},null,null,null,null,null,null,null,null,11,77,890,805,847.5]
[12,78,{"$f":"0.000000000384*AQ93^3-0.000000342064*AQ93^2+0.001060852819*AQ93+0.088327034395","v":0.98999623415201787},0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C93)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C93<$I$3,C93-D93,MIN($I$3,C93-D93))))","v":0},{"$f":"IF(C93<$I$7,MAX(0,C93-D93-E93-F93,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C93-D93-F93)),MIN(I$7,MAX(0,C93-D93-E93-F93))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C93-D93-E93-F93,MIN(I$7,C93-E93-F93)),MIN(I$7,MAX(0,C93-D93-F93))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C93-F93-G93,C93-D93-F93-G93),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C93-G93,IF(OPFOKLEGHEN!$J$18=\"nee\",C93-D93-G93)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C93-G93,C93-D93-F93-G93),C93-D93-F93-G93))","v":0.98999623415201787},0.98999623415201787,0.87454098153629933,7.584340358193101,{"$f":"SUM(K$16:K93)/$K$137","v":0.22998584205789166},6.7531797709938571E-2,7.584340358193101,{"$f":"IF(E93<I$3,P93*(1-I$6*D93/C93),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P93*(1-$I$6)+(C93-D93)/C93*(K93-P93*(1-I$6)),P93*(1-$I$6)+(C93-D93)/C93*(K93-P93*(1-I$6))))","v":7.584340358193101},7.584340358193101,7.584340358193101,7.584340358193101,{"$f":"MIN(K93,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K93-(G93/(C93-G93))*(Q93)*95%,K93-(G93/(C93-G93))*(P93)*84%))","v":7.584340358193101},7.584340358193101,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H93/C93*K93,IF(OPFOKLEGHEN!$H$20=\"ja\",O93-(K93-Q93)-(K93-S93),Q93-(K93-O93)-(K93-S93)))","v":7.584340358193101},{"$f":"IF(H93=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q93-(K93-R93)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O93*80%-(K93-S93)),(Q93-(K93-S93)-(K93-T93))),(N93-(K93-S93))))","v":15.168680716386202},{"$f":"IF(H93=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q93-(K93-R93)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O93*80%-(K93-S93)),(Q93-(K93-S93)-(K93-N93))),(N93-(K93-S93))))","v":15.168680716386202},{"$f":"IF(H93=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q93-(K93-R93)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O93-(K93-S93)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N93-(K93-Q93)-(K93-S93)),(Q93-(K93-N93/80%)))))),(O93-(K93-S93))))","v":15.168680716386202},1,null,null,{"$f":"IF(H93=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P93-(K93-R93),K93-(K93-O93)/I$6-(K93-R93)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K93-O93)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O93-(K93-S93),IF(OPFOKLEGHEN!$H$20=\"nee\",(O93-(K93-S93)),(O93-(K93-S93)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O93*80%-(K93-S93),0+O93-(K93-S93)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O93*80%-(K93-S93)),O93*93%-(K93-S93)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O93-(K93-S93))),O93-(K93-S93))))))))","v":7.584340358193101},{"$f":"IF(H93=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q93-(K93-R93),N93-(K93-R93)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q93-(K93-N93)-(K93-S93),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q93-(K93-N93)-(K93-S93)),(O93-(K93-S93)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q93*$N$135-(K93-N93)-(K93-S93),(Q93-(K93-N93)-(K93-S93))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N93*95%-(K93-Q93)/I$4-(K93-S93)),N93-(K93-Q93)/I$4-(K93-S93)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N93-(K93-Q93)/I$4-(K93-S93))),N93-(K93-Q93)/I$4-(K93-S93))))))))","v":7.584340358193101},null,null,null,null,null,null,null,null,12,78,{"$f":"AO92+11.4","v":901.4},{"$f":"AP92+10.7","v":815.7},858.55]
[12,79,{"$f":"0.000000000384*AQ94^3-0.000000342064*AQ94^2+0.001060852819*AQ94+0.088327034395","v":1.0046909588249839},0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C94)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C94<$I$3,C94-D94,MIN($I$3,C94-D94))))","v":0},{"$f":"IF(C94<$I$7,MAX(0,C94-D94-E94-F94,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C94-D94-F94)),MIN(I$7,MAX(0,C94-D94-E94-F94))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C94-D94-E94-F94,MIN(I$7,C94-E94-F94)),MIN(I$7,MAX(0,C94-D94-F94))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C94-F94-G94,C94-D94-F94-G94),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C94-G94,IF(OPFOKLEGHEN!$J$18=\"nee\",C94-D94-G94)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C94-G94,C94-D94-F94-G94),C94-D94-F94-G94))","v":1.0046909588249839},1.0046909588249839,0.89078149007886331,7.8398505580889193,{"$f":"SUM(K$16:K94)/$K$137","v":0.23916662158380123},7.0701848640299603E-2,7.8398505580889193,{"$f":"IF(E94<I$3,P94*(1-I$6*D94/C94),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P94*(1-$I$6)+(C94-D94)/C94*(K94-P94*(1-I$6)),P94*(1-$I$6)+(C94-D94)/C94*(K94-P94*(1-I$6))))","v":7.8398505580889193},7.8398505580889193,7.8398505580889193,7.8398505580889193,{"$f":"MIN(K94,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K94-(G94/(C94-G94))*(Q94)*95%,K94-(G94/(C94-G94))*(P94)*84%))","v":7.8398505580889193},7.8398505580889193,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H94/C94*K94,IF(OPFOKLEGHEN!$H$20=\"ja\",O94-(K94-Q94)-(K94-S94),Q94-(K94-O94)-(K94-S94)))","v":7.8398505580889193},{"$f":"IF(H94=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q94-(K94-R94)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O94*80%-(K94-S94)),(Q94-(K94-S94)-(K94-T94))),(N94-(K94-S94))))","v":15.679701116177839},{"$f":"IF(H94=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q94-(K94-R94)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O94*80%-(K94-S94)),(Q94-(K94-S94)-(K94-N94))),(N94-(K94-S94))))","v":15.679701116177839},{"$f":"IF(H94=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q94-(K94-R94)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O94-(K94-S94)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N94-(K94-Q94)-(K94-S94)),(Q94-(K94-N94/80%)))))),(O94-(K94-S94))))","v":15.679701116177839},1,null,null,{"$f":"IF(H94=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P94-(K94-R94),K94-(K94-O94)/I$6-(K94-R94)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K94-O94)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O94-(K94-S94),IF(OPFOKLEGHEN!$H$20=\"nee\",(O94-(K94-S94)),(O94-(K94-S94)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O94*80%-(K94-S94),0+O94-(K94-S94)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O94*80%-(K94-S94)),O94*93%-(K94-S94)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O94-(K94-S94))),O94-(K94-S94))))))))","v":7.8398505580889193},{"$f":"IF(H94=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q94-(K94-R94),N94-(K94-R94)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q94-(K94-N94)-(K94-S94),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q94-(K94-N94)-(K94-S94)),(O94-(K94-S94)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q94*$N$135-(K94-N94)-(K94-S94),(Q94-(K94-N94)-(K94-S94))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N94*95%-(K94-Q94)/I$4-(K94-S94)),N94-(K94-Q94)/I$4-(K94-S94)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N94-(K94-Q94)/I$4-(K94-S94))),N94-(K94-Q94)/I$4-(K94-S94))))))))","v":7.8398505580889193},null,null,null,null,null,null,null,null,12,79,912.8,826.40000000000009,869.6]
[12,80,1.0195467892483661,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C95)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C95<$I$3,C95-D95,MIN($I$3,C95-D95))))","v":0},{"$f":"IF(C95<$I$7,MAX(0,C95-D95-E95-F95,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C95-D95-F95)),MIN(I$7,MAX(0,C95-D95-E95-F95))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C95-D95-E95-F95,MIN(I$7,C95-E95-F95)),MIN(I$7,MAX(0,C95-D95-F95))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C95-F95-G95,C95-D95-F95-G95),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C95-G95,IF(OPFOKLEGHEN!$J$18=\"nee\",C95-D95-G95)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C95-G95,C95-D95-F95-G95),C95-D95-F95-G95))","v":1.0195467892483661},1.0195467892483661,0.90732359011146546,8.1035155532212197,{"$f":"SUM(K$16:K95)/$K$137","v":0.24865616339683272},7.4004708248595605E-2,8.1035155532212197,{"$f":"IF(E95<I$3,P95*(1-I$6*D95/C95),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P95*(1-$I$6)+(C95-D95)/C95*(K95-P95*(1-I$6)),P95*(1-$I$6)+(C95-D95)/C95*(K95-P95*(1-I$6))))","v":8.1035155532212197},8.1035155532212197,8.1035155532212197,8.1035155532212197,{"$f":"MIN(K95,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K95-(G95/(C95-G95))*(Q95)*95%,K95-(G95/(C95-G95))*(P95)*84%))","v":8.1035155532212197},8.1035155532212197,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H95/C95*K95,IF(OPFOKLEGHEN!$H$20=\"ja\",O95-(K95-Q95)-(K95-S95),Q95-(K95-O95)-(K95-S95)))","v":8.1035155532212197},{"$f":"IF(H95=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q95-(K95-R95)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O95*80%-(K95-S95)),(Q95-(K95-S95)-(K95-T95))),(N95-(K95-S95))))","v":16.207031106442439},{"$f":"IF(H95=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q95-(K95-R95)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O95*80%-(K95-S95)),(Q95-(K95-S95)-(K95-N95))),(N95-(K95-S95))))","v":16.207031106442439},{"$f":"IF(H95=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q95-(K95-R95)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O95-(K95-S95)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N95-(K95-Q95)-(K95-S95)),(Q95-(K95-N95/80%)))))),(O95-(K95-S95))))","v":16.207031106442439},1,null,null,{"$f":"IF(H95=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P95-(K95-R95),K95-(K95-O95)/I$6-(K95-R95)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K95-O95)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O95-(K95-S95),IF(OPFOKLEGHEN!$H$20=\"nee\",(O95-(K95-S95)),(O95-(K95-S95)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O95*80%-(K95-S95),0+O95-(K95-S95)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O95*80%-(K95-S95)),O95*93%-(K95-S95)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O95-(K95-S95))),O95-(K95-S95))))))))","v":8.1035155532212197},{"$f":"IF(H95=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q95-(K95-R95),N95-(K95-R95)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q95-(K95-N95)-(K95-S95),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q95-(K95-N95)-(K95-S95)),(O95-(K95-S95)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q95*$N$135-(K95-N95)-(K95-S95),(Q95-(K95-N95)-(K95-S95))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N95*95%-(K95-Q95)/I$4-(K95-S95)),N95-(K95-Q95)/I$4-(K95-S95)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N95-(K95-Q95)/I$4-(K95-S95))),N95-(K95-Q95)/I$4-(K95-S95))))))))","v":8.1035155532212197},null,null,null,null,null,null,null,null,12,80,924.19999999999993,837.10000000000014,880.65000000000009]
[12,81,1.0345668340541321,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C96)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C96<$I$3,C96-D96,MIN($I$3,C96-D96))))","v":0},{"$f":"IF(C96<$I$7,MAX(0,C96-D96-E96-F96,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C96-D96-F96)),MIN(I$7,MAX(0,C96-D96-E96-F96))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C96-D96-E96-F96,MIN(I$7,C96-E96-F96)),MIN(I$7,MAX(0,C96-D96-F96))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C96-F96-G96,C96-D96-F96-G96),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C96-G96,IF(OPFOKLEGHEN!$J$18=\"nee\",C96-D96-G96)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C96-G96,C96-D96-F96-G96),C96-D96-F96-G96))","v":1.0345668340541321},1.0345668340541321,0.92417288228550343,8.3755990493964081,{"$f":"SUM(K$16:K96)/$K$137","v":0.25846432589944429},7.7445607648528425E-2,8.3755990493964081,{"$f":"IF(E96<I$3,P96*(1-I$6*D96/C96),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P96*(1-$I$6)+(C96-D96)/C96*(K96-P96*(1-I$6)),P96*(1-$I$6)+(C96-D96)/C96*(K96-P96*(1-I$6))))","v":8.3755990493964081},8.3755990493964081,8.3755990493964081,8.3755990493964081,{"$f":"MIN(K96,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K96-(G96/(C96-G96))*(Q96)*95%,K96-(G96/(C96-G96))*(P96)*84%))","v":8.3755990493964081},8.3755990493964081,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H96/C96*K96,IF(OPFOKLEGHEN!$H$20=\"ja\",O96-(K96-Q96)-(K96-S96),Q96-(K96-O96)-(K96-S96)))","v":8.3755990493964081},{"$f":"IF(H96=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q96-(K96-R96)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O96*80%-(K96-S96)),(Q96-(K96-S96)-(K96-T96))),(N96-(K96-S96))))","v":16.751198098792816},{"$f":"IF(H96=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q96-(K96-R96)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O96*80%-(K96-S96)),(Q96-(K96-S96)-(K96-N96))),(N96-(K96-S96))))","v":16.751198098792816},{"$f":"IF(H96=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q96-(K96-R96)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O96-(K96-S96)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N96-(K96-Q96)-(K96-S96)),(Q96-(K96-N96/80%)))))),(O96-(K96-S96))))","v":16.751198098792816},1,null,null,{"$f":"IF(H96=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P96-(K96-R96),K96-(K96-O96)/I$6-(K96-R96)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K96-O96)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O96-(K96-S96),IF(OPFOKLEGHEN!$H$20=\"nee\",(O96-(K96-S96)),(O96-(K96-S96)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O96*80%-(K96-S96),0+O96-(K96-S96)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O96*80%-(K96-S96)),O96*93%-(K96-S96)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O96-(K96-S96))),O96-(K96-S96))))))))","v":8.3755990493964081},{"$f":"IF(H96=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q96-(K96-R96),N96-(K96-R96)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q96-(K96-N96)-(K96-S96),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q96-(K96-N96)-(K96-S96)),(O96-(K96-S96)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q96*$N$135-(K96-N96)-(K96-S96),(Q96-(K96-N96)-(K96-S96))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N96*95%-(K96-Q96)/I$4-(K96-S96)),N96-(K96-Q96)/I$4-(K96-S96)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N96-(K96-Q96)/I$4-(K96-S96))),N96-(K96-Q96)/I$4-(K96-S96))))))))","v":8.3755990493964081},null,null,null,null,null,null,null,null,12,81,935.59999999999991,847.80000000000018,891.7]
[12,82,1.0497542018742498,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C97)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C97<$I$3,C97-D97,MIN($I$3,C97-D97))))","v":0},{"$f":"IF(C97<$I$7,MAX(0,C97-D97-E97-F97,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C97-D97-F97)),MIN(I$7,MAX(0,C97-D97-E97-F97))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C97-D97-E97-F97,MIN(I$7,C97-E97-F97)),MIN(I$7,MAX(0,C97-D97-F97))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C97-F97-G97,C97-D97-F97-G97),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C97-G97,IF(OPFOKLEGHEN!$J$18=\"nee\",C97-D97-G97)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C97-G97,C97-D97-F97-G97),C97-D97-F97-G97))","v":1.0497542018742498},1.0497542018742498,0.94133507125828009,8.6563731106827877,{"$f":"SUM(K$16:K97)/$K$137","v":0.26860128609203282},8.102997660684802E-2,8.6563731106827877,{"$f":"IF(E97<I$3,P97*(1-I$6*D97/C97),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P97*(1-$I$6)+(C97-D97)/C97*(K97-P97*(1-I$6)),P97*(1-$I$6)+(C97-D97)/C97*(K97-P97*(1-I$6))))","v":8.6563731106827877},8.6563731106827877,8.6563731106827877,8.6563731106827877,{"$f":"MIN(K97,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K97-(G97/(C97-G97))*(Q97)*95%,K97-(G97/(C97-G97))*(P97)*84%))","v":8.6563731106827877},8.6563731106827877,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H97/C97*K97,IF(OPFOKLEGHEN!$H$20=\"ja\",O97-(K97-Q97)-(K97-S97),Q97-(K97-O97)-(K97-S97)))","v":8.6563731106827877},{"$f":"IF(H97=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q97-(K97-R97)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O97*80%-(K97-S97)),(Q97-(K97-S97)-(K97-T97))),(N97-(K97-S97))))","v":17.312746221365575},{"$f":"IF(H97=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q97-(K97-R97)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O97*80%-(K97-S97)),(Q97-(K97-S97)-(K97-N97))),(N97-(K97-S97))))","v":17.312746221365575},{"$f":"IF(H97=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q97-(K97-R97)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O97-(K97-S97)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N97-(K97-Q97)-(K97-S97)),(Q97-(K97-N97/80%)))))),(O97-(K97-S97))))","v":17.312746221365575},1,null,null,{"$f":"IF(H97=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P97-(K97-R97),K97-(K97-O97)/I$6-(K97-R97)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K97-O97)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O97-(K97-S97),IF(OPFOKLEGHEN!$H$20=\"nee\",(O97-(K97-S97)),(O97-(K97-S97)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O97*80%-(K97-S97),0+O97-(K97-S97)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O97*80%-(K97-S97)),O97*93%-(K97-S97)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O97-(K97-S97))),O97-(K97-S97))))))))","v":8.6563731106827877},{"$f":"IF(H97=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q97-(K97-R97),N97-(K97-R97)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q97-(K97-N97)-(K97-S97),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q97-(K97-N97)-(K97-S97)),(O97-(K97-S97)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q97*$N$135-(K97-N97)-(K97-S97),(Q97-(K97-N97)-(K97-S97))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N97*95%-(K97-Q97)/I$4-(K97-S97)),N97-(K97-Q97)/I$4-(K97-S97)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N97-(K97-Q97)/I$4-(K97-S97))),N97-(K97-Q97)/I$4-(K97-S97))))))))","v":8.6563731106827877},null,null,null,null,null,null,null,null,12,82,946.99999999999989,858.50000000000023,902.75]
[12,83,1.0651120013406881,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C98)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C98<$I$3,C98-D98,MIN($I$3,C98-D98))))","v":0},{"$f":"IF(C98<$I$7,MAX(0,C98-D98-E98-F98,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C98-D98-F98)),MIN(I$7,MAX(0,C98-D98-E98-F98))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C98-D98-E98-F98,MIN(I$7,C98-E98-F98)),MIN(I$7,MAX(0,C98-D98-F98))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C98-F98-G98,C98-D98-F98-G98),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C98-G98,IF(OPFOKLEGHEN!$J$18=\"nee\",C98-D98-G98)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C98-G98,C98-D98-F98-G98),C98-D98-F98-G98))","v":1.0651120013406881},1.0651120013406881,0.95881596762442789,8.9461184131382385,{"$f":"SUM(K$16:K98)/$K$137","v":0.27907754965791931},8.4763450718090605E-2,8.9461184131382385,{"$f":"IF(E98<I$3,P98*(1-I$6*D98/C98),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P98*(1-$I$6)+(C98-D98)/C98*(K98-P98*(1-I$6)),P98*(1-$I$6)+(C98-D98)/C98*(K98-P98*(1-I$6))))","v":8.9461184131382385},8.9461184131382385,8.9461184131382385,8.9461184131382385,{"$f":"MIN(K98,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K98-(G98/(C98-G98))*(Q98)*95%,K98-(G98/(C98-G98))*(P98)*84%))","v":8.9461184131382385},8.9461184131382385,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H98/C98*K98,IF(OPFOKLEGHEN!$H$20=\"ja\",O98-(K98-Q98)-(K98-S98),Q98-(K98-O98)-(K98-S98)))","v":8.9461184131382385},{"$f":"IF(H98=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q98-(K98-R98)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O98*80%-(K98-S98)),(Q98-(K98-S98)-(K98-T98))),(N98-(K98-S98))))","v":17.892236826276477},{"$f":"IF(H98=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q98-(K98-R98)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O98*80%-(K98-S98)),(Q98-(K98-S98)-(K98-N98))),(N98-(K98-S98))))","v":17.892236826276477},{"$f":"IF(H98=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q98-(K98-R98)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O98-(K98-S98)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N98-(K98-Q98)-(K98-S98)),(Q98-(K98-N98/80%)))))),(O98-(K98-S98))))","v":17.892236826276477},1,null,null,{"$f":"IF(H98=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P98-(K98-R98),K98-(K98-O98)/I$6-(K98-R98)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K98-O98)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O98-(K98-S98),IF(OPFOKLEGHEN!$H$20=\"nee\",(O98-(K98-S98)),(O98-(K98-S98)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O98*80%-(K98-S98),0+O98-(K98-S98)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O98*80%-(K98-S98)),O98*93%-(K98-S98)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O98-(K98-S98))),O98-(K98-S98))))))))","v":8.9461184131382385},{"$f":"IF(H98=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q98-(K98-R98),N98-(K98-R98)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q98-(K98-N98)-(K98-S98),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q98-(K98-N98)-(K98-S98)),(O98-(K98-S98)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q98*$N$135-(K98-N98)-(K98-S98),(Q98-(K98-N98)-(K98-S98))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N98*95%-(K98-Q98)/I$4-(K98-S98)),N98-(K98-Q98)/I$4-(K98-S98)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N98-(K98-Q98)/I$4-(K98-S98))),N98-(K98-Q98)/I$4-(K98-S98))))))))","v":8.9461184131382385},null,null,null,null,null,null,null,null,12,83,958.39999999999986,869.20000000000027,913.80000000000007]
[12,84,1.08085538197,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C99)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C99<$I$3,C99-D99,MIN($I$3,C99-D99))))","v":0},{"$f":"IF(C99<$I$7,MAX(0,C99-D99-E99-F99,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C99-D99-F99)),MIN(I$7,MAX(0,C99-D99-E99-F99))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C99-D99-E99-F99,MIN(I$7,C99-E99-F99)),MIN(I$7,MAX(0,C99-D99-F99))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C99-F99-G99,C99-D99-F99-G99),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C99-G99,IF(OPFOKLEGHEN!$J$18=\"nee\",C99-D99-G99)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C99-G99,C99-D99-F99-G99),C99-D99-F99-G99))","v":1.08085538197},1.08085538197,0.97662148988319786,9.2469385589532536,{"$f":"SUM(K$16:K99)/$K$137","v":0.28990608568298298},8.8669273852976391E-2,9.2469385589532536,{"$f":"IF(E99<I$3,P99*(1-I$6*D99/C99),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P99*(1-$I$6)+(C99-D99)/C99*(K99-P99*(1-I$6)),P99*(1-$I$6)+(C99-D99)/C99*(K99-P99*(1-I$6))))","v":9.2469385589532536},9.2469385589532536,9.2469385589532536,9.2469385589532536,{"$f":"MIN(K99,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K99-(G99/(C99-G99))*(Q99)*95%,K99-(G99/(C99-G99))*(P99)*84%))","v":9.2469385589532536},9.2469385589532536,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H99/C99*K99,IF(OPFOKLEGHEN!$H$20=\"ja\",O99-(K99-Q99)-(K99-S99),Q99-(K99-O99)-(K99-S99)))","v":9.2469385589532536},{"$f":"IF(H99=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q99-(K99-R99)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O99*80%-(K99-S99)),(Q99-(K99-S99)-(K99-T99))),(N99-(K99-S99))))","v":18.493877117906507},{"$f":"IF(H99=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q99-(K99-R99)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O99*80%-(K99-S99)),(Q99-(K99-S99)-(K99-N99))),(N99-(K99-S99))))","v":18.493877117906507},{"$f":"IF(H99=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q99-(K99-R99)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O99-(K99-S99)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N99-(K99-Q99)-(K99-S99)),(Q99-(K99-N99/80%)))))),(O99-(K99-S99))))","v":18.493877117906507},1,null,null,{"$f":"IF(H99=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P99-(K99-R99),K99-(K99-O99)/I$6-(K99-R99)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K99-O99)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O99-(K99-S99),IF(OPFOKLEGHEN!$H$20=\"nee\",(O99-(K99-S99)),(O99-(K99-S99)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O99*80%-(K99-S99),0+O99-(K99-S99)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O99*80%-(K99-S99)),O99*93%-(K99-S99)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O99-(K99-S99))),O99-(K99-S99))))))))","v":9.2469385589532536},{"$f":"IF(H99=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q99-(K99-R99),N99-(K99-R99)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q99-(K99-N99)-(K99-S99),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q99-(K99-N99)-(K99-S99)),(O99-(K99-S99)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q99*$N$135-(K99-N99)-(K99-S99),(Q99-(K99-N99)-(K99-S99))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N99*95%-(K99-Q99)/I$4-(K99-S99)),N99-(K99-Q99)/I$4-(K99-S99)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N99-(K99-Q99)/I$4-(K99-S99))),N99-(K99-Q99)/I$4-(K99-S99))))))))","v":9.2469385589532536},null,null,null,null,null,null,null,null,12,84,970,880,925]
[13,85,1.0971378458774621,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C100)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C100<$I$3,C100-D100,MIN($I$3,C100-D100))))","v":0},{"$f":"IF(C100<$I$7,MAX(0,C100-D100-E100-F100,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C100-D100-F100)),MIN(I$7,MAX(0,C100-D100-E100-F100))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C100-D100-E100-F100,MIN(I$7,C100-E100-F100)),MIN(I$7,MAX(0,C100-D100-F100))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C100-F100-G100,C100-D100-F100-G100),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C100-G100,IF(OPFOKLEGHEN!$J$18=\"nee\",C100-D100-G100)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C100-G100,C100-D100-F100-G100),C100-D100-F100-G100))","v":1.0971378458774621},1.0971378458774621,0.99475766644228514,9.5605438419758784,{"$f":"SUM(K$16:K100)/$K$137","v":0.30110186607581341},9.2767834083099285E-2,9.5605438419758784,{"$f":"IF(E100<I$3,P100*(1-I$6*D100/C100),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P100*(1-$I$6)+(C100-D100)/C100*(K100-P100*(1-I$6)),P100*(1-$I$6)+(C100-D100)/C100*(K100-P100*(1-I$6))))","v":9.5605438419758784},9.5605438419758784,9.5605438419758784,9.5605438419758784,{"$f":"MIN(K100,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K100-(G100/(C100-G100))*(Q100)*95%,K100-(G100/(C100-G100))*(P100)*84%))","v":9.5605438419758784},9.5605438419758784,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H100/C100*K100,IF(OPFOKLEGHEN!$H$20=\"ja\",O100-(K100-Q100)-(K100-S100),Q100-(K100-O100)-(K100-S100)))","v":9.5605438419758784},{"$f":"IF(H100=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q100-(K100-R100)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O100*80%-(K100-S100)),(Q100-(K100-S100)-(K100-T100))),(N100-(K100-S100))))","v":19.121087683951757},{"$f":"IF(H100=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q100-(K100-R100)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O100*80%-(K100-S100)),(Q100-(K100-S100)-(K100-N100))),(N100-(K100-S100))))","v":19.121087683951757},{"$f":"IF(H100=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q100-(K100-R100)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O100-(K100-S100)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N100-(K100-Q100)-(K100-S100)),(Q100-(K100-N100/80%)))))),(O100-(K100-S100))))","v":19.121087683951757},1,null,null,{"$f":"IF(H100=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P100-(K100-R100),K100-(K100-O100)/I$6-(K100-R100)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K100-O100)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O100-(K100-S100),IF(OPFOKLEGHEN!$H$20=\"nee\",(O100-(K100-S100)),(O100-(K100-S100)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O100*80%-(K100-S100),0+O100-(K100-S100)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O100*80%-(K100-S100)),O100*93%-(K100-S100)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O100-(K100-S100))),O100-(K100-S100))))))))","v":9.5605438419758784},{"$f":"IF(H100=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q100-(K100-R100),N100-(K100-R100)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q100-(K100-N100)-(K100-S100),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q100-(K100-N100)-(K100-S100)),(O100-(K100-S100)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q100*$N$135-(K100-N100)-(K100-S100),(Q100-(K100-N100)-(K100-S100))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N100*95%-(K100-Q100)/I$4-(K100-S100)),N100-(K100-Q100)/I$4-(K100-S100)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N100-(K100-Q100)/I$4-(K100-S100))),N100-(K100-Q100)/I$4-(K100-S100))))))))","v":9.5605438419758784},null,null,null,null,null,null,null,null,13,85,{"$f":"AO99+12.9","v":982.9},{"$f":"AP99+10","v":890},936.45]
[13,86,1.1136134831306359,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C101)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C101<$I$3,C101-D101,MIN($I$3,C101-D101))))","v":0},{"$f":"IF(C101<$I$7,MAX(0,C101-D101-E101-F101,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C101-D101-F101)),MIN(I$7,MAX(0,C101-D101-E101-F101))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C101-D101-E101-F101,MIN(I$7,C101-E101-F101)),MIN(I$7,MAX(0,C101-D101-F101))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C101-F101-G101,C101-D101-F101-G101),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C101-G101,IF(OPFOKLEGHEN!$J$18=\"nee\",C101-D101-G101)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C101-G101,C101-D101-F101-G101),C101-D101-F101-G101))","v":1.1136134831306359},1.1136134831306359,1.0132306376588618,9.8843223446533326,{"$f":"SUM(K$16:K101)/$K$137","v":0.3126768040847599},9.7037867767144598E-2,9.8843223446533326,{"$f":"IF(E101<I$3,P101*(1-I$6*D101/C101),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P101*(1-$I$6)+(C101-D101)/C101*(K101-P101*(1-I$6)),P101*(1-$I$6)+(C101-D101)/C101*(K101-P101*(1-I$6))))","v":9.8843223446533326},9.8843223446533326,9.8843223446533326,9.8843223446533326,{"$f":"MIN(K101,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K101-(G101/(C101-G101))*(Q101)*95%,K101-(G101/(C101-G101))*(P101)*84%))","v":9.8843223446533326},9.8843223446533326,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H101/C101*K101,IF(OPFOKLEGHEN!$H$20=\"ja\",O101-(K101-Q101)-(K101-S101),Q101-(K101-O101)-(K101-S101)))","v":9.8843223446533326},{"$f":"IF(H101=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q101-(K101-R101)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O101*80%-(K101-S101)),(Q101-(K101-S101)-(K101-T101))),(N101-(K101-S101))))","v":19.768644689306665},{"$f":"IF(H101=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q101-(K101-R101)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O101*80%-(K101-S101)),(Q101-(K101-S101)-(K101-N101))),(N101-(K101-S101))))","v":19.768644689306665},{"$f":"IF(H101=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q101-(K101-R101)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O101-(K101-S101)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N101-(K101-Q101)-(K101-S101)),(Q101-(K101-N101/80%)))))),(O101-(K101-S101))))","v":19.768644689306665},1,null,null,{"$f":"IF(H101=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P101-(K101-R101),K101-(K101-O101)/I$6-(K101-R101)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K101-O101)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O101-(K101-S101),IF(OPFOKLEGHEN!$H$20=\"nee\",(O101-(K101-S101)),(O101-(K101-S101)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O101*80%-(K101-S101),0+O101-(K101-S101)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O101*80%-(K101-S101)),O101*93%-(K101-S101)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O101-(K101-S101))),O101-(K101-S101))))))))","v":9.8843223446533326},{"$f":"IF(H101=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q101-(K101-R101),N101-(K101-R101)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q101-(K101-N101)-(K101-S101),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q101-(K101-N101)-(K101-S101)),(O101-(K101-S101)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q101*$N$135-(K101-N101)-(K101-S101),(Q101-(K101-N101)-(K101-S101))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N101*95%-(K101-Q101)/I$4-(K101-S101)),N101-(K101-Q101)/I$4-(K101-S101)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N101-(K101-Q101)/I$4-(K101-S101))),N101-(K101-Q101)/I$4-(K101-S101))))))))","v":9.8843223446533326},null,null,null,null,null,null,null,null,13,86,995.8,900,947.9]
[13,87,1.1302857523183538,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C102)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C102<$I$3,C102-D102,MIN($I$3,C102-D102))))","v":0},{"$f":"IF(C102<$I$7,MAX(0,C102-D102-E102-F102,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C102-D102-F102)),MIN(I$7,MAX(0,C102-D102-E102-F102))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C102-D102-E102-F102,MIN(I$7,C102-E102-F102)),MIN(I$7,MAX(0,C102-D102-F102))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C102-F102-G102,C102-D102-F102-G102),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C102-G102,IF(OPFOKLEGHEN!$J$18=\"nee\",C102-D102-G102)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C102-G102,C102-D102-F102-G102),C102-D102-F102-G102))","v":1.1302857523183538},1.1302857523183538,1.0320466579185175,10.218606866596131,{"$f":"SUM(K$16:K102)/$K$137","v":0.32464320267986696},0.10148616408605746,10.218606866596131,{"$f":"IF(E102<I$3,P102*(1-I$6*D102/C102),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P102*(1-$I$6)+(C102-D102)/C102*(K102-P102*(1-I$6)),P102*(1-$I$6)+(C102-D102)/C102*(K102-P102*(1-I$6))))","v":10.218606866596131},10.218606866596131,10.218606866596131,10.218606866596131,{"$f":"MIN(K102,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K102-(G102/(C102-G102))*(Q102)*95%,K102-(G102/(C102-G102))*(P102)*84%))","v":10.218606866596131},10.218606866596131,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H102/C102*K102,IF(OPFOKLEGHEN!$H$20=\"ja\",O102-(K102-Q102)-(K102-S102),Q102-(K102-O102)-(K102-S102)))","v":10.218606866596131},{"$f":"IF(H102=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q102-(K102-R102)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O102*80%-(K102-S102)),(Q102-(K102-S102)-(K102-T102))),(N102-(K102-S102))))","v":20.437213733192262},{"$f":"IF(H102=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q102-(K102-R102)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O102*80%-(K102-S102)),(Q102-(K102-S102)-(K102-N102))),(N102-(K102-S102))))","v":20.437213733192262},{"$f":"IF(H102=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q102-(K102-R102)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O102-(K102-S102)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N102-(K102-Q102)-(K102-S102)),(Q102-(K102-N102/80%)))))),(O102-(K102-S102))))","v":20.437213733192262},1,null,null,{"$f":"IF(H102=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P102-(K102-R102),K102-(K102-O102)/I$6-(K102-R102)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K102-O102)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O102-(K102-S102),IF(OPFOKLEGHEN!$H$20=\"nee\",(O102-(K102-S102)),(O102-(K102-S102)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O102*80%-(K102-S102),0+O102-(K102-S102)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O102*80%-(K102-S102)),O102*93%-(K102-S102)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O102-(K102-S102))),O102-(K102-S102))))))))","v":10.218606866596131},{"$f":"IF(H102=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q102-(K102-R102),N102-(K102-R102)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q102-(K102-N102)-(K102-S102),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q102-(K102-N102)-(K102-S102)),(O102-(K102-S102)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q102*$N$135-(K102-N102)-(K102-S102),(Q102-(K102-N102)-(K102-S102))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N102*95%-(K102-Q102)/I$4-(K102-S102)),N102-(K102-Q102)/I$4-(K102-S102)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N102-(K102-Q102)/I$4-(K102-S102))),N102-(K102-Q102)/I$4-(K102-S102))))))))","v":10.218606866596131},null,null,null,null,null,null,null,null,13,87,1008.6999999999999,910,959.34999999999991]
[13,88,1.1471581120294478,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C103)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C103<$I$3,C103-D103,MIN($I$3,C103-D103))))","v":0},{"$f":"IF(C103<$I$7,MAX(0,C103-D103-E103-F103,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C103-D103-F103)),MIN(I$7,MAX(0,C103-D103-E103-F103))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C103-D103-E103-F103,MIN(I$7,C103-E103-F103)),MIN(I$7,MAX(0,C103-D103-F103))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C103-F103-G103,C103-D103-F103-G103),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C103-G103,IF(OPFOKLEGHEN!$J$18=\"nee\",C103-D103-G103)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C103-G103,C103-D103-F103-G103),C103-D103-F103-G103))","v":1.1471581120294478},1.1471581120294478,1.0512120977528023,10.563740812109431,{"$f":"SUM(K$16:K103)/$K$137","v":0.33701376697139734},0.10611977071525457,10.563740812109431,{"$f":"IF(E103<I$3,P103*(1-I$6*D103/C103),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P103*(1-$I$6)+(C103-D103)/C103*(K103-P103*(1-I$6)),P103*(1-$I$6)+(C103-D103)/C103*(K103-P103*(1-I$6))))","v":10.563740812109431},10.563740812109431,10.563740812109431,10.563740812109431,{"$f":"MIN(K103,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K103-(G103/(C103-G103))*(Q103)*95%,K103-(G103/(C103-G103))*(P103)*84%))","v":10.563740812109431},10.563740812109431,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H103/C103*K103,IF(OPFOKLEGHEN!$H$20=\"ja\",O103-(K103-Q103)-(K103-S103),Q103-(K103-O103)-(K103-S103)))","v":10.563740812109431},{"$f":"IF(H103=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q103-(K103-R103)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O103*80%-(K103-S103)),(Q103-(K103-S103)-(K103-T103))),(N103-(K103-S103))))","v":21.127481624218863},{"$f":"IF(H103=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q103-(K103-R103)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O103*80%-(K103-S103)),(Q103-(K103-S103)-(K103-N103))),(N103-(K103-S103))))","v":21.127481624218863},{"$f":"IF(H103=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q103-(K103-R103)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O103-(K103-S103)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N103-(K103-Q103)-(K103-S103)),(Q103-(K103-N103/80%)))))),(O103-(K103-S103))))","v":21.127481624218863},1,null,null,{"$f":"IF(H103=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P103-(K103-R103),K103-(K103-O103)/I$6-(K103-R103)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K103-O103)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O103-(K103-S103),IF(OPFOKLEGHEN!$H$20=\"nee\",(O103-(K103-S103)),(O103-(K103-S103)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O103*80%-(K103-S103),0+O103-(K103-S103)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O103*80%-(K103-S103)),O103*93%-(K103-S103)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O103-(K103-S103))),O103-(K103-S103))))))))","v":10.563740812109431},{"$f":"IF(H103=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q103-(K103-R103),N103-(K103-R103)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q103-(K103-N103)-(K103-S103),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q103-(K103-N103)-(K103-S103)),(O103-(K103-S103)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q103*$N$135-(K103-N103)-(K103-S103),(Q103-(K103-N103)-(K103-S103))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N103*95%-(K103-Q103)/I$4-(K103-S103)),N103-(K103-Q103)/I$4-(K103-S103)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N103-(K103-Q103)/I$4-(K103-S103))),N103-(K103-Q103)/I$4-(K103-S103))))))))","v":10.563740812109431},null,null,null,null,null,null,null,null,13,88,1021.5999999999999,920,970.8]
[13,89,1.16423402085275,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C104)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C104<$I$3,C104-D104,MIN($I$3,C104-D104))))","v":0},{"$f":"IF(C104<$I$7,MAX(0,C104-D104-E104-F104,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C104-D104-F104)),MIN(I$7,MAX(0,C104-D104-E104-F104))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C104-D104-E104-F104,MIN(I$7,C104-E104-F104)),MIN(I$7,MAX(0,C104-D104-F104))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C104-F104-G104,C104-D104-F104-G104),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C104-G104,IF(OPFOKLEGHEN!$J$18=\"nee\",C104-D104-G104)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C104-G104,C104-D104-F104-G104),C104-D104-F104-G104))","v":1.16423402085275},1.16423402085275,1.0707334459960947,10.920078512619533,{"$f":"SUM(K$16:K104)/$K$137","v":0.34980161700592921},0.1109460031533263,10.920078512619533,{"$f":"IF(E104<I$3,P104*(1-I$6*D104/C104),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P104*(1-$I$6)+(C104-D104)/C104*(K104-P104*(1-I$6)),P104*(1-$I$6)+(C104-D104)/C104*(K104-P104*(1-I$6))))","v":10.920078512619533},10.920078512619533,10.920078512619533,10.920078512619533,{"$f":"MIN(K104,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K104-(G104/(C104-G104))*(Q104)*95%,K104-(G104/(C104-G104))*(P104)*84%))","v":10.920078512619533},10.920078512619533,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H104/C104*K104,IF(OPFOKLEGHEN!$H$20=\"ja\",O104-(K104-Q104)-(K104-S104),Q104-(K104-O104)-(K104-S104)))","v":10.920078512619533},{"$f":"IF(H104=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q104-(K104-R104)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O104*80%-(K104-S104)),(Q104-(K104-S104)-(K104-T104))),(N104-(K104-S104))))","v":21.840157025239066},{"$f":"IF(H104=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q104-(K104-R104)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O104*80%-(K104-S104)),(Q104-(K104-S104)-(K104-N104))),(N104-(K104-S104))))","v":21.840157025239066},{"$f":"IF(H104=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q104-(K104-R104)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O104-(K104-S104)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N104-(K104-Q104)-(K104-S104)),(Q104-(K104-N104/80%)))))),(O104-(K104-S104))))","v":21.840157025239066},1,null,null,{"$f":"IF(H104=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P104-(K104-R104),K104-(K104-O104)/I$6-(K104-R104)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K104-O104)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O104-(K104-S104),IF(OPFOKLEGHEN!$H$20=\"nee\",(O104-(K104-S104)),(O104-(K104-S104)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O104*80%-(K104-S104),0+O104-(K104-S104)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O104*80%-(K104-S104)),O104*93%-(K104-S104)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O104-(K104-S104))),O104-(K104-S104))))))))","v":10.920078512619533},{"$f":"IF(H104=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q104-(K104-R104),N104-(K104-R104)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q104-(K104-N104)-(K104-S104),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q104-(K104-N104)-(K104-S104)),(O104-(K104-S104)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q104*$N$135-(K104-N104)-(K104-S104),(Q104-(K104-N104)-(K104-S104))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N104*95%-(K104-Q104)/I$4-(K104-S104)),N104-(K104-Q104)/I$4-(K104-S104)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N104-(K104-Q104)/I$4-(K104-S104))),N104-(K104-Q104)/I$4-(K104-S104))))))))","v":10.920078512619533},null,null,null,null,null,null,null,null,13,89,1034.5,930,982.25]
[13,90,1.181516937377092,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C105)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C105<$I$3,C105-D105,MIN($I$3,C105-D105))))","v":0},{"$f":"IF(C105<$I$7,MAX(0,C105-D105-E105-F105,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C105-D105-F105)),MIN(I$7,MAX(0,C105-D105-E105-F105))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C105-D105-E105-F105,MIN(I$7,C105-E105-F105)),MIN(I$7,MAX(0,C105-D105-F105))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C105-F105-G105,C105-D105-F105-G105),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C105-G105,IF(OPFOKLEGHEN!$J$18=\"nee\",C105-D105-G105)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C105-G105,C105-D105-F105-G105),C105-D105-F105-G105))","v":1.181516937377092},1.181516937377092,1.0906173119825242,11.287985558423287,{"$f":"SUM(K$16:K105)/$K$137","v":0.36302030095094528},0.11597245436736255,11.287985558423287,{"$f":"IF(E105<I$3,P105*(1-I$6*D105/C105),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P105*(1-$I$6)+(C105-D105)/C105*(K105-P105*(1-I$6)),P105*(1-$I$6)+(C105-D105)/C105*(K105-P105*(1-I$6))))","v":11.287985558423287},11.287985558423287,11.287985558423287,11.287985558423287,{"$f":"MIN(K105,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K105-(G105/(C105-G105))*(Q105)*95%,K105-(G105/(C105-G105))*(P105)*84%))","v":11.287985558423287},11.287985558423287,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H105/C105*K105,IF(OPFOKLEGHEN!$H$20=\"ja\",O105-(K105-Q105)-(K105-S105),Q105-(K105-O105)-(K105-S105)))","v":11.287985558423287},{"$f":"IF(H105=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q105-(K105-R105)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O105*80%-(K105-S105)),(Q105-(K105-S105)-(K105-T105))),(N105-(K105-S105))))","v":22.575971116846574},{"$f":"IF(H105=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q105-(K105-R105)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O105*80%-(K105-S105)),(Q105-(K105-S105)-(K105-N105))),(N105-(K105-S105))))","v":22.575971116846574},{"$f":"IF(H105=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q105-(K105-R105)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O105-(K105-S105)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N105-(K105-Q105)-(K105-S105)),(Q105-(K105-N105/80%)))))),(O105-(K105-S105))))","v":22.575971116846574},1,null,null,{"$f":"IF(H105=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P105-(K105-R105),K105-(K105-O105)/I$6-(K105-R105)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K105-O105)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O105-(K105-S105),IF(OPFOKLEGHEN!$H$20=\"nee\",(O105-(K105-S105)),(O105-(K105-S105)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O105*80%-(K105-S105),0+O105-(K105-S105)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O105*80%-(K105-S105)),O105*93%-(K105-S105)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O105-(K105-S105))),O105-(K105-S105))))))))","v":11.287985558423287},{"$f":"IF(H105=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q105-(K105-R105),N105-(K105-R105)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q105-(K105-N105)-(K105-S105),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q105-(K105-N105)-(K105-S105)),(O105-(K105-S105)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q105*$N$135-(K105-N105)-(K105-S105),(Q105-(K105-N105)-(K105-S105))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N105*95%-(K105-Q105)/I$4-(K105-S105)),N105-(K105-Q105)/I$4-(K105-S105)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N105-(K105-Q105)/I$4-(K105-S105))),N105-(K105-Q105)/I$4-(K105-S105))))))))","v":11.287985558423287},null,null,null,null,null,null,null,null,13,90,1047.4000000000001,940,993.7]
[13,91,1.1987797738900001,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C106)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C106<$I$3,C106-D106,MIN($I$3,C106-D106))))","v":0},{"$f":"IF(C106<$I$7,MAX(0,C106-D106-E106-F106,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C106-D106-F106)),MIN(I$7,MAX(0,C106-D106-E106-F106))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C106-D106-E106-F106,MIN(I$7,C106-E106-F106)),MIN(I$7,MAX(0,C106-D106-F106))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C106-F106-G106,C106-D106-F106-G106),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C106-G106,IF(OPFOKLEGHEN!$J$18=\"nee\",C106-D106-G106)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C106-G106,C106-D106-F106-G106),C106-D106-F106-G106))","v":1.1987797738900001},1.1987797738900001,1.1108704277836907,11.665595642099076,{"$f":"SUM(K$16:K106)/$K$137","v":0.37668118145306412},0.12118369902180547,11.665595642099076,{"$f":"IF(E106<I$3,P106*(1-I$6*D106/C106),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P106*(1-$I$6)+(C106-D106)/C106*(K106-P106*(1-I$6)),P106*(1-$I$6)+(C106-D106)/C106*(K106-P106*(1-I$6))))","v":11.665595642099076},11.665595642099076,11.665595642099076,11.665595642099076,{"$f":"MIN(K106,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K106-(G106/(C106-G106))*(Q106)*95%,K106-(G106/(C106-G106))*(P106)*84%))","v":11.665595642099076},11.665595642099076,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H106/C106*K106,IF(OPFOKLEGHEN!$H$20=\"ja\",O106-(K106-Q106)-(K106-S106),Q106-(K106-O106)-(K106-S106)))","v":11.665595642099076},{"$f":"IF(H106=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q106-(K106-R106)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O106*80%-(K106-S106)),(Q106-(K106-S106)-(K106-T106))),(N106-(K106-S106))))","v":23.331191284198152},{"$f":"IF(H106=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q106-(K106-R106)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O106*80%-(K106-S106)),(Q106-(K106-S106)-(K106-N106))),(N106-(K106-S106))))","v":23.331191284198152},{"$f":"IF(H106=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q106-(K106-R106)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O106-(K106-S106)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N106-(K106-Q106)-(K106-S106)),(Q106-(K106-N106/80%)))))),(O106-(K106-S106))))","v":23.331191284198152},1,null,null,{"$f":"IF(H106=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P106-(K106-R106),K106-(K106-O106)/I$6-(K106-R106)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K106-O106)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O106-(K106-S106),IF(OPFOKLEGHEN!$H$20=\"nee\",(O106-(K106-S106)),(O106-(K106-S106)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O106*80%-(K106-S106),0+O106-(K106-S106)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O106*80%-(K106-S106)),O106*93%-(K106-S106)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O106-(K106-S106))),O106-(K106-S106))))))))","v":11.665595642099076},{"$f":"IF(H106=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q106-(K106-R106),N106-(K106-R106)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q106-(K106-N106)-(K106-S106),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q106-(K106-N106)-(K106-S106)),(O106-(K106-S106)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q106*$N$135-(K106-N106)-(K106-S106),(Q106-(K106-N106)-(K106-S106))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N106*95%-(K106-Q106)/I$4-(K106-S106)),N106-(K106-Q106)/I$4-(K106-S106)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N106-(K106-Q106)/I$4-(K106-S106))),N106-(K106-Q106)/I$4-(K106-S106))))))))","v":11.665595642099076},null,null,null,null,null,null,null,null,13,91,1060,950,1005]
[14,92,1.2147740073650739,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C107)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C107<$I$3,C107-D107,MIN($I$3,C107-D107))))","v":0},{"$f":"IF(C107<$I$7,MAX(0,C107-D107-E107-F107,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C107-D107-F107)),MIN(I$7,MAX(0,C107-D107-E107-F107))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C107-D107-E107-F107,MIN(I$7,C107-E107-F107)),MIN(I$7,MAX(0,C107-D107-F107))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C107-F107-G107,C107-D107-F107-G107),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C107-G107,IF(OPFOKLEGHEN!$J$18=\"nee\",C107-D107-G107)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C107-G107,C107-D107-F107-G107),C107-D107-F107-G107))","v":1.2147740073650739},1.2147740073650739,1.1314996504879373,12.040763355257409,{"$f":"SUM(K$16:K107)/$K$137","v":0.39078139839842591},0.12645550555749793,12.040763355257409,{"$f":"IF(E107<I$3,P107*(1-I$6*D107/C107),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P107*(1-$I$6)+(C107-D107)/C107*(K107-P107*(1-I$6)),P107*(1-$I$6)+(C107-D107)/C107*(K107-P107*(1-I$6))))","v":12.040763355257409},12.040763355257409,12.040763355257409,12.040763355257409,{"$f":"MIN(K107,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K107-(G107/(C107-G107))*(Q107)*95%,K107-(G107/(C107-G107))*(P107)*84%))","v":12.040763355257409},12.040763355257409,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H107/C107*K107,IF(OPFOKLEGHEN!$H$20=\"ja\",O107-(K107-Q107)-(K107-S107),Q107-(K107-O107)-(K107-S107)))","v":12.040763355257409},{"$f":"IF(H107=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q107-(K107-R107)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O107*80%-(K107-S107)),(Q107-(K107-S107)-(K107-T107))),(N107-(K107-S107))))","v":24.081526710514819},{"$f":"IF(H107=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q107-(K107-R107)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O107*80%-(K107-S107)),(Q107-(K107-S107)-(K107-N107))),(N107-(K107-S107))))","v":24.081526710514819},{"$f":"IF(H107=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q107-(K107-R107)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O107-(K107-S107)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N107-(K107-Q107)-(K107-S107)),(Q107-(K107-N107/80%)))))),(O107-(K107-S107))))","v":24.081526710514819},1,null,null,{"$f":"IF(H107=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P107-(K107-R107),K107-(K107-O107)/I$6-(K107-R107)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K107-O107)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O107-(K107-S107),IF(OPFOKLEGHEN!$H$20=\"nee\",(O107-(K107-S107)),(O107-(K107-S107)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O107*80%-(K107-S107),0+O107-(K107-S107)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O107*80%-(K107-S107)),O107*93%-(K107-S107)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O107-(K107-S107))),O107-(K107-S107))))))))","v":12.040763355257409},{"$f":"IF(H107=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q107-(K107-R107),N107-(K107-R107)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q107-(K107-N107)-(K107-S107),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q107-(K107-N107)-(K107-S107)),(O107-(K107-S107)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q107*$N$135-(K107-N107)-(K107-S107),(Q107-(K107-N107)-(K107-S107))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N107*95%-(K107-Q107)/I$4-(K107-S107)),N107-(K107-Q107)/I$4-(K107-S107)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N107-(K107-Q107)/I$4-(K107-S107))),N107-(K107-Q107)/I$4-(K107-S107))))))))","v":12.040763355257409},null,null,null,null,null,null,null,null,14,92,{"$f":"AO106+11.4","v":1071.4000000000001},{"$f":"AP106+9.3","v":959.3},1015.35]
[14,93,1.230945554115652,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C108)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C108<$I$3,C108-D108,MIN($I$3,C108-D108))))","v":0},{"$f":"IF(C108<$I$7,MAX(0,C108-D108-E108-F108,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C108-D108-F108)),MIN(I$7,MAX(0,C108-D108-E108-F108))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C108-D108-E108-F108,MIN(I$7,C108-E108-F108)),MIN(I$7,MAX(0,C108-D108-F108))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C108-F108-G108,C108-D108-F108-G108),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C108-G108,IF(OPFOKLEGHEN!$J$18=\"nee\",C108-D108-G108)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C108-G108,C108-D108-F108-G108),C108-D108-F108-G108))","v":1.230945554115652},1.230945554115652,1.1525119645219535,12.42763223423014,{"$f":"SUM(K$16:K108)/$K$137","v":0.4053346543216314},0.13193719152778571,12.42763223423014,{"$f":"IF(E108<I$3,P108*(1-I$6*D108/C108),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P108*(1-$I$6)+(C108-D108)/C108*(K108-P108*(1-I$6)),P108*(1-$I$6)+(C108-D108)/C108*(K108-P108*(1-I$6))))","v":12.42763223423014},12.42763223423014,12.42763223423014,12.42763223423014,{"$f":"MIN(K108,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K108-(G108/(C108-G108))*(Q108)*95%,K108-(G108/(C108-G108))*(P108)*84%))","v":12.42763223423014},12.42763223423014,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H108/C108*K108,IF(OPFOKLEGHEN!$H$20=\"ja\",O108-(K108-Q108)-(K108-S108),Q108-(K108-O108)-(K108-S108)))","v":12.42763223423014},{"$f":"IF(H108=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q108-(K108-R108)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O108*80%-(K108-S108)),(Q108-(K108-S108)-(K108-T108))),(N108-(K108-S108))))","v":24.85526446846028},{"$f":"IF(H108=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q108-(K108-R108)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O108*80%-(K108-S108)),(Q108-(K108-S108)-(K108-N108))),(N108-(K108-S108))))","v":24.85526446846028},{"$f":"IF(H108=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q108-(K108-R108)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O108-(K108-S108)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N108-(K108-Q108)-(K108-S108)),(Q108-(K108-N108/80%)))))),(O108-(K108-S108))))","v":24.85526446846028},1,null,null,{"$f":"IF(H108=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P108-(K108-R108),K108-(K108-O108)/I$6-(K108-R108)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K108-O108)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O108-(K108-S108),IF(OPFOKLEGHEN!$H$20=\"nee\",(O108-(K108-S108)),(O108-(K108-S108)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O108*80%-(K108-S108),0+O108-(K108-S108)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O108*80%-(K108-S108)),O108*93%-(K108-S108)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O108-(K108-S108))),O108-(K108-S108))))))))","v":12.42763223423014},{"$f":"IF(H108=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q108-(K108-R108),N108-(K108-R108)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q108-(K108-N108)-(K108-S108),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q108-(K108-N108)-(K108-S108)),(O108-(K108-S108)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q108*$N$135-(K108-N108)-(K108-S108),(Q108-(K108-N108)-(K108-S108))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N108*95%-(K108-Q108)/I$4-(K108-S108)),N108-(K108-Q108)/I$4-(K108-S108)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N108-(K108-Q108)/I$4-(K108-S108))),N108-(K108-Q108)/I$4-(K108-S108))))))))","v":12.42763223423014},null,null,null,null,null,null,null,null,14,93,1082.8000000000002,968.59999999999991,1025.7]
[14,94,1.2472969686277182,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C109)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C109<$I$3,C109-D109,MIN($I$3,C109-D109))))","v":0},{"$f":"IF(C109<$I$7,MAX(0,C109-D109-E109-F109,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C109-D109-F109)),MIN(I$7,MAX(0,C109-D109-E109-F109))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C109-D109-E109-F109,MIN(I$7,C109-E109-F109)),MIN(I$7,MAX(0,C109-D109-F109))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C109-F109-G109,C109-D109-F109-G109),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C109-G109,IF(OPFOKLEGHEN!$J$18=\"nee\",C109-D109-G109)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C109-G109,C109-D109-F109-G109),C109-D109-F109-G109))","v":1.2472969686277182},1.2472969686277182,1.1739144840154885,12.826567001504452,{"$f":"SUM(K$16:K109)/$K$137","v":0.42035507886194612},0.13763667787002495,12.826567001504452,{"$f":"IF(E109<I$3,P109*(1-I$6*D109/C109),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P109*(1-$I$6)+(C109-D109)/C109*(K109-P109*(1-I$6)),P109*(1-$I$6)+(C109-D109)/C109*(K109-P109*(1-I$6))))","v":12.826567001504452},12.826567001504452,12.826567001504452,{"$f":"K109-(G109/C109)*K109*95.1%","v":12.826567001504452},{"$f":"MIN(K109,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K109-(G109/(C109-G109))*(Q109)*95%,K109-(G109/(C109-G109))*(P109)*84%))","v":12.826567001504452},12.826567001504452,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H109/C109*K109,IF(OPFOKLEGHEN!$H$20=\"ja\",O109-(K109-Q109)-(K109-S109),Q109-(K109-O109)-(K109-S109)))","v":12.826567001504452},{"$f":"IF(H109=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q109-(K109-R109)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O109*80%-(K109-S109)),(Q109-(K109-S109)-(K109-T109))),(N109-(K109-S109))))","v":25.653134003008905},{"$f":"IF(H109=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q109-(K109-R109)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O109*80%-(K109-S109)),(Q109-(K109-S109)-(K109-N109))),(N109-(K109-S109))))","v":25.653134003008905},{"$f":"IF(H109=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q109-(K109-R109)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O109-(K109-S109)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N109-(K109-Q109)-(K109-S109)),(Q109-(K109-N109/80%)))))),(O109-(K109-S109))))","v":25.653134003008905},1,null,null,{"$f":"IF(H109=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P109-(K109-R109),K109-(K109-O109)/I$6-(K109-R109)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K109-O109)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O109-(K109-S109),IF(OPFOKLEGHEN!$H$20=\"nee\",(O109-(K109-S109)),(O109-(K109-S109)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O109*80%-(K109-S109),0+O109-(K109-S109)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O109*80%-(K109-S109)),O109*93%-(K109-S109)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O109-(K109-S109))),O109-(K109-S109))))))))","v":12.826567001504452},{"$f":"IF(H109=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q109-(K109-R109),N109-(K109-R109)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q109-(K109-N109)-(K109-S109),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q109-(K109-N109)-(K109-S109)),(O109-(K109-S109)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q109*$N$135-(K109-N109)-(K109-S109),(Q109-(K109-N109)-(K109-S109))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N109*95%-(K109-Q109)/I$4-(K109-S109)),N109-(K109-Q109)/I$4-(K109-S109)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N109-(K109-Q109)/I$4-(K109-S109))),N109-(K109-Q109)/I$4-(K109-S109))))))))","v":12.826567001504452},null,null,null,null,null,null,null,null,14,94,1094.2000000000003,977.89999999999986,1036.0500000000002]
[14,95,1.263830805387256,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C110)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C110<$I$3,C110-D110,MIN($I$3,C110-D110))))","v":0},{"$f":"IF(C110<$I$7,MAX(0,C110-D110-E110-F110,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C110-D110-F110)),MIN(I$7,MAX(0,C110-D110-E110-F110))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C110-D110-E110-F110,MIN(I$7,C110-E110-F110)),MIN(I$7,MAX(0,C110-D110-F110))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C110-F110-G110,C110-D110-F110-G110),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C110-G110,IF(OPFOKLEGHEN!$J$18=\"nee\",C110-D110-G110)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C110-G110,C110-D110-F110-G110),C110-D110-F110-G110))","v":1.263830805387256},1.263830805387256,1.1957144552099792,13.237943483365017,{"$f":"SUM(K$16:K110)/$K$137","v":0.43585724176629254},0.14356217247941513,13.237943483365017,{"$f":"IF(E110<I$3,P110*(1-I$6*D110/C110),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P110*(1-$I$6)+(C110-D110)/C110*(K110-P110*(1-I$6)),P110*(1-$I$6)+(C110-D110)/C110*(K110-P110*(1-I$6))))","v":13.237943483365017},13.237943483365017,13.237943483365017,{"$f":"K110-(G110/C110)*K110*95.1%","v":13.237943483365017},{"$f":"MIN(K110,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K110-(G110/(C110-G110))*(Q110)*95%,K110-(G110/(C110-G110))*(P110)*84%))","v":13.237943483365017},13.237943483365017,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H110/C110*K110,IF(OPFOKLEGHEN!$H$20=\"ja\",O110-(K110-Q110)-(K110-S110),Q110-(K110-O110)-(K110-S110)))","v":13.237943483365017},{"$f":"IF(H110=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q110-(K110-R110)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O110*80%-(K110-S110)),(Q110-(K110-S110)-(K110-T110))),(N110-(K110-S110))))","v":26.475886966730034},{"$f":"IF(H110=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q110-(K110-R110)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O110*80%-(K110-S110)),(Q110-(K110-S110)-(K110-N110))),(N110-(K110-S110))))","v":26.475886966730034},{"$f":"IF(H110=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q110-(K110-R110)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O110-(K110-S110)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N110-(K110-Q110)-(K110-S110)),(Q110-(K110-N110/80%)))))),(O110-(K110-S110))))","v":26.475886966730034},1,null,null,{"$f":"IF(H110=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P110-(K110-R110),K110-(K110-O110)/I$6-(K110-R110)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K110-O110)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O110-(K110-S110),IF(OPFOKLEGHEN!$H$20=\"nee\",(O110-(K110-S110)),(O110-(K110-S110)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O110*80%-(K110-S110),0+O110-(K110-S110)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O110*80%-(K110-S110)),O110*93%-(K110-S110)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O110-(K110-S110))),O110-(K110-S110))))))))","v":13.237943483365017},{"$f":"IF(H110=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q110-(K110-R110),N110-(K110-R110)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q110-(K110-N110)-(K110-S110),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q110-(K110-N110)-(K110-S110)),(O110-(K110-S110)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q110*$N$135-(K110-N110)-(K110-S110),(Q110-(K110-N110)-(K110-S110))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N110*95%-(K110-Q110)/I$4-(K110-S110)),N110-(K110-Q110)/I$4-(K110-S110)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N110-(K110-Q110)/I$4-(K110-S110))),N110-(K110-Q110)/I$4-(K110-S110))))))))","v":13.237943483365017},null,null,null,null,null,null,null,null,14,95,1105.6000000000004,987.19999999999982,1046.4000000000001]
[14,96,1.2805496188802499,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C111)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C111<$I$3,C111-D111,MIN($I$3,C111-D111))))","v":0},{"$f":"IF(C111<$I$7,MAX(0,C111-D111-E111-F111,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C111-D111-F111)),MIN(I$7,MAX(0,C111-D111-E111-F111))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C111-D111-E111-F111,MIN(I$7,C111-E111-F111)),MIN(I$7,MAX(0,C111-D111-F111))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C111-F111-G111,C111-D111-F111-G111),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C111-G111,IF(OPFOKLEGHEN!$J$18=\"nee\",C111-D111-G111)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C111-G111,C111-D111-F111-G111),C111-D111-F111-G111))","v":1.2805496188802499},1.2805496188802499,1.2179192589119072,13.662148935160657,{"$f":"SUM(K$16:K111)/$K$137","v":0.45185616627314246},0.14972218011134966,13.662148935160657,{"$f":"IF(E111<I$3,P111*(1-I$6*D111/C111),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P111*(1-$I$6)+(C111-D111)/C111*(K111-P111*(1-I$6)),P111*(1-$I$6)+(C111-D111)/C111*(K111-P111*(1-I$6))))","v":13.662148935160657},13.662148935160657,13.662148935160657,13.662148935160657,{"$f":"MIN(K111,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K111-(G111/(C111-G111))*(Q111)*95%,K111-(G111/(C111-G111))*(P111)*84%))","v":13.662148935160657},13.662148935160657,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H111/C111*K111,IF(OPFOKLEGHEN!$H$20=\"ja\",O111-(K111-Q111)-(K111-S111),Q111-(K111-O111)-(K111-S111)))","v":13.662148935160657},{"$f":"IF(H111=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q111-(K111-R111)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O111*80%-(K111-S111)),(Q111-(K111-S111)-(K111-T111))),(N111-(K111-S111))))","v":27.324297870321313},{"$f":"IF(H111=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q111-(K111-R111)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O111*80%-(K111-S111)),(Q111-(K111-S111)-(K111-N111))),(N111-(K111-S111))))","v":27.324297870321313},{"$f":"IF(H111=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q111-(K111-R111)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O111-(K111-S111)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N111-(K111-Q111)-(K111-S111)),(Q111-(K111-N111/80%)))))),(O111-(K111-S111))))","v":27.324297870321313},1,null,null,{"$f":"IF(H111=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P111-(K111-R111),K111-(K111-O111)/I$6-(K111-R111)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K111-O111)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O111-(K111-S111),IF(OPFOKLEGHEN!$H$20=\"nee\",(O111-(K111-S111)),(O111-(K111-S111)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O111*80%-(K111-S111),0+O111-(K111-S111)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O111*80%-(K111-S111)),O111*93%-(K111-S111)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O111-(K111-S111))),O111-(K111-S111))))))))","v":13.662148935160657},{"$f":"IF(H111=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q111-(K111-R111),N111-(K111-R111)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q111-(K111-N111)-(K111-S111),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q111-(K111-N111)-(K111-S111)),(O111-(K111-S111)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q111*$N$135-(K111-N111)-(K111-S111),(Q111-(K111-N111)-(K111-S111))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N111*95%-(K111-Q111)/I$4-(K111-S111)),N111-(K111-Q111)/I$4-(K111-S111)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N111-(K111-Q111)/I$4-(K111-S111))),N111-(K111-Q111)/I$4-(K111-S111))))))))","v":13.662148935160657},null,null,null,null,null,null,null,null,14,96,1117.0000000000005,996.49999999999977,1056.75]
[14,97,1.2974559635926843,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C112)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C112<$I$3,C112-D112,MIN($I$3,C112-D112))))","v":0},{"$f":"IF(C112<$I$7,MAX(0,C112-D112-E112-F112,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C112-D112-F112)),MIN(I$7,MAX(0,C112-D112-E112-F112))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C112-D112-E112-F112,MIN(I$7,C112-E112-F112)),MIN(I$7,MAX(0,C112-D112-F112))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C112-F112-G112,C112-D112-F112-G112),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C112-G112,IF(OPFOKLEGHEN!$J$18=\"nee\",C112-D112-G112)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C112-G112,C112-D112-F112-G112),C112-D112-F112-G112))","v":1.2974559635926843},1.2974559635926843,1.2405364129917138,14.099582375708192,{"$f":"SUM(K$16:K112)/$K$137","v":0.4683673428880103},0.1561255126077277,{"$f":"(((($K112)*(1-($I$6*(D112)/C112)))))","v":14.099582375708192},{"$f":"IF(E112<I$3,P112*(1-I$6*D112/C112),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P112*(1-$I$6)+(C112-D112)/C112*(K112-P112*(1-I$6)),P112*(1-$I$6)+(C112-D112)/C112*(K112-P112*(1-I$6))))","v":14.099582375708192},{"$f":"IF(E112=0,K112,K112-K112*I$4*E112/C112)","v":14.099582375708192},{"$f":"IF(F112=0,K112,K112-K112*I$4*F112/C112)","v":14.099582375708192},14.099582375708192,{"$f":"MIN(K112,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K112-(G112/(C112-G112))*(Q112)*95%,K112-(G112/(C112-G112))*(P112)*84%))","v":14.099582375708192},14.099582375708192,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H112/C112*K112,IF(OPFOKLEGHEN!$H$20=\"ja\",O112-(K112-Q112)-(K112-S112),Q112-(K112-O112)-(K112-S112)))","v":14.099582375708192},{"$f":"IF(H112=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q112-(K112-R112)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O112*80%-(K112-S112)),(Q112-(K112-S112)-(K112-T112))),(N112-(K112-S112))))","v":28.199164751416383},{"$f":"IF(H112=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q112-(K112-R112)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O112*80%-(K112-S112)),(Q112-(K112-S112)-(K112-N112))),(N112-(K112-S112))))","v":28.199164751416383},{"$f":"IF(H112=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q112-(K112-R112)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O112-(K112-S112)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N112-(K112-Q112)-(K112-S112)),(Q112-(K112-N112/80%)))))),(O112-(K112-S112))))","v":28.199164751416383},{"$f":"Q112/K112","v":1},null,null,{"$f":"IF(H112=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P112-(K112-R112),K112-(K112-O112)/I$6-(K112-R112)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K112-O112)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O112-(K112-S112),IF(OPFOKLEGHEN!$H$20=\"nee\",(O112-(K112-S112)),(O112-(K112-S112)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O112*80%-(K112-S112),0+O112-(K112-S112)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O112*80%-(K112-S112)),O112*93%-(K112-S112)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O112-(K112-S112))),O112-(K112-S112))))))))","v":14.099582375708192},{"$f":"IF(H112=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q112-(K112-R112),N112-(K112-R112)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q112-(K112-N112)-(K112-S112),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q112-(K112-N112)-(K112-S112)),(O112-(K112-S112)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q112*$N$135-(K112-N112)-(K112-S112),(Q112-(K112-N112)-(K112-S112))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N112*95%-(K112-Q112)/I$4-(K112-S112)),N112-(K112-Q112)/I$4-(K112-S112)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N112-(K112-Q112)/I$4-(K112-S112))),N112-(K112-Q112)/I$4-(K112-S112))))))))","v":14.099582375708192},null,null,null,null,null,null,null,null,14,97,1128.4000000000005,1005.7999999999997,1067.1000000000001]
[14,98,1.3146354509675,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C113)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C113<$I$3,C113-D113,MIN($I$3,C113-D113))))","v":0},{"$f":"IF(C113<$I$7,MAX(0,C113-D113-E113-F113,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C113-D113-F113)),MIN(I$7,MAX(0,C113-D113-E113-F113))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C113-D113-E113-F113,MIN(I$7,C113-E113-F113)),MIN(I$7,MAX(0,C113-D113-F113))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C113-F113-G113,C113-D113-F113-G113),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C113-G113,IF(OPFOKLEGHEN!$J$18=\"nee\",C113-D113-G113)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C113-G113,C113-D113-F113-G113),C113-D113-F113-G113))","v":1.3146354509675},1.3146354509675,1.2635735749291241,14.551574280606271,{"$f":"SUM(K$16:K113)/$K$137","v":0.48540782015671319},0.16279158441774139,14.551574280606271,{"$f":"IF(E113<I$3,P113*(1-I$6*D113/C113),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P113*(1-$I$6)+(C113-D113)/C113*(K113-P113*(1-I$6)),P113*(1-$I$6)+(C113-D113)/C113*(K113-P113*(1-I$6))))","v":14.551574280606271},14.551574280606271,14.551574280606271,14.551574280606271,{"$f":"MIN(K113,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K113-(G113/(C113-G113))*(Q113)*95%,K113-(G113/(C113-G113))*(P113)*84%))","v":14.551574280606271},14.551574280606271,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H113/C113*K113,IF(OPFOKLEGHEN!$H$20=\"ja\",O113-(K113-Q113)-(K113-S113),Q113-(K113-O113)-(K113-S113)))","v":14.551574280606271},{"$f":"IF(H113=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q113-(K113-R113)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O113*80%-(K113-S113)),(Q113-(K113-S113)-(K113-T113))),(N113-(K113-S113))))","v":29.103148561212542},{"$f":"IF(H113=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q113-(K113-R113)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O113*80%-(K113-S113)),(Q113-(K113-S113)-(K113-N113))),(N113-(K113-S113))))","v":29.103148561212542},{"$f":"IF(H113=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q113-(K113-R113)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O113-(K113-S113)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N113-(K113-Q113)-(K113-S113)),(Q113-(K113-N113/80%)))))),(O113-(K113-S113))))","v":29.103148561212542},1,null,null,{"$f":"IF(H113=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P113-(K113-R113),K113-(K113-O113)/I$6-(K113-R113)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K113-O113)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O113-(K113-S113),IF(OPFOKLEGHEN!$H$20=\"nee\",(O113-(K113-S113)),(O113-(K113-S113)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O113*80%-(K113-S113),0+O113-(K113-S113)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O113*80%-(K113-S113)),O113*93%-(K113-S113)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O113-(K113-S113))),O113-(K113-S113))))))))","v":14.551574280606271},{"$f":"IF(H113=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q113-(K113-R113),N113-(K113-R113)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q113-(K113-N113)-(K113-S113),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q113-(K113-N113)-(K113-S113)),(O113-(K113-S113)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q113*$N$135-(K113-N113)-(K113-S113),(Q113-(K113-N113)-(K113-S113))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N113*95%-(K113-Q113)/I$4-(K113-S113)),N113-(K113-Q113)/I$4-(K113-S113)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N113-(K113-Q113)/I$4-(K113-S113))),N113-(K113-Q113)/I$4-(K113-S113))))))))","v":14.551574280606271},null,null,null,null,null,null,null,null,14,98,1140,1015,1077.5]
[15,99,1.331925458405774,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C114)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C114<$I$3,C114-D114,MIN($I$3,C114-D114))))","v":0},{"$f":"IF(C114<$I$7,MAX(0,C114-D114-E114-F114,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C114-D114-F114)),MIN(I$7,MAX(0,C114-D114-E114-F114))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C114-D114-E114-F114,MIN(I$7,C114-E114-F114)),MIN(I$7,MAX(0,C114-D114-F114))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C114-F114-G114,C114-D114-F114-G114),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C114-G114,IF(OPFOKLEGHEN!$J$18=\"nee\",C114-D114-G114)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C114-G114,C114-D114-F114-G114),C114-D114-F114-G114))","v":1.331925458405774},1.331925458405774,1.2870385444057348,15.016737172413135,{"$f":"SUM(K$16:K114)/$K$137","v":0.5029930218333204},0.16970970092110732,15.016737172413135,{"$f":"IF(E114<I$3,P114*(1-I$6*D114/C114),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P114*(1-$I$6)+(C114-D114)/C114*(K114-P114*(1-I$6)),P114*(1-$I$6)+(C114-D114)/C114*(K114-P114*(1-I$6))))","v":15.016737172413135},15.016737172413135,15.016737172413135,15.016737172413135,{"$f":"MIN(K114,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K114-(G114/(C114-G114))*(Q114)*95%,K114-(G114/(C114-G114))*(P114)*84%))","v":15.016737172413135},{"$f":"$K114*(1-($I$6*(D114)/C114))-($I$4*F114/C114)","v":15.016737172413135},0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H114/C114*K114,IF(OPFOKLEGHEN!$H$20=\"ja\",O114-(K114-Q114)-(K114-S114),Q114-(K114-O114)-(K114-S114)))","v":15.016737172413135},{"$f":"IF(H114=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q114-(K114-R114)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O114*80%-(K114-S114)),(Q114-(K114-S114)-(K114-T114))),(N114-(K114-S114))))","v":30.033474344826271},{"$f":"IF(H114=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q114-(K114-R114)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O114*80%-(K114-S114)),(Q114-(K114-S114)-(K114-N114))),(N114-(K114-S114))))","v":30.033474344826271},{"$f":"IF(H114=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q114-(K114-R114)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O114-(K114-S114)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N114-(K114-Q114)-(K114-S114)),(Q114-(K114-N114/80%)))))),(O114-(K114-S114))))","v":30.033474344826271},1,null,null,{"$f":"IF(H114=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P114-(K114-R114),K114-(K114-O114)/I$6-(K114-R114)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K114-O114)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O114-(K114-S114),IF(OPFOKLEGHEN!$H$20=\"nee\",(O114-(K114-S114)),(O114-(K114-S114)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O114*80%-(K114-S114),0+O114-(K114-S114)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O114*80%-(K114-S114)),O114*93%-(K114-S114)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O114-(K114-S114))),O114-(K114-S114))))))))","v":15.016737172413135},{"$f":"IF(H114=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q114-(K114-R114),N114-(K114-R114)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q114-(K114-N114)-(K114-S114),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q114-(K114-N114)-(K114-S114)),(O114-(K114-S114)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q114*$N$135-(K114-N114)-(K114-S114),(Q114-(K114-N114)-(K114-S114))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N114*95%-(K114-Q114)/I$4-(K114-S114)),N114-(K114-Q114)/I$4-(K114-S114)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N114-(K114-Q114)/I$4-(K114-S114))),N114-(K114-Q114)/I$4-(K114-S114))))))))","v":15.016737172413135},null,null,null,null,null,null,null,null,15,99,{"$f":"AO113+12.1","v":1152.0999999999999},{"$f":"AP113+8.6","v":1023.6},1087.8499999999999]
[15,100,1.3494106728619515,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C115)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C115<$I$3,C115-D115,MIN($I$3,C115-D115))))","v":0},{"$f":"IF(C115<$I$7,MAX(0,C115-D115-E115-F115,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C115-D115-F115)),MIN(I$7,MAX(0,C115-D115-E115-F115))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C115-D115-E115-F115,MIN(I$7,C115-E115-F115)),MIN(I$7,MAX(0,C115-D115-F115))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C115-F115-G115,C115-D115-F115-G115),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C115-G115,IF(OPFOKLEGHEN!$J$18=\"nee\",C115-D115-G115)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C115-G115,C115-D115-F115-G115),C115-D115-F115-G115))","v":1.3494106728619515},1.3494106728619515,1.3109392659457497,15.496400027603221,{"$f":"SUM(K$16:K115)/$K$137","v":0.52113992795666919},0.17689954369410069,15.496400027603221,{"$f":"IF(E115<I$3,P115*(1-I$6*D115/C115),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P115*(1-$I$6)+(C115-D115)/C115*(K115-P115*(1-I$6)),P115*(1-$I$6)+(C115-D115)/C115*(K115-P115*(1-I$6))))","v":15.496400027603221},15.496400027603221,15.496400027603221,15.496400027603221,{"$f":"MIN(K115,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K115-(G115/(C115-G115))*(Q115)*95%,K115-(G115/(C115-G115))*(P115)*84%))","v":15.496400027603221},15.496400027603221,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H115/C115*K115,IF(OPFOKLEGHEN!$H$20=\"ja\",O115-(K115-Q115)-(K115-S115),Q115-(K115-O115)-(K115-S115)))","v":15.496400027603221},{"$f":"IF(H115=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q115-(K115-R115)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O115*80%-(K115-S115)),(Q115-(K115-S115)-(K115-T115))),(N115-(K115-S115))))","v":30.992800055206441},{"$f":"IF(H115=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q115-(K115-R115)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O115*80%-(K115-S115)),(Q115-(K115-S115)-(K115-N115))),(N115-(K115-S115))))","v":30.992800055206441},{"$f":"IF(H115=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q115-(K115-R115)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O115-(K115-S115)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N115-(K115-Q115)-(K115-S115)),(Q115-(K115-N115/80%)))))),(O115-(K115-S115))))","v":30.992800055206441},1,null,null,{"$f":"IF(H115=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P115-(K115-R115),K115-(K115-O115)/I$6-(K115-R115)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K115-O115)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O115-(K115-S115),IF(OPFOKLEGHEN!$H$20=\"nee\",(O115-(K115-S115)),(O115-(K115-S115)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O115*80%-(K115-S115),0+O115-(K115-S115)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O115*80%-(K115-S115)),O115*93%-(K115-S115)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O115-(K115-S115))),O115-(K115-S115))))))))","v":15.496400027603221},{"$f":"IF(H115=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q115-(K115-R115),N115-(K115-R115)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q115-(K115-N115)-(K115-S115),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q115-(K115-N115)-(K115-S115)),(O115-(K115-S115)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q115*$N$135-(K115-N115)-(K115-S115),(Q115-(K115-N115)-(K115-S115))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N115*95%-(K115-Q115)/I$4-(K115-S115)),N115-(K115-Q115)/I$4-(K115-S115)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N115-(K115-Q115)/I$4-(K115-S115))),N115-(K115-Q115)/I$4-(K115-S115))))))))","v":15.496400027603221},null,null,null,null,null,null,null,null,15,100,1164.1999999999998,1032.2,1098.1999999999998]
[15,101,1.3670936488220173,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C116)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C116<$I$3,C116-D116,MIN($I$3,C116-D116))))","v":0},{"$f":"IF(C116<$I$7,MAX(0,C116-D116-E116-F116,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C116-D116-F116)),MIN(I$7,MAX(0,C116-D116-E116-F116))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C116-D116-E116-F116,MIN(I$7,C116-E116-F116)),MIN(I$7,MAX(0,C116-D116-F116))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C116-F116-G116,C116-D116-F116-G116),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C116-G116,IF(OPFOKLEGHEN!$J$18=\"nee\",C116-D116-G116)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C116-G116,C116-D116-F116-G116),C116-D116-F116-G116))","v":1.3670936488220173},1.3670936488220173,1.3352838316057536,15.991012479131474,{"$f":"SUM(K$16:K116)/$K$137","v":0.53986604510382585},0.18437126260185832,15.991012479131474,{"$f":"IF(E116<I$3,P116*(1-I$6*D116/C116),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P116*(1-$I$6)+(C116-D116)/C116*(K116-P116*(1-I$6)),P116*(1-$I$6)+(C116-D116)/C116*(K116-P116*(1-I$6))))","v":15.991012479131474},15.991012479131474,15.991012479131474,15.991012479131474,{"$f":"MIN(K116,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K116-(G116/(C116-G116))*(Q116)*95%,K116-(G116/(C116-G116))*(P116)*84%))","v":15.991012479131474},15.991012479131474,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H116/C116*K116,IF(OPFOKLEGHEN!$H$20=\"ja\",O116-(K116-Q116)-(K116-S116),Q116-(K116-O116)-(K116-S116)))","v":15.991012479131474},{"$f":"IF(H116=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q116-(K116-R116)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O116*80%-(K116-S116)),(Q116-(K116-S116)-(K116-T116))),(N116-(K116-S116))))","v":31.982024958262947},{"$f":"IF(H116=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q116-(K116-R116)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O116*80%-(K116-S116)),(Q116-(K116-S116)-(K116-N116))),(N116-(K116-S116))))","v":31.982024958262947},{"$f":"IF(H116=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q116-(K116-R116)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O116-(K116-S116)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N116-(K116-Q116)-(K116-S116)),(Q116-(K116-N116/80%)))))),(O116-(K116-S116))))","v":31.982024958262947},1,null,null,{"$f":"IF(H116=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P116-(K116-R116),K116-(K116-O116)/I$6-(K116-R116)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K116-O116)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O116-(K116-S116),IF(OPFOKLEGHEN!$H$20=\"nee\",(O116-(K116-S116)),(O116-(K116-S116)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O116*80%-(K116-S116),0+O116-(K116-S116)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O116*80%-(K116-S116)),O116*93%-(K116-S116)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O116-(K116-S116))),O116-(K116-S116))))))))","v":15.991012479131474},{"$f":"IF(H116=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q116-(K116-R116),N116-(K116-R116)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q116-(K116-N116)-(K116-S116),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q116-(K116-N116)-(K116-S116)),(O116-(K116-S116)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q116*$N$135-(K116-N116)-(K116-S116),(Q116-(K116-N116)-(K116-S116))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N116*95%-(K116-Q116)/I$4-(K116-S116)),N116-(K116-Q116)/I$4-(K116-S116)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N116-(K116-Q116)/I$4-(K116-S116))),N116-(K116-Q116)/I$4-(K116-S116))))))))","v":15.991012479131474},null,null,null,null,null,null,null,null,15,101,1176.2999999999997,1040.8,1108.5499999999997]
[15,102,1.3849769407719552,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C117)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C117<$I$3,C117-D117,MIN($I$3,C117-D117))))","v":0},{"$f":"IF(C117<$I$7,MAX(0,C117-D117-E117-F117,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C117-D117-F117)),MIN(I$7,MAX(0,C117-D117-E117-F117))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C117-D117-E117-F117,MIN(I$7,C117-E117-F117)),MIN(I$7,MAX(0,C117-D117-F117))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C117-F117-G117,C117-D117-F117-G117),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C117-G117,IF(OPFOKLEGHEN!$J$18=\"nee\",C117-D117-G117)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C117-G117,C117-D117-F117-G117),C117-D117-F117-G117))","v":1.3849769407719552},1.3849769407719552,1.3600804837144354,16.501037742036907,{"$f":"SUM(K$16:K117)/$K$137","v":0.55918942229525048},0.19213537096892289,16.501037742036907,{"$f":"IF(E117<I$3,P117*(1-I$6*D117/C117),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P117*(1-$I$6)+(C117-D117)/C117*(K117-P117*(1-I$6)),P117*(1-$I$6)+(C117-D117)/C117*(K117-P117*(1-I$6))))","v":16.501037742036907},16.501037742036907,16.501037742036907,16.501037742036907,{"$f":"MIN(K117,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K117-(G117/(C117-G117))*(Q117)*95%,K117-(G117/(C117-G117))*(P117)*84%))","v":16.501037742036907},16.501037742036907,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H117/C117*K117,IF(OPFOKLEGHEN!$H$20=\"ja\",O117-(K117-Q117)-(K117-S117),Q117-(K117-O117)-(K117-S117)))","v":16.501037742036907},{"$f":"IF(H117=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q117-(K117-R117)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O117*80%-(K117-S117)),(Q117-(K117-S117)-(K117-T117))),(N117-(K117-S117))))","v":33.002075484073814},{"$f":"IF(H117=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q117-(K117-R117)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O117*80%-(K117-S117)),(Q117-(K117-S117)-(K117-N117))),(N117-(K117-S117))))","v":33.002075484073814},{"$f":"IF(H117=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q117-(K117-R117)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O117-(K117-S117)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N117-(K117-Q117)-(K117-S117)),(Q117-(K117-N117/80%)))))),(O117-(K117-S117))))","v":33.002075484073814},1,null,null,{"$f":"IF(H117=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P117-(K117-R117),K117-(K117-O117)/I$6-(K117-R117)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K117-O117)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O117-(K117-S117),IF(OPFOKLEGHEN!$H$20=\"nee\",(O117-(K117-S117)),(O117-(K117-S117)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O117*80%-(K117-S117),0+O117-(K117-S117)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O117*80%-(K117-S117)),O117*93%-(K117-S117)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O117-(K117-S117))),O117-(K117-S117))))))))","v":16.501037742036907},{"$f":"IF(H117=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q117-(K117-R117),N117-(K117-R117)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q117-(K117-N117)-(K117-S117),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q117-(K117-N117)-(K117-S117)),(O117-(K117-S117)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q117*$N$135-(K117-N117)-(K117-S117),(Q117-(K117-N117)-(K117-S117))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N117*95%-(K117-Q117)/I$4-(K117-S117)),N117-(K117-Q117)/I$4-(K117-S117)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N117-(K117-Q117)/I$4-(K117-S117))),N117-(K117-Q117)/I$4-(K117-S117))))))))","v":16.501037742036907},null,null,null,null,null,null,null,null,15,102,1188.3999999999996,1049.3999999999999,1118.8999999999996]
[15,103,1.403063103197749,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C118)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C118<$I$3,C118-D118,MIN($I$3,C118-D118))))","v":0},{"$f":"IF(C118<$I$7,MAX(0,C118-D118-E118-F118,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C118-D118-F118)),MIN(I$7,MAX(0,C118-D118-E118-F118))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C118-D118-E118-F118,MIN(I$7,C118-E118-F118)),MIN(I$7,MAX(0,C118-D118-F118))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C118-F118-G118,C118-D118-F118-G118),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C118-G118,IF(OPFOKLEGHEN!$J$18=\"nee\",C118-D118-G118)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C118-G118,C118-D118-F118-G118),C118-D118-F118-G118))","v":1.403063103197749},1.403063103197749,1.3853376176631913,17.026953008100222,{"$f":"SUM(K$16:K118)/$K$137","v":0.57912866736212276},0.20020275797195466,17.026953008100222,{"$f":"IF(E118<I$3,P118*(1-I$6*D118/C118),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P118*(1-$I$6)+(C118-D118)/C118*(K118-P118*(1-I$6)),P118*(1-$I$6)+(C118-D118)/C118*(K118-P118*(1-I$6))))","v":17.026953008100222},17.026953008100222,17.026953008100222,17.026953008100222,{"$f":"MIN(K118,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K118-(G118/(C118-G118))*(Q118)*95%,K118-(G118/(C118-G118))*(P118)*84%))","v":17.026953008100222},17.026953008100222,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H118/C118*K118,IF(OPFOKLEGHEN!$H$20=\"ja\",O118-(K118-Q118)-(K118-S118),Q118-(K118-O118)-(K118-S118)))","v":17.026953008100222},{"$f":"IF(H118=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q118-(K118-R118)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O118*80%-(K118-S118)),(Q118-(K118-S118)-(K118-T118))),(N118-(K118-S118))))","v":34.053906016200443},{"$f":"IF(H118=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q118-(K118-R118)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O118*80%-(K118-S118)),(Q118-(K118-S118)-(K118-N118))),(N118-(K118-S118))))","v":34.053906016200443},{"$f":"IF(H118=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q118-(K118-R118)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O118-(K118-S118)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N118-(K118-Q118)-(K118-S118)),(Q118-(K118-N118/80%)))))),(O118-(K118-S118))))","v":34.053906016200443},1,null,null,{"$f":"IF(H118=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P118-(K118-R118),K118-(K118-O118)/I$6-(K118-R118)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K118-O118)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O118-(K118-S118),IF(OPFOKLEGHEN!$H$20=\"nee\",(O118-(K118-S118)),(O118-(K118-S118)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O118*80%-(K118-S118),0+O118-(K118-S118)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O118*80%-(K118-S118)),O118*93%-(K118-S118)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O118-(K118-S118))),O118-(K118-S118))))))))","v":17.026953008100222},{"$f":"IF(H118=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q118-(K118-R118),N118-(K118-R118)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q118-(K118-N118)-(K118-S118),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q118-(K118-N118)-(K118-S118)),(O118-(K118-S118)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q118*$N$135-(K118-N118)-(K118-S118),(Q118-(K118-N118)-(K118-S118))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N118*95%-(K118-Q118)/I$4-(K118-S118)),N118-(K118-Q118)/I$4-(K118-S118)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N118-(K118-Q118)/I$4-(K118-S118))),N118-(K118-Q118)/I$4-(K118-S118))))))))","v":17.026953008100222},null,null,null,null,null,null,null,null,15,103,1200.4999999999995,1057.9999999999998,1129.2499999999995]
[15,104,1.4213546905853829,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C119)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C119<$I$3,C119-D119,MIN($I$3,C119-D119))))","v":0},{"$f":"IF(C119<$I$7,MAX(0,C119-D119-E119-F119,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C119-D119-F119)),MIN(I$7,MAX(0,C119-D119-E119-F119))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C119-D119-E119-F119,MIN(I$7,C119-E119-F119)),MIN(I$7,MAX(0,C119-D119-F119))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C119-F119-G119,C119-D119-F119-G119),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C119-G119,IF(OPFOKLEGHEN!$J$18=\"nee\",C119-D119-G119)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C119-G119,C119-D119-F119-G119),C119-D119-F119-G119))","v":1.4213546905853829},1.4213546905853829,1.4110637847485474,17.569249851507397,{"$f":"SUM(K$16:K119)/$K$137","v":0.59970296378871535},0.20858470143342114,17.569249851507397,{"$f":"IF(E119<I$3,P119*(1-I$6*D119/C119),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P119*(1-$I$6)+(C119-D119)/C119*(K119-P119*(1-I$6)),P119*(1-$I$6)+(C119-D119)/C119*(K119-P119*(1-I$6))))","v":17.569249851507397},17.569249851507397,17.569249851507397,17.569249851507397,{"$f":"MIN(K119,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K119-(G119/(C119-G119))*(Q119)*95%,K119-(G119/(C119-G119))*(P119)*84%))","v":17.569249851507397},17.569249851507397,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H119/C119*K119,IF(OPFOKLEGHEN!$H$20=\"ja\",O119-(K119-Q119)-(K119-S119),Q119-(K119-O119)-(K119-S119)))","v":17.569249851507397},{"$f":"IF(H119=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q119-(K119-R119)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O119*80%-(K119-S119)),(Q119-(K119-S119)-(K119-T119))),(N119-(K119-S119))))","v":35.138499703014794},{"$f":"IF(H119=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q119-(K119-R119)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O119*80%-(K119-S119)),(Q119-(K119-S119)-(K119-N119))),(N119-(K119-S119))))","v":35.138499703014794},{"$f":"IF(H119=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q119-(K119-R119)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O119-(K119-S119)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N119-(K119-Q119)-(K119-S119)),(Q119-(K119-N119/80%)))))),(O119-(K119-S119))))","v":35.138499703014794},1,null,null,{"$f":"IF(H119=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P119-(K119-R119),K119-(K119-O119)/I$6-(K119-R119)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K119-O119)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O119-(K119-S119),IF(OPFOKLEGHEN!$H$20=\"nee\",(O119-(K119-S119)),(O119-(K119-S119)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O119*80%-(K119-S119),0+O119-(K119-S119)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O119*80%-(K119-S119)),O119*93%-(K119-S119)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O119-(K119-S119))),O119-(K119-S119))))))))","v":17.569249851507397},{"$f":"IF(H119=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q119-(K119-R119),N119-(K119-R119)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q119-(K119-N119)-(K119-S119),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q119-(K119-N119)-(K119-S119)),(O119-(K119-S119)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q119*$N$135-(K119-N119)-(K119-S119),(Q119-(K119-N119)-(K119-S119))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N119*95%-(K119-Q119)/I$4-(K119-S119)),N119-(K119-Q119)/I$4-(K119-S119)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N119-(K119-Q119)/I$4-(K119-S119))),N119-(K119-Q119)/I$4-(K119-S119))))))))","v":17.569249851507397},null,null,null,null,null,null,null,null,15,104,1212.5999999999995,1066.5999999999997,1139.5999999999995]
[15,105,1.4399441362450001,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C120)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C120<$I$3,C120-D120,MIN($I$3,C120-D120))))","v":0},{"$f":"IF(C120<$I$7,MAX(0,C120-D120-E120-F120,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C120-D120-F120)),MIN(I$7,MAX(0,C120-D120-E120-F120))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C120-D120-E120-F120,MIN(I$7,C120-E120-F120)),MIN(I$7,MAX(0,C120-D120-F120))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C120-F120-G120,C120-D120-F120-G120),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C120-G120,IF(OPFOKLEGHEN!$J$18=\"nee\",C120-D120-G120)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C120-G120,C120-D120-F120-G120),C120-D120-F120-G120))","v":1.4399441362450001},1.4399441362450001,1.4372676950673688,18.129566262005234,{"$f":"SUM(K$16:K120)/$K$137","v":0.62093341321100781},0.21730644492129556,18.129566262005234,{"$f":"IF(E120<I$3,P120*(1-I$6*D120/C120),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P120*(1-$I$6)+(C120-D120)/C120*(K120-P120*(1-I$6)),P120*(1-$I$6)+(C120-D120)/C120*(K120-P120*(1-I$6))))","v":18.129566262005234},18.129566262005234,18.129566262005234,18.129566262005234,{"$f":"MIN(K120,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K120-(G120/(C120-G120))*(Q120)*95%,K120-(G120/(C120-G120))*(P120)*84%))","v":18.129566262005234},18.129566262005234,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H120/C120*K120,IF(OPFOKLEGHEN!$H$20=\"ja\",O120-(K120-Q120)-(K120-S120),Q120-(K120-O120)-(K120-S120)))","v":18.129566262005234},{"$f":"IF(H120=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q120-(K120-R120)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O120*80%-(K120-S120)),(Q120-(K120-S120)-(K120-T120))),(N120-(K120-S120))))","v":36.259132524010468},{"$f":"IF(H120=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q120-(K120-R120)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O120*80%-(K120-S120)),(Q120-(K120-S120)-(K120-N120))),(N120-(K120-S120))))","v":36.259132524010468},{"$f":"IF(H120=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q120-(K120-R120)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O120-(K120-S120)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N120-(K120-Q120)-(K120-S120)),(Q120-(K120-N120/80%)))))),(O120-(K120-S120))))","v":36.259132524010468},1,null,null,{"$f":"IF(H120=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P120-(K120-R120),K120-(K120-O120)/I$6-(K120-R120)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K120-O120)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O120-(K120-S120),IF(OPFOKLEGHEN!$H$20=\"nee\",(O120-(K120-S120)),(O120-(K120-S120)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O120*80%-(K120-S120),0+O120-(K120-S120)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O120*80%-(K120-S120)),O120*93%-(K120-S120)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O120-(K120-S120))),O120-(K120-S120))))))))","v":18.129566262005234},{"$f":"IF(H120=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q120-(K120-R120),N120-(K120-R120)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q120-(K120-N120)-(K120-S120),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q120-(K120-N120)-(K120-S120)),(O120-(K120-S120)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q120*$N$135-(K120-N120)-(K120-S120),(Q120-(K120-N120)-(K120-S120))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N120*95%-(K120-Q120)/I$4-(K120-S120)),N120-(K120-Q120)/I$4-(K120-S120)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N120-(K120-Q120)/I$4-(K120-S120))),N120-(K120-Q120)/I$4-(K120-S120))))))))","v":18.129566262005234},null,null,null,null,null,null,null,null,15,105,1225,1075,1150]
[16,106,1.4586552602864737,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C121)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C121<$I$3,C121-D121,MIN($I$3,C121-D121))))","v":0},{"$f":"IF(C121<$I$7,MAX(0,C121-D121-E121-F121,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C121-D121-F121)),MIN(I$7,MAX(0,C121-D121-E121-F121))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C121-D121-E121-F121,MIN(I$7,C121-E121-F121)),MIN(I$7,MAX(0,C121-D121-F121))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C121-F121-G121,C121-D121-F121-G121),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C121-G121,IF(OPFOKLEGHEN!$J$18=\"nee\",C121-D121-G121)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C121-G121,C121-D121-F121-G121),C121-D121-F121-G121))","v":1.4586552602864737},1.4586552602864737,1.4639582204658335,18.706194745909716,{"$f":"SUM(K$16:K121)/$K$137","v":0.64283911772137392},0.22635349806694399,18.706194745909716,{"$f":"IF(E121<I$3,P121*(1-I$6*D121/C121),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P121*(1-$I$6)+(C121-D121)/C121*(K121-P121*(1-I$6)),P121*(1-$I$6)+(C121-D121)/C121*(K121-P121*(1-I$6))))","v":18.706194745909716},18.706194745909716,18.706194745909716,18.706194745909716,{"$f":"MIN(K121,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K121-(G121/(C121-G121))*(Q121)*95%,K121-(G121/(C121-G121))*(P121)*84%))","v":18.706194745909716},18.706194745909716,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H121/C121*K121,IF(OPFOKLEGHEN!$H$20=\"ja\",O121-(K121-Q121)-(K121-S121),Q121-(K121-O121)-(K121-S121)))","v":18.706194745909716},{"$f":"IF(H121=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q121-(K121-R121)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O121*80%-(K121-S121)),(Q121-(K121-S121)-(K121-T121))),(N121-(K121-S121))))","v":37.412389491819432},{"$f":"IF(H121=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q121-(K121-R121)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O121*80%-(K121-S121)),(Q121-(K121-S121)-(K121-N121))),(N121-(K121-S121))))","v":37.412389491819432},{"$f":"IF(H121=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q121-(K121-R121)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O121-(K121-S121)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N121-(K121-Q121)-(K121-S121)),(Q121-(K121-N121/80%)))))),(O121-(K121-S121))))","v":37.412389491819432},1,null,null,{"$f":"IF(H121=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P121-(K121-R121),K121-(K121-O121)/I$6-(K121-R121)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K121-O121)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O121-(K121-S121),IF(OPFOKLEGHEN!$H$20=\"nee\",(O121-(K121-S121)),(O121-(K121-S121)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O121*80%-(K121-S121),0+O121-(K121-S121)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O121*80%-(K121-S121)),O121*93%-(K121-S121)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O121-(K121-S121))),O121-(K121-S121))))))))","v":18.706194745909716},{"$f":"IF(H121=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q121-(K121-R121),N121-(K121-R121)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q121-(K121-N121)-(K121-S121),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q121-(K121-N121)-(K121-S121)),(O121-(K121-S121)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q121*$N$135-(K121-N121)-(K121-S121),(Q121-(K121-N121)-(K121-S121))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N121*95%-(K121-Q121)/I$4-(K121-S121)),N121-(K121-Q121)/I$4-(K121-S121)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N121-(K121-Q121)/I$4-(K121-S121))),N121-(K121-Q121)/I$4-(K121-S121))))))))","v":18.706194745909716},null,null,null,null,null,null,null,null,16,106,{"$f":"AO120+12.1","v":1237.0999999999999},{"$f":"AP120+8.6","v":1083.5999999999999},1160.3499999999999]
[16,107,1.4775794850882515,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C122)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C122<$I$3,C122-D122,MIN($I$3,C122-D122))))","v":0},{"$f":"IF(C122<$I$7,MAX(0,C122-D122-E122-F122,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C122-D122-F122)),MIN(I$7,MAX(0,C122-D122-E122-F122))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C122-D122-E122-F122,MIN(I$7,C122-E122-F122)),MIN(I$7,MAX(0,C122-D122-F122))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C122-F122-G122,C122-D122-F122-G122),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C122-G122,IF(OPFOKLEGHEN!$J$18=\"nee\",C122-D122-G122)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C122-G122,C122-D122-F122-G122),C122-D122-F122-G122))","v":1.4775794850882515},1.4775794850882515,1.4911443975431682,19.300771090959213,{"$f":"SUM(K$16:K122)/$K$137","v":0.66544109498525417},0.23575142770920501,19.300771090959213,{"$f":"IF(E122<I$3,P122*(1-I$6*D122/C122),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P122*(1-$I$6)+(C122-D122)/C122*(K122-P122*(1-I$6)),P122*(1-$I$6)+(C122-D122)/C122*(K122-P122*(1-I$6))))","v":19.300771090959213},19.300771090959213,19.300771090959213,19.300771090959213,{"$f":"MIN(K122,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K122-(G122/(C122-G122))*(Q122)*95%,K122-(G122/(C122-G122))*(P122)*84%))","v":19.300771090959213},19.300771090959213,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H122/C122*K122,IF(OPFOKLEGHEN!$H$20=\"ja\",O122-(K122-Q122)-(K122-S122),Q122-(K122-O122)-(K122-S122)))","v":19.300771090959213},{"$f":"IF(H122=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q122-(K122-R122)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O122*80%-(K122-S122)),(Q122-(K122-S122)-(K122-T122))),(N122-(K122-S122))))","v":38.601542181918425},{"$f":"IF(H122=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q122-(K122-R122)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O122*80%-(K122-S122)),(Q122-(K122-S122)-(K122-N122))),(N122-(K122-S122))))","v":38.601542181918425},{"$f":"IF(H122=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q122-(K122-R122)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O122-(K122-S122)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N122-(K122-Q122)-(K122-S122)),(Q122-(K122-N122/80%)))))),(O122-(K122-S122))))","v":38.601542181918425},1,null,null,{"$f":"IF(H122=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P122-(K122-R122),K122-(K122-O122)/I$6-(K122-R122)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K122-O122)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O122-(K122-S122),IF(OPFOKLEGHEN!$H$20=\"nee\",(O122-(K122-S122)),(O122-(K122-S122)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O122*80%-(K122-S122),0+O122-(K122-S122)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O122*80%-(K122-S122)),O122*93%-(K122-S122)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O122-(K122-S122))),O122-(K122-S122))))))))","v":19.300771090959213},{"$f":"IF(H122=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q122-(K122-R122),N122-(K122-R122)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q122-(K122-N122)-(K122-S122),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q122-(K122-N122)-(K122-S122)),(O122-(K122-S122)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q122*$N$135-(K122-N122)-(K122-S122),(Q122-(K122-N122)-(K122-S122))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N122*95%-(K122-Q122)/I$4-(K122-S122)),N122-(K122-Q122)/I$4-(K122-S122)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N122-(K122-Q122)/I$4-(K122-S122))),N122-(K122-Q122)/I$4-(K122-S122))))))))","v":19.300771090959213},null,null,null,null,null,null,null,null,16,107,1249.1999999999998,1092.1999999999998,1170.6999999999998]
[16,108,1.4967193651363173,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C123)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C123<$I$3,C123-D123,MIN($I$3,C123-D123))))","v":0},{"$f":"IF(C123<$I$7,MAX(0,C123-D123-E123-F123,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C123-D123-F123)),MIN(I$7,MAX(0,C123-D123-E123-F123))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C123-D123-E123-F123,MIN(I$7,C123-E123-F123)),MIN(I$7,MAX(0,C123-D123-F123))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C123-F123-G123,C123-D123-F123-G123),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C123-G123,IF(OPFOKLEGHEN!$J$18=\"nee\",C123-D123-G123)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C123-G123,C123-D123-F123-G123),C123-D123-F123-G123))","v":1.4967193651363173},1.4967193651363173,1.5188354307111678,19.91384871802094,{"$f":"SUM(K$16:K123)/$K$137","v":0.68876101074612717},0.24551320337286089,19.91384871802094,{"$f":"IF(E123<I$3,P123*(1-I$6*D123/C123),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P123*(1-$I$6)+(C123-D123)/C123*(K123-P123*(1-I$6)),P123*(1-$I$6)+(C123-D123)/C123*(K123-P123*(1-I$6))))","v":19.91384871802094},19.91384871802094,19.91384871802094,19.91384871802094,{"$f":"MIN(K123,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K123-(G123/(C123-G123))*(Q123)*95%,K123-(G123/(C123-G123))*(P123)*84%))","v":19.91384871802094},19.91384871802094,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H123/C123*K123,IF(OPFOKLEGHEN!$H$20=\"ja\",O123-(K123-Q123)-(K123-S123),Q123-(K123-O123)-(K123-S123)))","v":19.91384871802094},{"$f":"IF(H123=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q123-(K123-R123)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O123*80%-(K123-S123)),(Q123-(K123-S123)-(K123-T123))),(N123-(K123-S123))))","v":39.827697436041881},{"$f":"IF(H123=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q123-(K123-R123)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O123*80%-(K123-S123)),(Q123-(K123-S123)-(K123-N123))),(N123-(K123-S123))))","v":39.827697436041881},{"$f":"IF(H123=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q123-(K123-R123)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O123-(K123-S123)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N123-(K123-Q123)-(K123-S123)),(Q123-(K123-N123/80%)))))),(O123-(K123-S123))))","v":39.827697436041881},1,null,null,{"$f":"IF(H123=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P123-(K123-R123),K123-(K123-O123)/I$6-(K123-R123)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K123-O123)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O123-(K123-S123),IF(OPFOKLEGHEN!$H$20=\"nee\",(O123-(K123-S123)),(O123-(K123-S123)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O123*80%-(K123-S123),0+O123-(K123-S123)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O123*80%-(K123-S123)),O123*93%-(K123-S123)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O123-(K123-S123))),O123-(K123-S123))))))))","v":19.91384871802094},{"$f":"IF(H123=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q123-(K123-R123),N123-(K123-R123)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q123-(K123-N123)-(K123-S123),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q123-(K123-N123)-(K123-S123)),(O123-(K123-S123)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q123*$N$135-(K123-N123)-(K123-S123),(Q123-(K123-N123)-(K123-S123))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N123*95%-(K123-Q123)/I$4-(K123-S123)),N123-(K123-Q123)/I$4-(K123-S123)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N123-(K123-Q123)/I$4-(K123-S123))),N123-(K123-Q123)/I$4-(K123-S123))))))))","v":19.91384871802094},null,null,null,null,null,null,null,null,16,108,1261.2999999999997,1100.7999999999997,1181.0499999999997]
[16,109,1.5160774549166551,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C124)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C124<$I$3,C124-D124,MIN($I$3,C124-D124))))","v":0},{"$f":"IF(C124<$I$7,MAX(0,C124-D124-E124-F124,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C124-D124-F124)),MIN(I$7,MAX(0,C124-D124-E124-F124))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C124-D124-E124-F124,MIN(I$7,C124-E124-F124)),MIN(I$7,MAX(0,C124-D124-F124))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C124-F124-G124,C124-D124-F124-G124),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C124-G124,IF(OPFOKLEGHEN!$J$18=\"nee\",C124-D124-G124)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C124-G124,C124-D124-F124-G124),C124-D124-F124-G124))","v":1.5160774549166551},1.5160774549166551,1.5470406953105251,20.545997635190133,{"$f":"SUM(K$16:K124)/$K$137","v":0.71282119824981871},0.25565225367987721,20.545997635190133,{"$f":"IF(E124<I$3,P124*(1-I$6*D124/C124),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P124*(1-$I$6)+(C124-D124)/C124*(K124-P124*(1-I$6)),P124*(1-$I$6)+(C124-D124)/C124*(K124-P124*(1-I$6))))","v":20.545997635190133},20.545997635190133,20.545997635190133,20.545997635190133,{"$f":"MIN(K124,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K124-(G124/(C124-G124))*(Q124)*95%,K124-(G124/(C124-G124))*(P124)*84%))","v":20.545997635190133},20.545997635190133,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H124/C124*K124,IF(OPFOKLEGHEN!$H$20=\"ja\",O124-(K124-Q124)-(K124-S124),Q124-(K124-O124)-(K124-S124)))","v":20.545997635190133},{"$f":"IF(H124=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q124-(K124-R124)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O124*80%-(K124-S124)),(Q124-(K124-S124)-(K124-T124))),(N124-(K124-S124))))","v":41.091995270380266},{"$f":"IF(H124=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q124-(K124-R124)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O124*80%-(K124-S124)),(Q124-(K124-S124)-(K124-N124))),(N124-(K124-S124))))","v":41.091995270380266},{"$f":"IF(H124=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q124-(K124-R124)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O124-(K124-S124)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N124-(K124-Q124)-(K124-S124)),(Q124-(K124-N124/80%)))))),(O124-(K124-S124))))","v":41.091995270380266},1,null,null,{"$f":"IF(H124=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P124-(K124-R124),K124-(K124-O124)/I$6-(K124-R124)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K124-O124)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O124-(K124-S124),IF(OPFOKLEGHEN!$H$20=\"nee\",(O124-(K124-S124)),(O124-(K124-S124)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O124*80%-(K124-S124),0+O124-(K124-S124)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O124*80%-(K124-S124)),O124*93%-(K124-S124)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O124-(K124-S124))),O124-(K124-S124))))))))","v":20.545997635190133},{"$f":"IF(H124=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q124-(K124-R124),N124-(K124-R124)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q124-(K124-N124)-(K124-S124),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q124-(K124-N124)-(K124-S124)),(O124-(K124-S124)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q124*$N$135-(K124-N124)-(K124-S124),(Q124-(K124-N124)-(K124-S124))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N124*95%-(K124-Q124)/I$4-(K124-S124)),N124-(K124-Q124)/I$4-(K124-S124)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N124-(K124-Q124)/I$4-(K124-S124))),N124-(K124-Q124)/I$4-(K124-S124))))))))","v":20.545997635190133},null,null,null,null,null,null,null,null,16,109,1273.3999999999996,1109.3999999999996,1191.3999999999996]
[16,110,1.5356563089152491,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C125)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C125<$I$3,C125-D125,MIN($I$3,C125-D125))))","v":0},{"$f":"IF(C125<$I$7,MAX(0,C125-D125-E125-F125,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C125-D125-F125)),MIN(I$7,MAX(0,C125-D125-E125-F125))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C125-D125-E125-F125,MIN(I$7,C125-E125-F125)),MIN(I$7,MAX(0,C125-D125-F125))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C125-F125-G125,C125-D125-F125-G125),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C125-G125,IF(OPFOKLEGHEN!$J$18=\"nee\",C125-D125-G125)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C125-G125,C125-D125-F125-G125),C125-D125-F125-G125))","v":1.5356563089152491},1.5356563089152491,1.5757697407850417,21.197804915988431,{"$f":"SUM(K$16:K125)/$K$137","v":0.73764467822880064},0.26618248182177257,21.197804915988431,{"$f":"IF(E125<I$3,P125*(1-I$6*D125/C125),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P125*(1-$I$6)+(C125-D125)/C125*(K125-P125*(1-I$6)),P125*(1-$I$6)+(C125-D125)/C125*(K125-P125*(1-I$6))))","v":21.197804915988431},21.197804915988431,21.197804915988431,21.197804915988431,{"$f":"MIN(K125,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K125-(G125/(C125-G125))*(Q125)*95%,K125-(G125/(C125-G125))*(P125)*84%))","v":21.197804915988431},21.197804915988431,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H125/C125*K125,IF(OPFOKLEGHEN!$H$20=\"ja\",O125-(K125-Q125)-(K125-S125),Q125-(K125-O125)-(K125-S125)))","v":21.197804915988431},{"$f":"IF(H125=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q125-(K125-R125)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O125*80%-(K125-S125)),(Q125-(K125-S125)-(K125-T125))),(N125-(K125-S125))))","v":42.395609831976863},{"$f":"IF(H125=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q125-(K125-R125)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O125*80%-(K125-S125)),(Q125-(K125-S125)-(K125-N125))),(N125-(K125-S125))))","v":42.395609831976863},{"$f":"IF(H125=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q125-(K125-R125)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O125-(K125-S125)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N125-(K125-Q125)-(K125-S125)),(Q125-(K125-N125/80%)))))),(O125-(K125-S125))))","v":42.395609831976863},1,null,null,{"$f":"IF(H125=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P125-(K125-R125),K125-(K125-O125)/I$6-(K125-R125)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K125-O125)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O125-(K125-S125),IF(OPFOKLEGHEN!$H$20=\"nee\",(O125-(K125-S125)),(O125-(K125-S125)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O125*80%-(K125-S125),0+O125-(K125-S125)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O125*80%-(K125-S125)),O125*93%-(K125-S125)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O125-(K125-S125))),O125-(K125-S125))))))))","v":21.197804915988431},{"$f":"IF(H125=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q125-(K125-R125),N125-(K125-R125)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q125-(K125-N125)-(K125-S125),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q125-(K125-N125)-(K125-S125)),(O125-(K125-S125)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q125*$N$135-(K125-N125)-(K125-S125),(Q125-(K125-N125)-(K125-S125))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N125*95%-(K125-Q125)/I$4-(K125-S125)),N125-(K125-Q125)/I$4-(K125-S125)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N125-(K125-Q125)/I$4-(K125-S125))),N125-(K125-Q125)/I$4-(K125-S125))))))))","v":21.197804915988431},null,null,null,null,null,null,null,null,16,110,1285.4999999999995,1117.9999999999995,1201.7499999999995]
[16,111,1.555458481618083,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C126)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C126<$I$3,C126-D126,MIN($I$3,C126-D126))))","v":0},{"$f":"IF(C126<$I$7,MAX(0,C126-D126-E126-F126,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C126-D126-F126)),MIN(I$7,MAX(0,C126-D126-E126-F126))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C126-D126-E126-F126,MIN(I$7,C126-E126-F126)),MIN(I$7,MAX(0,C126-D126-F126))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C126-F126-G126,C126-D126-F126-G126),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C126-G126,IF(OPFOKLEGHEN!$J$18=\"nee\",C126-D126-G126)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C126-G126,C126-D126-F126-G126),C126-D126-F126-G126))","v":1.555458481618083},1.555458481618083,1.6050322939147728,21.869875190804191,{"$f":"SUM(K$16:K126)/$K$137","v":0.76325517946198695},0.27711828152731338,21.869875190804191,{"$f":"IF(E126<I$3,P126*(1-I$6*D126/C126),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P126*(1-$I$6)+(C126-D126)/C126*(K126-P126*(1-I$6)),P126*(1-$I$6)+(C126-D126)/C126*(K126-P126*(1-I$6))))","v":21.869875190804191},21.869875190804191,21.869875190804191,21.869875190804191,{"$f":"MIN(K126,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K126-(G126/(C126-G126))*(Q126)*95%,K126-(G126/(C126-G126))*(P126)*84%))","v":21.869875190804191},21.869875190804191,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H126/C126*K126,IF(OPFOKLEGHEN!$H$20=\"ja\",O126-(K126-Q126)-(K126-S126),Q126-(K126-O126)-(K126-S126)))","v":21.869875190804191},{"$f":"IF(H126=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q126-(K126-R126)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O126*80%-(K126-S126)),(Q126-(K126-S126)-(K126-T126))),(N126-(K126-S126))))","v":43.739750381608381},{"$f":"IF(H126=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q126-(K126-R126)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O126*80%-(K126-S126)),(Q126-(K126-S126)-(K126-N126))),(N126-(K126-S126))))","v":43.739750381608381},{"$f":"IF(H126=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q126-(K126-R126)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O126-(K126-S126)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N126-(K126-Q126)-(K126-S126)),(Q126-(K126-N126/80%)))))),(O126-(K126-S126))))","v":43.739750381608381},1,null,null,{"$f":"IF(H126=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P126-(K126-R126),K126-(K126-O126)/I$6-(K126-R126)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K126-O126)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O126-(K126-S126),IF(OPFOKLEGHEN!$H$20=\"nee\",(O126-(K126-S126)),(O126-(K126-S126)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O126*80%-(K126-S126),0+O126-(K126-S126)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O126*80%-(K126-S126)),O126*93%-(K126-S126)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O126-(K126-S126))),O126-(K126-S126))))))))","v":21.869875190804191},{"$f":"IF(H126=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q126-(K126-R126),N126-(K126-R126)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q126-(K126-N126)-(K126-S126),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q126-(K126-N126)-(K126-S126)),(O126-(K126-S126)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q126*$N$135-(K126-N126)-(K126-S126),(Q126-(K126-N126)-(K126-S126))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N126*95%-(K126-Q126)/I$4-(K126-S126)),N126-(K126-Q126)/I$4-(K126-S126)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N126-(K126-Q126)/I$4-(K126-S126))),N126-(K126-Q126)/I$4-(K126-S126))))))))","v":21.869875190804191},null,null,null,null,null,null,null,null,16,111,1297.5999999999995,1126.5999999999995,1212.0999999999995]
[16,112,1.5755838337225001,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C127)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C127<$I$3,C127-D127,MIN($I$3,C127-D127))))","v":0},{"$f":"IF(C127<$I$7,MAX(0,C127-D127-E127-F127,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C127-D127-F127)),MIN(I$7,MAX(0,C127-D127-E127-F127))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C127-D127-E127-F127,MIN(I$7,C127-E127-F127)),MIN(I$7,MAX(0,C127-D127-F127))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C127-F127-G127,C127-D127-F127-G127),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C127-G127,IF(OPFOKLEGHEN!$J$18=\"nee\",C127-D127-G127)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C127-G127,C127-D127-F127-G127),C127-D127-F127-G127))","v":1.5755838337225001},1.5755838337225001,1.6348382621092228,22.56422469200524,{"$f":"SUM(K$16:K127)/$K$137","v":0.78967879181728196},0.2884923704913912,22.56422469200524,{"$f":"IF(E127<I$3,P127*(1-I$6*D127/C127),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P127*(1-$I$6)+(C127-D127)/C127*(K127-P127*(1-I$6)),P127*(1-$I$6)+(C127-D127)/C127*(K127-P127*(1-I$6))))","v":22.56422469200524},22.56422469200524,22.56422469200524,22.56422469200524,{"$f":"MIN(K127,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K127-(G127/(C127-G127))*(Q127)*95%,K127-(G127/(C127-G127))*(P127)*84%))","v":22.56422469200524},22.56422469200524,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H127/C127*K127,IF(OPFOKLEGHEN!$H$20=\"ja\",O127-(K127-Q127)-(K127-S127),Q127-(K127-O127)-(K127-S127)))","v":22.56422469200524},{"$f":"IF(H127=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q127-(K127-R127)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O127*80%-(K127-S127)),(Q127-(K127-S127)-(K127-T127))),(N127-(K127-S127))))","v":45.12844938401048},{"$f":"IF(H127=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q127-(K127-R127)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O127*80%-(K127-S127)),(Q127-(K127-S127)-(K127-N127))),(N127-(K127-S127))))","v":45.12844938401048},{"$f":"IF(H127=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q127-(K127-R127)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O127-(K127-S127)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N127-(K127-Q127)-(K127-S127)),(Q127-(K127-N127/80%)))))),(O127-(K127-S127))))","v":45.12844938401048},1,null,null,{"$f":"IF(H127=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P127-(K127-R127),K127-(K127-O127)/I$6-(K127-R127)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K127-O127)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O127-(K127-S127),IF(OPFOKLEGHEN!$H$20=\"nee\",(O127-(K127-S127)),(O127-(K127-S127)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O127*80%-(K127-S127),0+O127-(K127-S127)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O127*80%-(K127-S127)),O127*93%-(K127-S127)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O127-(K127-S127))),O127-(K127-S127))))))))","v":22.56422469200524},{"$f":"IF(H127=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q127-(K127-R127),N127-(K127-R127)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q127-(K127-N127)-(K127-S127),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q127-(K127-N127)-(K127-S127)),(O127-(K127-S127)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q127*$N$135-(K127-N127)-(K127-S127),(Q127-(K127-N127)-(K127-S127))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N127*95%-(K127-Q127)/I$4-(K127-S127)),N127-(K127-Q127)/I$4-(K127-S127)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N127-(K127-Q127)/I$4-(K127-S127))),N127-(K127-Q127)/I$4-(K127-S127))))))))","v":22.56422469200524},null,null,null,null,null,null,null,null,16,112,1310,1135,1222.5]
[17,113,1.5966289385177499,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C128)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C128<$I$3,C128-D128,MIN($I$3,C128-D128))))","v":0},{"$f":"IF(C128<$I$7,MAX(0,C128-D128-E128-F128,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C128-D128-F128)),MIN(I$7,MAX(0,C128-D128-E128-F128))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C128-D128-E128-F128,MIN(I$7,C128-E128-F128)),MIN(I$7,MAX(0,C128-D128-F128))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C128-F128-G128,C128-D128-F128-G128),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C128-G128,IF(OPFOKLEGHEN!$J$18=\"nee\",C128-D128-G128)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C128-G128,C128-D128-F128-G128),C128-D128-F128-G128))","v":1.5966289385177499},1.5966289385177499,1.6651977367616904,23.290237359043481,{"$f":"SUM(K$16:K128)/$K$137","v":0.81695259413215693},0.30043342712008142,23.290237359043481,{"$f":"IF(E128<I$3,P128*(1-I$6*D128/C128),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P128*(1-$I$6)+(C128-D128)/C128*(K128-P128*(1-I$6)),P128*(1-$I$6)+(C128-D128)/C128*(K128-P128*(1-I$6))))","v":23.290237359043481},23.290237359043481,23.290237359043481,23.290237359043481,{"$f":"MIN(K128,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K128-(G128/(C128-G128))*(Q128)*95%,K128-(G128/(C128-G128))*(P128)*84%))","v":23.290237359043481},23.290237359043481,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H128/C128*K128,IF(OPFOKLEGHEN!$H$20=\"ja\",O128-(K128-Q128)-(K128-S128),Q128-(K128-O128)-(K128-S128)))","v":23.290237359043481},{"$f":"IF(H128=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q128-(K128-R128)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O128*80%-(K128-S128)),(Q128-(K128-S128)-(K128-T128))),(N128-(K128-S128))))","v":46.580474718086961},{"$f":"IF(H128=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q128-(K128-R128)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O128*80%-(K128-S128)),(Q128-(K128-S128)-(K128-N128))),(N128-(K128-S128))))","v":46.580474718086961},{"$f":"IF(H128=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q128-(K128-R128)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O128-(K128-S128)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N128-(K128-Q128)-(K128-S128)),(Q128-(K128-N128/80%)))))),(O128-(K128-S128))))","v":46.580474718086961},1,null,null,{"$f":"IF(H128=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P128-(K128-R128),K128-(K128-O128)/I$6-(K128-R128)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K128-O128)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O128-(K128-S128),IF(OPFOKLEGHEN!$H$20=\"nee\",(O128-(K128-S128)),(O128-(K128-S128)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O128*80%-(K128-S128),0+O128-(K128-S128)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O128*80%-(K128-S128)),O128*93%-(K128-S128)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O128-(K128-S128))),O128-(K128-S128))))))))","v":23.290237359043481},{"$f":"IF(H128=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q128-(K128-R128),N128-(K128-R128)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q128-(K128-N128)-(K128-S128),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q128-(K128-N128)-(K128-S128)),(O128-(K128-S128)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q128*$N$135-(K128-N128)-(K128-S128),(Q128-(K128-N128)-(K128-S128))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N128*95%-(K128-Q128)/I$4-(K128-S128)),N128-(K128-Q128)/I$4-(K128-S128)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N128-(K128-Q128)/I$4-(K128-S128))),N128-(K128-Q128)/I$4-(K128-S128))))))))","v":23.290237359043481},null,null,null,null,null,null,null,null,17,113,{"$f":"AO127+12.9","v":1322.9},{"$f":"AP127+8.6","v":1143.5999999999999},1233.25]
[17,114,1.6179233439829999,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C129)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C129<$I$3,C129-D129,MIN($I$3,C129-D129))))","v":0},{"$f":"IF(C129<$I$7,MAX(0,C129-D129-E129-F129,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C129-D129-F129)),MIN(I$7,MAX(0,C129-D129-E129-F129))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C129-D129-E129-F129,MIN(I$7,C129-E129-F129)),MIN(I$7,MAX(0,C129-D129-F129))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C129-F129-G129,C129-D129-F129-G129),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C129-G129,IF(OPFOKLEGHEN!$J$18=\"nee\",C129-D129-G129)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C129-G129,C129-D129-F129-G129),C129-D129-F129-G129))","v":1.6179233439829999},1.6179233439829999,1.6961209966659074,24.039137291395235,{"$f":"SUM(K$16:K129)/$K$137","v":0.8451033883124951},0.31283808803870511,24.039137291395235,{"$f":"IF(E129<I$3,P129*(1-I$6*D129/C129),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P129*(1-$I$6)+(C129-D129)/C129*(K129-P129*(1-I$6)),P129*(1-$I$6)+(C129-D129)/C129*(K129-P129*(1-I$6))))","v":24.039137291395235},24.039137291395235,24.039137291395235,24.039137291395235,{"$f":"MIN(K129,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K129-(G129/(C129-G129))*(Q129)*95%,K129-(G129/(C129-G129))*(P129)*84%))","v":24.039137291395235},24.039137291395235,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H129/C129*K129,IF(OPFOKLEGHEN!$H$20=\"ja\",O129-(K129-Q129)-(K129-S129),Q129-(K129-O129)-(K129-S129)))","v":24.039137291395235},{"$f":"IF(H129=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q129-(K129-R129)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O129*80%-(K129-S129)),(Q129-(K129-S129)-(K129-T129))),(N129-(K129-S129))))","v":48.078274582790471},{"$f":"IF(H129=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q129-(K129-R129)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O129*80%-(K129-S129)),(Q129-(K129-S129)-(K129-N129))),(N129-(K129-S129))))","v":48.078274582790471},{"$f":"IF(H129=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q129-(K129-R129)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O129-(K129-S129)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N129-(K129-Q129)-(K129-S129)),(Q129-(K129-N129/80%)))))),(O129-(K129-S129))))","v":48.078274582790471},1,null,null,{"$f":"IF(H129=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P129-(K129-R129),K129-(K129-O129)/I$6-(K129-R129)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K129-O129)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O129-(K129-S129),IF(OPFOKLEGHEN!$H$20=\"nee\",(O129-(K129-S129)),(O129-(K129-S129)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O129*80%-(K129-S129),0+O129-(K129-S129)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O129*80%-(K129-S129)),O129*93%-(K129-S129)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O129-(K129-S129))),O129-(K129-S129))))))))","v":24.039137291395235},{"$f":"IF(H129=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q129-(K129-R129),N129-(K129-R129)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q129-(K129-N129)-(K129-S129),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q129-(K129-N129)-(K129-S129)),(O129-(K129-S129)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q129*$N$135-(K129-N129)-(K129-S129),(Q129-(K129-N129)-(K129-S129))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N129*95%-(K129-Q129)/I$4-(K129-S129)),N129-(K129-Q129)/I$4-(K129-S129)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N129-(K129-Q129)/I$4-(K129-S129))),N129-(K129-Q129)/I$4-(K129-S129))))))))","v":24.039137291395235},null,null,null,null,null,null,null,null,17,114,1335.8000000000002,1152.1999999999998,1244]
[17,115,1.6394699123702499,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C130)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C130<$I$3,C130-D130,MIN($I$3,C130-D130))))","v":0},{"$f":"IF(C130<$I$7,MAX(0,C130-D130-E130-F130,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C130-D130-F130)),MIN(I$7,MAX(0,C130-D130-E130-F130))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C130-D130-E130-F130,MIN(I$7,C130-E130-F130)),MIN(I$7,MAX(0,C130-D130-F130))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C130-F130-G130,C130-D130-F130-G130),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C130-G130,IF(OPFOKLEGHEN!$J$18=\"nee\",C130-D130-G130)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C130-G130,C130-D130-F130-G130),C130-D130-F130-G130))","v":1.6394699123702499},1.6394699123702499,1.7276185114961276,24.811636270149574,{"$f":"SUM(K$16:K130)/$K$137","v":0.87415880978839011},0.32572353550995448,24.811636270149574,{"$f":"IF(E130<I$3,P130*(1-I$6*D130/C130),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P130*(1-$I$6)+(C130-D130)/C130*(K130-P130*(1-I$6)),P130*(1-$I$6)+(C130-D130)/C130*(K130-P130*(1-I$6))))","v":24.811636270149574},24.811636270149574,24.811636270149574,24.811636270149574,{"$f":"MIN(K130,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K130-(G130/(C130-G130))*(Q130)*95%,K130-(G130/(C130-G130))*(P130)*84%))","v":24.811636270149574},24.811636270149574,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H130/C130*K130,IF(OPFOKLEGHEN!$H$20=\"ja\",O130-(K130-Q130)-(K130-S130),Q130-(K130-O130)-(K130-S130)))","v":24.811636270149574},{"$f":"IF(H130=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q130-(K130-R130)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O130*80%-(K130-S130)),(Q130-(K130-S130)-(K130-T130))),(N130-(K130-S130))))","v":49.623272540299148},{"$f":"IF(H130=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q130-(K130-R130)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O130*80%-(K130-S130)),(Q130-(K130-S130)-(K130-N130))),(N130-(K130-S130))))","v":49.623272540299148},{"$f":"IF(H130=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q130-(K130-R130)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O130-(K130-S130)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N130-(K130-Q130)-(K130-S130)),(Q130-(K130-N130/80%)))))),(O130-(K130-S130))))","v":49.623272540299148},1,null,null,{"$f":"IF(H130=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P130-(K130-R130),K130-(K130-O130)/I$6-(K130-R130)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K130-O130)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O130-(K130-S130),IF(OPFOKLEGHEN!$H$20=\"nee\",(O130-(K130-S130)),(O130-(K130-S130)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O130*80%-(K130-S130),0+O130-(K130-S130)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O130*80%-(K130-S130)),O130*93%-(K130-S130)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O130-(K130-S130))),O130-(K130-S130))))))))","v":24.811636270149574},{"$f":"IF(H130=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q130-(K130-R130),N130-(K130-R130)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q130-(K130-N130)-(K130-S130),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q130-(K130-N130)-(K130-S130)),(O130-(K130-S130)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q130*$N$135-(K130-N130)-(K130-S130),(Q130-(K130-N130)-(K130-S130))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N130*95%-(K130-Q130)/I$4-(K130-S130)),N130-(K130-Q130)/I$4-(K130-S130)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N130-(K130-Q130)/I$4-(K130-S130))),N130-(K130-Q130)/I$4-(K130-S130))))))))","v":24.811636270149574},null,null,null,null,null,null,null,null,17,115,1348.7000000000003,1160.7999999999997,1254.75]
[17,116,1.6612715059315002,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C131)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C131<$I$3,C131-D131,MIN($I$3,C131-D131))))","v":0},{"$f":"IF(C131<$I$7,MAX(0,C131-D131-E131-F131,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C131-D131-F131)),MIN(I$7,MAX(0,C131-D131-E131-F131))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C131-D131-E131-F131,MIN(I$7,C131-E131-F131)),MIN(I$7,MAX(0,C131-D131-F131))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C131-F131-G131,C131-D131-F131-G131),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C131-G131,IF(OPFOKLEGHEN!$J$18=\"nee\",C131-D131-G131)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C131-G131,C131-D131-F131-G131),C131-D131-F131-G131))","v":1.6612715059315002},1.6612715059315002,1.7597009453518353,25.608467505789857,{"$f":"SUM(K$16:K131)/$K$137","v":0.90414735260882695},0.33910756057895247,25.608467505789857,{"$f":"IF(E131<I$3,P131*(1-I$6*D131/C131),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P131*(1-$I$6)+(C131-D131)/C131*(K131-P131*(1-I$6)),P131*(1-$I$6)+(C131-D131)/C131*(K131-P131*(1-I$6))))","v":25.608467505789857},25.608467505789857,25.608467505789857,25.608467505789857,{"$f":"MIN(K131,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K131-(G131/(C131-G131))*(Q131)*95%,K131-(G131/(C131-G131))*(P131)*84%))","v":25.608467505789857},25.608467505789857,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H131/C131*K131,IF(OPFOKLEGHEN!$H$20=\"ja\",O131-(K131-Q131)-(K131-S131),Q131-(K131-O131)-(K131-S131)))","v":25.608467505789857},{"$f":"IF(H131=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q131-(K131-R131)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O131*80%-(K131-S131)),(Q131-(K131-S131)-(K131-T131))),(N131-(K131-S131))))","v":51.216935011579714},{"$f":"IF(H131=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q131-(K131-R131)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O131*80%-(K131-S131)),(Q131-(K131-S131)-(K131-N131))),(N131-(K131-S131))))","v":51.216935011579714},{"$f":"IF(H131=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q131-(K131-R131)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O131-(K131-S131)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N131-(K131-Q131)-(K131-S131)),(Q131-(K131-N131/80%)))))),(O131-(K131-S131))))","v":51.216935011579714},1,null,null,{"$f":"IF(H131=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P131-(K131-R131),K131-(K131-O131)/I$6-(K131-R131)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K131-O131)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O131-(K131-S131),IF(OPFOKLEGHEN!$H$20=\"nee\",(O131-(K131-S131)),(O131-(K131-S131)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O131*80%-(K131-S131),0+O131-(K131-S131)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O131*80%-(K131-S131)),O131*93%-(K131-S131)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O131-(K131-S131))),O131-(K131-S131))))))))","v":25.608467505789857},{"$f":"IF(H131=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q131-(K131-R131),N131-(K131-R131)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q131-(K131-N131)-(K131-S131),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q131-(K131-N131)-(K131-S131)),(O131-(K131-S131)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q131*$N$135-(K131-N131)-(K131-S131),(Q131-(K131-N131)-(K131-S131))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N131*95%-(K131-Q131)/I$4-(K131-S131)),N131-(K131-Q131)/I$4-(K131-S131)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N131-(K131-Q131)/I$4-(K131-S131))),N131-(K131-Q131)/I$4-(K131-S131))))))))","v":25.608467505789857},null,null,null,null,null,null,null,null,17,116,1361.6000000000004,1169.3999999999996,1265.5]
[17,117,1.6833309869187498,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C132)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C132<$I$3,C132-D132,MIN($I$3,C132-D132))))","v":0},{"$f":"IF(C132<$I$7,MAX(0,C132-D132-E132-F132,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C132-D132-F132)),MIN(I$7,MAX(0,C132-D132-E132-F132))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C132-D132-E132-F132,MIN(I$7,C132-E132-F132)),MIN(I$7,MAX(0,C132-D132-F132))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C132-F132-G132,C132-D132-F132-G132),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C132-G132,IF(OPFOKLEGHEN!$J$18=\"nee\",C132-D132-G132)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C132-G132,C132-D132-F132-G132),C132-D132-F132-G132))","v":1.6833309869187498},1.6833309869187498,1.7923791603682901,26.430386257168902,{"$f":"SUM(K$16:K132)/$K$137","v":0.93509839526120719},0.35300858357177645,26.430386257168902,{"$f":"IF(E132<I$3,P132*(1-I$6*D132/C132),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P132*(1-$I$6)+(C132-D132)/C132*(K132-P132*(1-I$6)),P132*(1-$I$6)+(C132-D132)/C132*(K132-P132*(1-I$6))))","v":26.430386257168902},26.430386257168902,26.430386257168902,26.430386257168902,{"$f":"MIN(K132,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K132-(G132/(C132-G132))*(Q132)*95%,K132-(G132/(C132-G132))*(P132)*84%))","v":26.430386257168902},26.430386257168902,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H132/C132*K132,IF(OPFOKLEGHEN!$H$20=\"ja\",O132-(K132-Q132)-(K132-S132),Q132-(K132-O132)-(K132-S132)))","v":26.430386257168902},{"$f":"IF(H132=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q132-(K132-R132)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O132*80%-(K132-S132)),(Q132-(K132-S132)-(K132-T132))),(N132-(K132-S132))))","v":52.860772514337803},{"$f":"IF(H132=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q132-(K132-R132)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O132*80%-(K132-S132)),(Q132-(K132-S132)-(K132-N132))),(N132-(K132-S132))))","v":52.860772514337803},{"$f":"IF(H132=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q132-(K132-R132)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O132-(K132-S132)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N132-(K132-Q132)-(K132-S132)),(Q132-(K132-N132/80%)))))),(O132-(K132-S132))))","v":52.860772514337803},1,null,null,{"$f":"IF(H132=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P132-(K132-R132),K132-(K132-O132)/I$6-(K132-R132)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K132-O132)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O132-(K132-S132),IF(OPFOKLEGHEN!$H$20=\"nee\",(O132-(K132-S132)),(O132-(K132-S132)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O132*80%-(K132-S132),0+O132-(K132-S132)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O132*80%-(K132-S132)),O132*93%-(K132-S132)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O132-(K132-S132))),O132-(K132-S132))))))))","v":26.430386257168902},{"$f":"IF(H132=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q132-(K132-R132),N132-(K132-R132)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q132-(K132-N132)-(K132-S132),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q132-(K132-N132)-(K132-S132)),(O132-(K132-S132)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q132*$N$135-(K132-N132)-(K132-S132),(Q132-(K132-N132)-(K132-S132))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N132*95%-(K132-Q132)/I$4-(K132-S132)),N132-(K132-Q132)/I$4-(K132-S132)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N132-(K132-Q132)/I$4-(K132-S132))),N132-(K132-Q132)/I$4-(K132-S132))))))))","v":26.430386257168902},null,null,null,null,null,null,null,null,17,117,1374.5000000000005,1177.9999999999995,1276.25]
[17,118,1.705651217584,0,{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C133)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C133<$I$3,C133-D133,MIN($I$3,C133-D133))))","v":0},{"$f":"IF(C133<$I$7,MAX(0,C133-D133-E133-F133,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C133-D133-F133)),MIN(I$7,MAX(0,C133-D133-E133-F133))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C133-D133-E133-F133,MIN(I$7,C133-E133-F133)),MIN(I$7,MAX(0,C133-D133-F133))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C133-F133-G133,C133-D133-F133-G133),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C133-G133,IF(OPFOKLEGHEN!$J$18=\"nee\",C133-D133-G133)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C133-G133,C133-D133-F133-G133),C133-D133-F133-G133))","v":1.705651217584},1.705651217584,1.8256642203941094,27.27817046763327,{"$f":"SUM(K$16:K133)/$K$137","v":0.96704222723580102},0.36744567524894123,27.27817046763327,{"$f":"IF(E133<I$3,P133*(1-I$6*D133/C133),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P133*(1-$I$6)+(C133-D133)/C133*(K133-P133*(1-I$6)),P133*(1-$I$6)+(C133-D133)/C133*(K133-P133*(1-I$6))))","v":27.27817046763327},27.27817046763327,27.27817046763327,27.27817046763327,{"$f":"MIN(K133,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K133-(G133/(C133-G133))*(Q133)*95%,K133-(G133/(C133-G133))*(P133)*84%))","v":27.27817046763327},27.27817046763327,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H133/C133*K133,IF(OPFOKLEGHEN!$H$20=\"ja\",O133-(K133-Q133)-(K133-S133),Q133-(K133-O133)-(K133-S133)))","v":27.27817046763327},{"$f":"IF(H133=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q133-(K133-R133)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O133*80%-(K133-S133)),(Q133-(K133-S133)-(K133-T133))),(N133-(K133-S133))))","v":54.55634093526654},{"$f":"IF(H133=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q133-(K133-R133)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O133*80%-(K133-S133)),(Q133-(K133-S133)-(K133-N133))),(N133-(K133-S133))))","v":54.55634093526654},{"$f":"IF(H133=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q133-(K133-R133)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O133-(K133-S133)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N133-(K133-Q133)-(K133-S133)),(Q133-(K133-N133/80%)))))),(O133-(K133-S133))))","v":54.55634093526654},1,null,null,{"$f":"IF(H133=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P133-(K133-R133),K133-(K133-O133)/I$6-(K133-R133)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K133-O133)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O133-(K133-S133),IF(OPFOKLEGHEN!$H$20=\"nee\",(O133-(K133-S133)),(O133-(K133-S133)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O133*80%-(K133-S133),0+O133-(K133-S133)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O133*80%-(K133-S133)),O133*93%-(K133-S133)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O133-(K133-S133))),O133-(K133-S133))))))))","v":27.27817046763327},{"$f":"IF(H133=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q133-(K133-R133),N133-(K133-R133)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q133-(K133-N133)-(K133-S133),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q133-(K133-N133)-(K133-S133)),(O133-(K133-S133)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q133*$N$135-(K133-N133)-(K133-S133),(Q133-(K133-N133)-(K133-S133))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N133*95%-(K133-Q133)/I$4-(K133-S133)),N133-(K133-Q133)/I$4-(K133-S133)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N133-(K133-Q133)/I$4-(K133-S133))),N133-(K133-Q133)/I$4-(K133-S133))))))))","v":27.27817046763327},null,null,null,null,null,null,null,null,17,118,1387.4000000000005,1186.5999999999995,1287]
[17,119,1.7277068391474997,{"$f":"MIN(C134,J$5)","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",0,MIN(I$3,C134)))","v":0},{"$f":"IF(I$3=0,0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",0,IF(C134<$I$3,C134-D134,MIN($I$3,C134-D134))))","v":0},{"$f":"IF(C134<$I$7,MAX(0,C134-D134-E134-F134,IF(OPFOKLEGHEN!$H$15=\"warmtewisselaar\",IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",MIN(I$7,MAX(0,C134-D134-F134)),MIN(I$7,MAX(0,C134-D134-E134-F134))))),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",MIN(I$7,C134-D134-E134-F134,MIN(I$7,C134-E134-F134)),MIN(I$7,MAX(0,C134-D134-F134))))","v":0},{"$f":"IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",C134-F134-G134,C134-D134-F134-G134),IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",C134-G134,IF(OPFOKLEGHEN!$J$18=\"nee\",C134-D134-G134)))),IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$J$18=\"ja\",C134-G134,C134-D134-F134-G134),C134-D134-F134-G134))","v":1.7277068391474997},1.7277068391474997,1.8595673947371558,28.144016798309401,{"$f":"SUM(K$16:K134)/$K$137","v":1},0.38232168938342681,28.144016798309401,{"$f":"IF(E134<I$3,P134*(1-I$6*D134/C134),IF(OPFOKLEGHEN!$H$11=\"droogtunnel (platen) 55%\",P134*(1-$I$6)+(C134-D134)/C134*(K134-P134*(1-I$6)),P134*(1-$I$6)+(C134-D134)/C134*(K134-P134*(1-I$6))))","v":28.144016798309401},28.144016798309401,28.144016798309401,28.144016798309401,{"$f":"MIN(K134,IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",K134-(G134/(C134-G134))*(Q134)*95%,K134-(G134/(C134-G134))*(P134)*84%))","v":28.144016798309401},28.144016798309401,0,{"$f":"IF(OPFOKLEGHEN!$J$18=\"nee\",H134/C134*K134,IF(OPFOKLEGHEN!$H$20=\"ja\",O134-(K134-Q134)-(K134-S134),Q134-(K134-O134)-(K134-S134)))","v":28.144016798309401},{"$f":"IF(H134=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q134-(K134-R134)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O134*80%-(K134-S134)),(Q134-(K134-S134)-(K134-T134))),(N134-(K134-S134))))","v":56.288033596618803},{"$f":"IF(H134=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q134-(K134-R134)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",3*(O134*80%-(K134-S134)),(Q134-(K134-S134)-(K134-N134))),(N134-(K134-S134))))","v":56.288033596618803},{"$f":"IF(H134=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q134-(K134-R134)))+IF(OPFOKLEGHEN!$H$12>0,IF(OPFOKLEGHEN!$H$13=\"serie geschakeld met warmtewisselaar\",(O134-(K134-S134)),IF(OPFOKLEGHEN!$H$13=\"parallel geschakeld met warmtewisselaar\",IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"nee\",(N134-(K134-Q134)-(K134-S134)),(Q134-(K134-N134/80%)))))),(O134-(K134-S134))))","v":56.288033596618803},1,null,null,{"$f":"IF(H134=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",P134-(K134-R134),K134-(K134-O134)/I$6-(K134-R134)/95%)+IF(OPFOKLEGHEN!$J$18=\"ja\",J$5/I$5*(K134-O134)*(1-I$6)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",O134-(K134-S134),IF(OPFOKLEGHEN!$H$20=\"nee\",(O134-(K134-S134)),(O134-(K134-S134)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",O134*80%-(K134-S134),0+O134-(K134-S134)))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(O134*80%-(K134-S134)),O134*93%-(K134-S134)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",O134-(K134-S134))),O134-(K134-S134))))))))","v":28.144016798309401},{"$f":"IF(H134=0,0,IF(OPFOKLEGHEN!$H$11=\"geen droogtunnel\",IF(OPFOKLEGHEN!$H$15=\"geen warmtewisselaar\",Q134-(K134-R134),N134-(K134-R134)),IF(OPFOKLEGHEN!$H$12>=0,IF(OPFOKLEGHEN!$L$9=\"ja\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$H$20=\"ja\",Q134-(K134-N134)-(K134-S134),IF(OPFOKLEGHEN!$H$20=\"nee\",(Q134-(K134-N134)-(K134-S134)),(O134-(K134-S134)))),IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",1*Q134*$N$135-(K134-N134)-(K134-S134),(Q134-(K134-N134)-(K134-S134))*N$135))),IF(OPFOKLEGHEN!$L$9=\"nee\",IF(OPFOKLEGHEN!$J$18=\"nee\",IF(OPFOKLEGHEN!$H$20=\"nee\",(N134*95%-(K134-Q134)/I$4-(K134-S134)),N134-(K134-Q134)/I$4-(K134-S134)),IF(OPFOKLEGHEN!$H$20=\"nee\",IF(OPFOKLEGHEN!$J$18=\"ja\",IF(OPFOKLEGHEN!$L$9=\"nee\",N134-(K134-Q134)/I$4-(K134-S134))),N134-(K134-Q134)/I$4-(K134-S134))))))))","v":28.144016798309401},null,null,null,null,null,null,null,null,17,119,1400,1195,1297.5]
[null,null,null,null,null,null,null,null,null,null,null,null,null,{"$f":"MAX(84%,N134/K134)","v":1},null,null,null,null,null,null,null,null,null,null,null,null,null,null,"K71-(K71-O71)/I$6)-((K71-T71)/95%)+ALS(LEGPLUIMVEE!$J$18=\"ja\",(K71-O71)*(1-I$6))"]
[null,null,null," ",null,null,null," ",null,null," ",null,null,{"$f":"N134/K134","v":1},"  ",null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,{"$f":"SUM(C16:C134)","v":94.818695699867362},null,null,0,null,null,null,{"$f":"SUM(J16:J134)","v":90.576443754598273},{"$f":"SUM(K16:K134)","v":853.94170897620143},null,9.0396046086671955,853.94170897620143,853.94170897620143,853.94170897620143,853.94170897620143,853.94170897620143,853.94170897620143,853.69086185883964,347.6565734224036,{"$f":"SUM(V16:V135)","v":853.94170897620143},{"$f":"SUM(W16:W134)","v":1707.8834179524029},{"$f":"SUM(X16:X134)","v":1707.8834179524029},1707.8834179524029," ",null,null,{"$f":"SUM(AC16:AC134)","v":853.94170897620143},853.94170897620143,null,{"$f":"SUM(AF16:AF71)","v":20.580314798992582},{"$f":"SUM(AG16:AG71)","v":0},null,{"$f":"SUM(AI16:AI71)","v":20.580314798992582},{"$f":"SUM(AJ16:AJ71)","v":0},null,{"$f":"SUM(AL16:AL71)","v":0.34629071839757863},{"$f":"SUM(AM16:AM71)","v":252},null,null,{"$f":"SUM(AP16:AP71)","v":15417.6},{"$f":"SUM(AQ16:AQ71)","v":16351.7},{"$f":"SUM(AR16:AR71)","v":347.66265050806948}]
[null,null,null,null,null,null," ",null,null," ",null,null,{"$f":"($K137-M137)/$K137","v":0.989414260348631},{"$f":"ROUND(($K137-N137)/$K137,2)","v":0},{"$f":"ROUND(($K137-O137)/$K137,2)","v":0},{"$f":"ROUND(($K137-P137)/$K137,2)","v":0},{"$f":"ROUND(($K137-Q137)/$K137,2)","v":0},{"$f":"MIN(98%,($K137-R137)/$K137)","v":0},0,2.937520380197019E-4,0.5928802050912676,{"$f":"V137/K137","v":1},{"$f":"W137/K137","v":2},{"$f":"X137/K137","v":2},{"$f":"Y137/$K137","v":2},{"$f":"AVERAGE(Z16:Z134)","v":1},null,null,{"$f":"AC137/$K137","v":1},{"$f":"AD137/$K137","v":1},null,{"$f":"($J137-AF137)/$J137","v":0.77278513103526658},{"$f":"($K137-AG137)/$K137","v":1},null,{"$f":"($K137-AI137)/$K137","v":0.97589962572074562},{"$f":"($K137-AJ137)/$K137","v":1},null,{"$f":"($K137-AL137)/$K137","v":0.99959447967612136},{"$f":"($K137-AM137)/$K137","v":0.70489789015912441},null,null,{"$f":"($K137-AP137)/$K137","v":-17.054628129693189},{"$f":"($K137-AQ137)/$K137","v":-18.148496704305735},{"$f":"($K137-AR137)/$K137","v":0.59287308858014975}]
[null,null,null,null,null,null,null," ",null,null,63,null,null,null," ",null,{"$f":"$Q$138","v":0}]
[null,null,null,null,null," "," ",null,null,null,null,null," "," "," "," "," ",null," ",null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," ",null,null," ",null,null," ",null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null," "]

{"sheet":"Max waarden","index":2,"n_rows":46,"n_cols":9,"rows_kept":46,"cut":false,"hidden":true,"merged":[]}
["Overzicht maximale waarden rekenmodel reducties fijnstof"]
[]
[null,"waarden in m3/dier/uur"]
[]
["Maximale ventilatie:"]
["Opfok leghennen",{"$f":"IF(OPFOKLEGHEN!$L$25=\"luchtconditioneringsunit\",1.73,1.73)","v":1.73}]
["Leghennen",{"$f":"IF(#REF!=\"luchtconditioneringsunit\",8.01/2,8.01)","v":{"$error":"#REF!"}},{"$f":"#REF!","v":{"$error":"#REF!"}}]
["Opfok vleeskuikenouderdieren",4.8600000000000003]
["Vleeskuikenouderdieren",15]
["Vleeskuikens",6.1761991606700253]
["Vleeskalkoenen hennen",12.35]
["Vleeskalkoenen hanen",24.84]
["Vleeseenden",12.56]
[]
[]
["Debiet door droogtunnel",null,"rekenwaarde","in overzicht"]
["Opfok leghennen","bandendroger (30%)",0.81,0.85,"Deze waarden staan (nog) niet genoemd in de beschrijvingen."]
[null,"platendroger (55%)",0.84499999999999997,0.85]
["Leghennen","bandendroger (30%)",1.835,2]
[null,"platendroger (55%)",1.899,2]
[]
[]
["Debiet door warmtewisselaar"]
["ZONDER FILTERS"]
["Reductiepercentage op stalniveau:",0.13,null,0.31,null,0.37,null,0.5]
[null,"rekenwaarde","in overzicht","rekenwaarde","in overzicht","rekenwaarde","in overzicht","rekenwaarde","in overzicht"]
["Opfok leghennen",0.17499999999999999,0.2,0.434,0.4,0.52700000000000002,0.55000000000000004,0.745,0.8]
["Leghennen",0.439,0.4,1.048,1,1.252,1.25,1.708,1.8]
["Opfok vleeskuikenouderdieren",0.42,0.4,1.0469999999999999,1,1.2789999999999999,1.3,1.84,1.9]
["Vleeskuikenouderdieren",0.59499999999999997,0.6,1.4850000000000001,1.5,1.845,1.85,2.8450000000000002,2.9]
["Vleeskuikens",0.35699999999999998,0.35,1.0009999999999999,1,1.27,1.3,1.9750000000000001,2]
["Vleeskalkoenen hennen",1.2450000000000001,1.1000000000000001,3.17,3,3.86,3.85,5.5,5.6]
["Vleeskalkoenen hanen",2.6949999999999998,2.5,6.75,6.2,8.1750000000000007,8.1999999999999993,11.5,11.7]
["Vleeseenden",0.88,0.8,2.4849999999999999,2.2999999999999998,3.12,3.15,4.7300000000000004,4.8]
[]
["MET FILTERS"]
["Reductiepercentage op stalniveau:",0.13,null,0.31,null,0.37,null,0.5]
[null,"rekenwaarde","in overzicht","rekenwaarde","in overzicht","rekenwaarde","in overzicht","rekenwaarde","in overzicht"]
["Opfok leghennen",0.14099999999999999,0.15,0.34599999999999997,0.35,0.41799999999999998,0.4,0.58099999999999996,0.6]
["Leghennen",0.35499999999999998,0.35,0.84699999999999998,0.85,1.012,1,1.369,1.4]
["Opfok vleeskuikenouderdieren",0.33700000000000002,0.35,0.83099999999999996,0.85,1.008,1.1000000000000001,1.417,1.45]
["Vleeskuikenouderdieren",0.48,0.5,1.161,1.2,1.4219999999999999,1.5,2.0750000000000002,2.1]
["Vleeskuikens",0.28499999999999998,0.3,0.76500000000000001,0.75,0.95799999999999996,1,1.4350000000000001,1.45]
["Vleeskalkoenen hennen",0.999,0.9,2.5099999999999998,2.5,3.0449999999999999,3,4.2699999999999996,4.3]
["Vleeskalkoenen hanen",2.165,2.2000000000000002,5.3579999999999997,5.3,6.4749999999999996,6.2,9.01,9]
["Vleeseenden",0.69199999999999995,0.7,1.91,1.9,2.375,2.2999999999999998,3.51,3.6]

{"sheet":"Reductietechnieken","index":3,"n_rows":55,"n_cols":29,"rows_kept":55,"cut":false,"hidden":true,"merged":[]}
[null,"serie alles\nvoetnoot 2",null,null,"A","B","C","D","E","F","G","H","I","J","K","L","M","N","O","P","Q","R","S","T","U","V","W","X","Y"]
[null,null,null,null,{"$f":"+D3","v":0.65},{"$f":"+D4","v":0.4},{"$f":"+D5","v":0.25},{"$f":"+D6","v":0.19999999999999996},{"$f":"+D8","v":0.44999999999999996},{"$f":"+D9","v":0.7},{"$f":"+D10","v":0.45999999999999996},{"$f":"+D11","v":0.51},{"$f":"+D12","v":0.66999999999999993},{"$f":"+D13","v":0.6},{"$f":"+D14","v":0.43000000000000005},{"$f":"+D15","v":0.69},{"$f":"+D16","v":0.69},{"$f":"+D17","v":0.87},{"$f":"+D18","v":0.87},{"$f":"+D19","v":0.85},{"$f":"+D20","v":0.7},{"$f":"+D21","v":0.8},{"$f":"+D22","v":0.63},{"$f":"+D23","v":0.63},{"$f":"+D24","v":0.5},{"$f":"+D25","v":0.5}]
["A","chemische wasser",0.35,{"$f":"+(1-C3)","v":0.65},{"$f":"1-($D$3*E2)","v":0.5774999999999999},{"$f":"1-($D$3*F2)","v":0.74},0.83750000000000002,0.87,0.70750000000000002,0.54500000000000004,0.70100000000000007,0.66849999999999998,0.5645,0.61,0.72049999999999992,0.5515000000000001,0.5515000000000001,0.4345,0.4345,0.44750000000000001,0.54500000000000004,0.48,0.59050000000000002,0.59050000000000002,0.67500000000000004,0.67500000000000004]
["B","bio wasser 60%",0.6,{"$f":"+(1-C4)","v":0.4},{"$f":"1-+$D$4*E2","v":0.74},{"$f":"1-+$D$4*F2","v":0.84},0.9,0.92,0.82000000000000006,0.72,0.81600000000000006,0.79600000000000004,0.73199999999999998,0.76,0.82799999999999996,0.72399999999999998,0.72399999999999998,0.65199999999999991,0.65199999999999991,0.65999999999999992,0.72,0.67999999999999994,0.748,0.748,0.8,0.8]
["C","bio wasser 75%",0.75,0.25,{"$f":"1-+$D$5*E2","v":0.83750000000000002},{"$f":"1-+$D$5*F2","v":0.9},0.9375,0.95,0.88749999999999996,0.82499999999999996,0.88500000000000001,0.87250000000000005,0.83250000000000002,0.85,0.89249999999999996,0.82750000000000001,0.82750000000000001,0.78249999999999997,0.78249999999999997,0.78749999999999998,0.82499999999999996,0.8,0.84250000000000003,0.84250000000000003,0.875,0.875]
["D","biofilter",0.8,0.19999999999999996,{"$f":"1-+$D$6*E2","v":0.87},{"$f":"1-+$D$6*F2","v":0.92},0.95,0.96,0.91,0.8600000000000001,0.90800000000000003,0.89800000000000002,0.8660000000000001,0.88,0.91400000000000003,0.8620000000000001,0.8620000000000001,0.82600000000000007,0.82600000000000007,0.83000000000000007,0.8600000000000001,0.84000000000000008,0.874,0.874,0.9,0.9]
[null,"GEEN DROOGTUNNEL"]
["E","DROOGTUNNEL (PLATEN) 55%",0.55000000000000004,0.44999999999999996,{"$f":"1-+$D$8*E2","v":0.70750000000000002},{"$f":"1-+$D$8*F2","v":0.82000000000000006},0.88749999999999996,0.91,0.7975000000000001,0.68500000000000005,0.79300000000000004,0.77049999999999996,0.69850000000000012,0.73,0.80649999999999999,0.6895,0.6895,0.60850000000000004,0.60850000000000004,0.61750000000000005,0.68500000000000005,0.64,0.71650000000000003,0.71650000000000003,0.77500000000000002,0.77500000000000002]
["F","DROOGTUNNEL (BANDEN) 30%",0.3,0.7,{"$f":"1-+$D$9*E2","v":0.54500000000000004},{"$f":"1-+$D$9*F2","v":0.72},0.82499999999999996,0.8600000000000001,0.68500000000000005,0.51,0.67800000000000005,0.64300000000000002,0.53100000000000014,0.58000000000000007,0.69900000000000007,0.51700000000000013,0.51700000000000013,0.39100000000000001,0.39100000000000001,0.40500000000000003,0.51,0.44000000000000006,0.55900000000000005,0.55900000000000005,0.65,0.65]
["G","OLIEFILM",0.54,0.45999999999999996,{"$f":"1-+$D$10*E2","v":0.70100000000000007},{"$f":"1-+$D$10*F2","v":0.81600000000000006},0.88500000000000001,0.90800000000000003,0.79300000000000004,0.67800000000000005,0.78839999999999999,0.76540000000000008,0.69180000000000008,0.72399999999999998,0.80220000000000002,0.6826000000000001,0.6826000000000001,0.59980000000000011,0.59980000000000011,0.60899999999999999,0.67800000000000005,0.63200000000000001,0.71019999999999994,0.71019999999999994,0.77,0.77]
["H","negatieve ionisatie",0.49,0.51,{"$f":"1-+$D$11*E2","v":0.66849999999999998},{"$f":"1-+$D$11*F2","v":0.79600000000000004},0.87250000000000005,0.89800000000000002,0.77049999999999996,0.64300000000000002,0.76540000000000008,0.7399,0.65830000000000011,0.69399999999999995,0.78069999999999995,0.64810000000000001,0.64810000000000001,0.55630000000000002,0.55630000000000002,0.5665,0.64300000000000002,0.59199999999999997,0.67869999999999997,0.67869999999999997,0.745,0.745]
["I","water wasser",0.33,0.66999999999999993,{"$f":"1-+$D$12*E2","v":0.5645},{"$f":"1-+$D$12*F2","v":0.73199999999999998},0.83250000000000002,0.8660000000000001,0.69850000000000012,0.53100000000000014,0.69180000000000008,0.65830000000000011,0.55110000000000015,0.59800000000000009,0.71189999999999998,0.53770000000000007,0.53770000000000007,0.41710000000000003,0.41710000000000003,0.4305000000000001,0.53100000000000014,0.46400000000000008,0.57790000000000008,0.57790000000000008,0.66500000000000004,0.66500000000000004]
["J","droogfilter",0.4,0.6,{"$f":"1-+$D$13*E2","v":0.61},{"$f":"1-+$D$13*F2","v":0.76},0.85,0.88,0.73,0.58000000000000007,0.72399999999999998,0.69399999999999995,0.59800000000000009,0.64,0.74199999999999999,0.58600000000000008,0.58600000000000008,0.47799999999999998,0.47799999999999998,0.49,0.58000000000000007,0.52,0.622,0.622,0.7,0.7]
["K","ionisatiefilter",0.56999999999999995,0.43000000000000005,{"$f":"1-+$D$14*E2","v":0.72049999999999992},{"$f":"1-+$D$14*F2","v":0.82799999999999996},0.89249999999999996,0.91400000000000003,0.80649999999999999,0.69900000000000007,0.80220000000000002,0.78069999999999995,0.71189999999999998,0.74199999999999999,0.81509999999999994,0.70330000000000004,0.70330000000000004,0.6258999999999999,0.6258999999999999,0.63449999999999995,0.69900000000000007,0.65599999999999992,0.72909999999999997,0.72909999999999997,0.78499999999999992,0.78499999999999992]
["L","warmtewisselaar zonder stof 31%",0.31,0.69,{"$f":"1-+$D$15*E2","v":0.5515000000000001},{"$f":"1-+$D$15*F2","v":0.72399999999999998},0.82750000000000001,0.8620000000000001,0.6895,0.51700000000000013,0.6826000000000001,0.64810000000000001,0.53770000000000007,0.58600000000000008,0.70330000000000004,0.52390000000000003,0.52390000000000003,0.39970000000000006,0.39970000000000006,0.41350000000000009,0.51700000000000013,0.44800000000000006,0.56530000000000002,0.56530000000000002,0.65500000000000003,0.65500000000000003]
["M","warmtewisselaar met stof 31%",0.31,0.69,{"$f":"1-+$D$16*E2","v":0.5515000000000001},{"$f":"1-+$D$16*F2","v":0.72399999999999998},0.82750000000000001,0.8620000000000001,0.6895,0.51700000000000013,0.6826000000000001,0.64810000000000001,0.53770000000000007,0.58600000000000008,0.70330000000000004,0.52390000000000003,0.52390000000000003,0.39970000000000006,0.39970000000000006,0.41350000000000009,0.51700000000000013,0.44800000000000006,0.56530000000000002,0.56530000000000002,0.65500000000000003,0.65500000000000003]
["N","warmtewisselaar zonder stof 13%",0.13,0.87,{"$f":"1-+$D$17*E2","v":0.4345},{"$f":"1-+$D$17*F2","v":0.65199999999999991},0.78249999999999997,0.82600000000000007,0.60850000000000004,0.39100000000000001,0.59980000000000011,0.55630000000000002,0.41710000000000003,0.47799999999999998,0.6258999999999999,0.39970000000000006,0.39970000000000006,0.24309999999999998,0.24309999999999998,0.26050000000000006,0.39100000000000001,0.30399999999999994,0.45189999999999997,0.45189999999999997,0.56499999999999995,0.56499999999999995]
["O","warmtewisselaar met stof 13%",0.13,0.87,{"$f":"1-+$D$18*E2","v":0.4345},{"$f":"1-+$D$18*F2","v":0.65199999999999991},0.78249999999999997,0.82600000000000007,0.60850000000000004,0.39100000000000001,0.59980000000000011,0.55630000000000002,0.41710000000000003,0.47799999999999998,0.6258999999999999,0.39970000000000006,0.39970000000000006,0.24309999999999998,0.24309999999999998,0.26050000000000006,0.39100000000000001,0.30399999999999994,0.45189999999999997,0.45189999999999997,0.56499999999999995,0.56499999999999995]
["P","oliefim",0.15,0.85,{"$f":"1-+$D$19*E2","v":0.44750000000000001},{"$f":"1-+$D$19*F2","v":0.65999999999999992},0.78749999999999998,0.83000000000000007,0.61750000000000005,0.40500000000000003,0.60899999999999999,0.5665,0.4305000000000001,0.49,0.63449999999999995,0.41350000000000009,0.41350000000000009,0.26050000000000006,0.26050000000000006,0.27750000000000008,0.40500000000000003,0.31999999999999995,0.46450000000000002,0.46450000000000002,0.57499999999999996,0.57499999999999996]
["Q","oliefilm",0.3,0.7,{"$f":"1-+$D$20*E2","v":0.54500000000000004},{"$f":"1-+$D$20*F2","v":0.72},0.82499999999999996,0.8600000000000001,0.68500000000000005,0.51,0.67800000000000005,0.64300000000000002,0.53100000000000014,0.58000000000000007,0.69900000000000007,0.51700000000000013,0.51700000000000013,0.39100000000000001,0.39100000000000001,0.40500000000000003,0.51,0.44000000000000006,0.55900000000000005,0.55900000000000005,0.65,0.65]
["R","strooiselschuif",0.2,0.8,{"$f":"1-+$D$21*E2","v":0.48},{"$f":"1-+$D$21*F2","v":0.67999999999999994},0.8,0.84000000000000008,0.64,0.44000000000000006,0.63200000000000001,0.59199999999999997,0.46400000000000008,0.52,0.65599999999999992,0.44800000000000006,0.44800000000000006,0.30399999999999994,0.30399999999999994,0.31999999999999995,0.44000000000000006,0.35999999999999988,0.496,0.496,0.6,0.6]
["S","warmtewisselaar zonder stof 37%",0.37,0.63,{"$f":"1-+$D$22*E2","v":0.59050000000000002},{"$f":"1-+$D$22*F2","v":0.748},0.84250000000000003,0.874,0.71650000000000003,0.55900000000000005,0.71019999999999994,0.67869999999999997,0.57790000000000008,0.622,0.72909999999999997,0.56530000000000002,0.56530000000000002,0.45189999999999997,0.45189999999999997,0.46450000000000002,0.55900000000000005,0.496,0.60309999999999997,0.60309999999999997,0.68500000000000005,0.68500000000000005]
["T","warmtewisselaar met stof 37%",0.37,0.63,{"$f":"1-+$D$23*E2","v":0.59050000000000002},{"$f":"1-+$D$23*F2","v":0.748},0.84250000000000003,0.874,0.71650000000000003,0.55900000000000005,0.71019999999999994,0.67869999999999997,0.57790000000000008,0.622,0.72909999999999997,0.56530000000000002,0.56530000000000002,0.45189999999999997,0.45189999999999997,0.46450000000000002,0.55900000000000005,0.496,0.60309999999999997,0.60309999999999997,0.68500000000000005,0.68500000000000005]
["U","warmtewisselaar zonder stof 50%",0.5,0.5,{"$f":"1-+$D$24*E2","v":0.67500000000000004},{"$f":"1-+$D$24*F2","v":0.8},0.875,0.9,0.77500000000000002,0.65,0.77,0.745,0.66500000000000004,0.7,0.78499999999999992,0.65500000000000003,0.65500000000000003,0.56499999999999995,0.56499999999999995,0.57499999999999996,0.65,0.6,0.68500000000000005,0.68500000000000005,0.75,0.75]
["V","warmtewisselaar met stof 50%",0.5,0.5,{"$f":"1-+$D$25*E2","v":0.67500000000000004},{"$f":"1-+$D$25*F2","v":0.8},0.875,0.9,0.77500000000000002,0.65,0.77,0.745,0.66500000000000004,0.7,0.78499999999999992,0.65500000000000003,0.65500000000000003,0.56499999999999995,0.56499999999999995,0.57499999999999996,0.65,0.6,0.68500000000000005,0.68500000000000005,0.75,0.75]
[]
[]
[null,"percentages berekend door 1 x (1-%)x(1-%)"]
[null,"rood","afwijkend"]
[null,"paars"," 1% afwijkend"]
[null,"blauw","kan niet gecombineerd"]
[null,"GEEN TECHNIEK"]
[null,"CHEMISCHE WASSER 35%","ALLE VENTILATIELUCHT"]
[null,"CHEMISCHE WASSER 70%"]
[null,"BIO WASSER 60%","DEEL VENTILATIELUCHT"]
[null,"BIO WASSER 75%",null,null,null,null,{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,"BIOFILTER","GEEN TECHNIEK",null,null,null,{"$f":"IF(#REF!=\"Alle lucht moet door de luchtwasser of biofilter. De combinatie met een stoffilter is daarom niet mogelijk.\",CHEMISCHE WASSER NIET TOEGESTAAN,\"CHEMISCHEWASSER\")","v":{"$error":"#REF!"}}]
[null,"WATERLUCHTWASSYSTEEM","WATERLUCHTWASSYSTEEM",null,null,null,"CHEMISCHE WASSER NIET TOEGESTAAN"]
[null,"DROOGFILTERWAND","DROOGFILTERWAND"]
[null,"IONISATIEFILTER","IONISATIEFILTER"]
[null,"LUCHTCONDITIONERINGSUNIT"]
[null,"WARMTEWISSELAAR 13%","ALLE VENTILATIELUCHT"]
[null,"WARMTEWISSELAAR 31%","75% VENTILATIE"]
[null,"WARMTEWISSELAAR 37%","50% VENTILATIE"]
[null,"WARMTEWISSELAAR 50%","25% VENTILATIE"]
[null,"ZONDER STOFFILTER"]
[null,"MET STOFFILTER"]
[]
[null,"PARALLEL GESCHAKELD MET WARMTEWISSELAAR"]
[null,"SERIE GESCHAKELD MET WARMTEWISSELAAR"]
[]
[null,"JA","JA",null,{"$f":"#REF!","v":{"$error":"#REF!"}}]
[null,"NEE","NEE"]
[null,null,{"$f":"IF(#REF!=\"geen techniek\",\"GEEN TECHNIEK\",\"JA\")","v":{"$error":"#REF!"}}]
[null,null,"NEE"]